Revision History for SIR 2012-5044

**U.S. Geological Survey Scientific Investigations Report SIR 2012–5044**

May 4, 2012

Subsequent to the publication of this report (U.S. Geological Survey Scientific Investigations Report SIR 2012–5044), a typographical error was found that affects two instantaneous-streamflow values presented in table 2. For the site 287 Bypass Bridge, the instantaneous-streamflow value should be 3,140—with footnote 4 (43,140). For the site Townsend Bridge, the instantaneous-streamflow value should be 3,250—with footnote 4 (43,140). This error does not affect any related text, interpretations, or conclusions. Corrections to the online version of this report (accessed at *http://pubs.usgs.gov/sir/2012/5044/)* have been made.