Revision History for USGS Scientific Investigations Report 2013–5005

Water Quality, Streamflow Conditions, and Annual Flow-Duration Curves for Streams of the San Juan–Chama Project, Southern Colorado and Northern New Mexico, 1935–2010

-----------------------------------------------------

First posted January 2013

-----------------------------------------------------

Description of Changes to May 2013 Revision

On page 35, the equation for calculating the center of mass of annual discharge (CT) was added to the text:



where

*Ti* is the ordinal day of the water year, and

*Qi* is the daily mean streamflow.