# Black Bayou Hydrologic Restoration CS-27 2010 Project Area Land-Water Data

# Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: U.S. Geological Survey, National Wetlands Research Center
      Publication_Date: 2013
      Title:
        Black Bayou Hydrologic Restoration CS-27 2010 Project Area Land-Water Data
      Geospatial_Data_Presentation_Form: raster digital data
      Publication_Information:
        Publication_Place: Lafayette, LA
        Publisher: U.S. Geological Survey, National Wetlands Research Center
      Online_Linkage: <http://pubs.er.usgs.gov/publication/ds745>
      Larger_Work_Citation:
        Citation_Information:
          Originator: Coastal Protection and Restoration Authority of Louisiana
          Originator:
            U.S. Department of Commerce, National Oceanic Atmospheric Administration
          Originator:
            U.S. Department of Agriculture, Natural Resources Conservation Service
          Originator: U.S. Department of Interior, U.S. Fish and Wildlife Service
          Originator: U.S. Department of the Army, Corp of Engineers
          Originator: U.S. Environmental Protection Agency
          Publication_Date: 2013
          Title:
            Coastal Wetlands Planning, Protection and Restoration Act (CWPPRA) Authorizing Bill
          Geospatial_Data_Presentation_Form: document
          Online_Linkage: <http://www.lacoast.gov>
  Description:
    Abstract:
      The Louisiana State Legislature created the Coastal Wetlands Planning, Protection and Restoration Act (CWPPRA) in order to conserve, restore, create, and enhance Louisiana's coastal wetlands. The restoration plans developed persuant to these acts specifically require an evaluation of the effectiveness of each coastal wetland restoration project in achieving long-term solutions to arresting coastal wetland loss. This data set consists of digital data describing wetland land-water classification for the Black Bayou Hydrologic Restoration for the year 2010. The land-water data were derived from interpretation of color infrared photography flown at 1:12000. All areas characterized by emergent vegetation, wetland forest, scrub-shrub, or uplands are classified as land, while open water, aquatics, and mud flats were classified as water.
    Purpose:
      The intended use of this data set is to provide information to aid efforts in the conservation, restoration, creation, and enhancement of Louisiana's coastal wetlands. The land-water data is used for time comparisons to measure the rate of success for the CWPPRA's CS-27.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 2013
    Currentness_Reference: publication date
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -91.005940
      East_Bounding_Coordinate: -90.966075
      North_Bounding_Coordinate: 29.417730
      South_Bounding_Coordinate: 29.373609
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: None
      Theme_Keyword: CWPPRA
      Theme_Keyword: Breaux Act
      Theme_Keyword: land-water
      Theme_Keyword: wetland
      Theme_Keyword: mapping
      Theme_Keyword: map
      Theme_Keyword: marsh
      Theme_Keyword: restoration
      Theme_Keyword: protection
      Theme_Keyword: coastal
      Theme_Keyword: scanning
      Theme_Keyword: cartography
      Theme_Keyword: Geographic Information System
    Theme:
      Theme_Keyword_Thesaurus: ISO 19115 Topic Category
      Theme_Keyword: imageryBaseMapsEarthCover
    Place:
      Place_Keyword_Thesaurus: None
      Place_Keyword: Louisiana
      Place_Keyword: Black Bayou
      Place_Keyword: Calcasieu Parish
      Place_Keyword: Cameron Parish
    Place:
      Place_Keyword_Thesaurus: Geographic Names Information System
      Place_Keyword: State of Louisiana
      Place_Keyword: Black Bayou
      Place_Keyword: Calcasieu Parish
      Place_Keyword: Cameron Parish
  Access_Constraints:
    It is strongly recommended that these data are directly acquired from the U.S. Geological Survey, National Wetlands Research Center and not indirectly through other sources which may have changed in some way. The distributor makes no claim as to the data's suitability for other purposes.
  Use_Constraints:
    Acknowledgement of the U.S. Geological Survey (USGS), National Wetlands Research Center (NWRC) as a data source would be appreciated in products developed from these data. Such acknowledgement as is standard for citation and legal practices for data sources is expected by users of this data. Sharing new data layers developed directly from these data would be appreciated by the USGS NWRC staff. Users should be aware that comparison with other datasets for the same area from other time periods may be inaccurate because of inconsistencies resulting from changes in mapping conventions, data collection procedures, and computer processes over time. The distributor shall not be liable for improper or incorrect use of these data, based on the description of appropriate/inappropriate uses described in this metadata document. These data are not legal documents and are not to be used as such.
  Point_of_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey, National Wetlands Research Center
        Contact_Person: William Jones
      Contact_Position: Geographer
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 700 Cajundome Blvd
        City: Lafayette
        State_or_Province: LA
        Postal_Code: 70506-3152
        Country: USA
      Contact_Voice_Telephone: 337 266-8500
      Contact_Facsimile_Telephone: 337 266-8616
      Contact_Electronic_Mail_Address: william_jones@usgs.gov
      Contact_Instructions:
        Additional contact: Information Services, Voice 337-266-8692, Email nwrclibrary@usgs.gov
  Data_Set_Credit:
    The U.S. Geological Survey (USGS) National Wetlands Research Center (NWRC) would like to acknowledge the assistance of the Coastal Protection and Restoration Authority of Louisiana, U.S. Department of Commerce, U.S. Department of Agriculture, U.S. Department of the Interior, U.S. Department of the Army, and the U.S. Environmental Protection Agency.
  Native_Data_Set_Environment:
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.0.0.535
  Cross_Reference:
    Citation_Information:
      Originator: U.S. Geological Survey, National Wetlands Research Center
      Publication_Date: 2013
      Title: Black Bayou Hydrologic Restoration CS-27 2010 Photomosaic Data

Data_Quality_Information:
  Attribute_Accuracy:
    Attribute_Accuracy_Report:
      Quality control processes are in place to ensure optimal accuracy. Land-Water data will go through several review steps by different GIS Specialists to verify the accuracy of the classification.
  Logical_Consistency_Report:
    All Land-Water Classification data has gone through extensive Quality Assurance and Quality Control to ensure accuracy.
  Completeness_Report:
    For all calculations and manipulations done in ERDAS Imagine, the software manual was consulted. Standard Operating Procedures for the Land-Water Classification were developed by Geographic Information Systems staff at the U.S. Geological Survey, National Wetlands Research Center.
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report:
        The accuracy of the horizontal positions is based on the accuracy of the georeferenced data source (which can be USGS DOQQs, DEMS, flight line center points, and/or calibration reports). The sources used vary from project to project. All USGS Mapping products adhere to the National Mapping Accuracy Standard.
  Lineage:
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: unknown
          Publication_Date: 2013
          Title:
            Black Bayou Hydrologic Restoration CS-27 2010 CIR aerial photography
          Geospatial_Data_Presentation_Form: remote-sensing image
          Publication_Information:
            Publication_Place: Louisiana
            Publisher: unknown
      Source_Scale_Denominator: 12000
      Type_of_Source_Media: Stable-based material
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 2010
        Source_Currentness_Reference: Date of source photography
      Source_Citation_Abbreviation: Aerial photo
      Source_Contribution: The primary data source for classification of land-water data
    Process_Step:
      Process_Description:
        Land-Water Classification: After high-resolution, color-infrared photography is acquired, a Land-Water Classification is conducted. An unsupervised classification is performed by using ERDAS Imagine software. When performing the unsupervised classification process, maximum illiterations are set to 30, and the convergence threshold is set at 0.980. Depending on the color balance, tone, and other aspects of the imagery, the number of classes is set between 50 and 100. If it is determined that the maximum iterations have been reached before the convergence threshold is achieved, the maximum iterations will be increased to ensure the convergence threshold is achieved. This procedure results in a thematic raster image with 50-100 different classes, depending upon the range of pixel values. These individual classes are then interpreted to be either land or water based upon the GIS Specialist's interpretation. Ancillary datasets from 1998 through 2010 are used to help classify areas that are difficult to identify. The file is then manually edited to correct any misclassified pixels. The finished classification is recoded into the two classes, land and water. All areas characterized by emergent vegetation, wetland forest, scrub-shrub, or uplands are classified as land, while open water, aquatics and mud flats are classified as water. After completion of the classification process, the GIS specialist will perform a quality assurance (QA) self-check of the results. In addition, a second GIS specialist will perform a final, in-house quality control (QC) review to assure accuracy and data integrity.
      Process_Date: 2010
      Source_Produced_Citation_Abbreviation: Digital map
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization: U.S. Geological Survey, National Wetlands Research Center
            Contact_Person: William Jones
          Contact_Position: Geographer
          Contact_Address:
            Address_Type: mailing and physical address
            Address: 700 Cajundome Blvd
            City: Lafayette
            State_or_Province: LA
            Postal_Code: 70506
            Country: USA
          Contact_Voice_Telephone: 337 266-8500
          Contact_Facsimile_Telephone: 337 266-8616
          Contact_Electronic_Mail_Address: jonesb@usgs.gov

Spatial_Data_Organization_Information:
  Indirect_Spatial_Reference: Coastal Louisiana
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: G-polygon
      Point_and_Vector_Object_Count: 2025

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Grid_Coordinate_System:
        Grid_Coordinate_System_Name: Universal Transverse Mercator
        Universal_Transverse_Mercator:
          UTM_Zone_Number: 15
          Transverse_Mercator:
            Scale_Factor_at_Central_Meridian: 0.999600
            Longitude_of_Central_Meridian: -93.000000
            Latitude_of_Projection_Origin: 0.000000
            False_Easting: 500000.000000
            False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.000008
          Ordinate_Resolution: 0.000008
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222

Entity_and_Attribute_Information:
  Overview_Description:
    Entity_and_Attribute_Overview:
      All areas characterized as emergent vegetation, wetland forest, scrub-shrub, or uplands are classified as land, while open water aquatics, and mud flats are classified as water. Items within the attribute table in addition to ArcInfo items (e.g. area. perimeter) include: 1) Class- classified as either land or water, 2) Acres- acreage figures
    Entity_and_Attribute_Detail_Citation: Producer defined

Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey, National Wetland Research Center
      Contact_Position: Spatial Analysis Database Administrator
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 700 Cajundome Blvd
        City: Lafayette
        State_or_Province: LA
        Postal_Code: 70506
        Country: USA
      Contact_Voice_Telephone: 337 266-8500
      Contact_Facsimile_Telephone: 337 266-8513
      Contact_Instructions:
        Additional contact: Information Services, Voice 337-266-8692, Email nwrclibrary@usgs.gov
  Resource_Description: Downloadable Data
  Distribution_Liability:
    Although these data have been processed successfully on a computer system at the U.S. Geological Survey, National Wetlands Research Center, no warranty expressed or implied is made regarding the accuracy or utility of the data on any other system or for general or scientific purposes, nor shall the act of distribution constitute any such warranty. This disclaimer applies both to individual use of the data and aggregate use with other data. It is strongly recommended that these data are directly acquired from a U.S. Geological Survey server, and not indirectly through other sources which may have changed the data in some way. It is also strongly recommended that careful attention be paid to the contents of the metadata file associated with these data. The U.S. Geological Survey shall not be held liable for improper or incorrect use of the data described and/or contained herein.
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: ARCE
        Format_Version_Number: 8+
        File_Decompression_Technique: zipped
        Transfer_Size: 6.831
      Digital_Transfer_Option:
        Online_Option:
          Computer_Contact_Information:
            Network_Address:
              Network_Resource_Name:
                <http://sabdata.cr.usgs.gov/sabnet_pub/pub_sab_app.aspx?prodid=25840>
    Fees: None, if available on line
    Ordering_Instructions:
      To obtain the land-water data through the sabdata.nwrc.gov server, search on the title of the data set and use the download option.
  Custom_Order_Process: None
  Technical_Prerequisites: None

Metadata_Reference_Information:
  Metadata_Date: 20130215
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey, National Wetlands Research Center
        Contact_Person: William Jones
      Contact_Position: GIS specialist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 700 Cajundome Blvd
        City: Lafayette
        State_or_Province: LA
        Postal_Code: 70506
        Country: USA
      Contact_Voice_Telephone: 337 266-8500
      Contact_Facsimile_Telephone: 337 266-8616
      Contact_Electronic_Mail_Address: jonesb@usgs.gov
      Contact_Instructions:
        Additional contact: Information Services, Voice 337-266-8692, Email nwrclibrary@usgs.gov
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Access_Constraints: None
  Metadata_Use_Constraints:
    Acknowledgement of the U.S. Geological Survey, National Wetlands Research Center as the metadata source would be appreciated. Please cite the original metadata when using portions of the record when creating a similar record for slightly altered data for reprojection or subsetting. Any use of trade, product, or firm names is for descriptive purposes only and does not imply endorsement by the U.S. Government.
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile

Generated by `mp` version 2.9.6 on Fri Mar 01 14:24:15 2013