U.S. DEPARTMENT OF THE INTERIOR TO ACCOMPANY MAP MF-2329

U.S. GEOLOGICAL SURVEY

**MAP SHOWING INVENTORY AND REGIONAL SUSCEPTIBILITY FOR HOLOCENE DEBRIS FLOWS AND RELATED FAST-MOVING LANDSLIDES IN THE CONTERMINOUS UNITED STATES**

## By Earl E. Brabb, Joseph P. Colgan, and Timothy C. Best

## INTRODUCTION

 Debris flows, debris avalanches, mud flows, and lahars are fast-moving landslides that occur in a wide variety of environments throughout the world. They are particularly dangerous to life and property because they move quickly, destroy objects in their paths, and can strike with little warning. U.S. Geological Survey scientists are assessing debris-flow hazards and developing real-time techniques for monitoring hazardous areas so that road closures, evacuations, or corrective actions can be taken (Highland and others, 1997).

 According to the classifications of Varnes (1978) and Cruden and Varnes (1996), a debris flow is a type of slope movement that contains a significant proportion of particles larger than 2 mm and that resembles a viscous fluid. Debris avalanches are extremely rapid, tend to be large, and often occur on open slopes rather than down channels. A lahar is a debris flow from a volcano. A mudflow is a flowing mass of predominantly fine-grained material that possesses a high degree of fluidity (Jackson, 1997). In the interest of brevity, the term "debris flow" will be used in this report for all of the rapid slope movements described above.

## WHAT CAUSES DEBRIS FLOWS?

 Debris flows in the Appalachian Mountains are often triggered by hurricanes, which dump large amounts of rain on the ground in a short period of time, such as the November 1977 storm in North Carolina (Neary and Swift, 1987) and Hurricane Camille in Virginia (Williams and Guy, 1973). Both of these storms caused large numbers of debris flows and extensive damage. High-intensity rainfall is also a common trigger for debris flows in the Coast Ranges from California to Washington, such as the 1982 storm in the San Francisco Bay region, which triggered 18,000 debris flows, killed 25 people, and caused at least $65,000,000 in damages (Ellen and Wieczorek, 1988). Debris flows in arid and semi-arid regions of the American West seem to be caused primarily by locally intense storms between the months of June and October. Examples include flows along the Colorado River and its tributaries (Webb and others, 1989), flows in central Utah (Baum and Fleming, 1989), and those in other desert areas of Utah, Arizona, Nevada, Oregon, and California (Blackwelder, 1928). Rapid snowmelt was the main trigger for the 1983 debris flows in Utah (Brabb and others, 1989b). Earthquakes and volcanic eruptions commonly trigger debris avalanches, which can also be initiated by heavy or prolonged rainfall.

 Some of the lahars triggered by the 1980 eruption of Mount St. Helens were generated when snow avalanches were rapidly melted and mixed with pyroclastic material during the initial eruption. Other lahars formed more than four hours later when avalanche debris saturated with melted ice was set in motion by another eruption and harmonic tremors (Fairchild, 1987). These lahars extended as much as 22 km from their source on the volcano down the various forks of the Toutle River. Other volcanoes in Washington and California, such as Mt. Rainier (Crandell and Waldron, 1956) and Mount Shasta (Crandell and others, 1984), have runout distances in excess of 40 km.

 Fire can increase the danger of debris flows by accelerating surface erosion and causing water-repellent soils to develop on burned areas. These water-repellent soils can facilitate small debris flows during mild rainstorms or after very little rain has fallen, according to Wells (1987).

## NEED FOR A DEBRIS FLOW MAP

 A new responsibility to evaluate landslide hazards in the United States, combined with a statement by Radbruch-Hall and others (1982, p. 2) that debris flows in arid regions had not been included in their overview of landslides in the United States, led the first author to make a reconnaissance of landslide problems in all 50 states in the early 1980’s. Conversations with state highway engineers and members of state geological surveys were supplemented by visits to landslides described by them and in published reports (compiled by Alger and Brabb, 1985) and to other areas where landslides could be expected. Debris flows and other landslides visited were plotted on topographic maps, mostly at 1:500,000 scale. The results of this investigation (Brabb, 1989) constituted the first comprehensive report to give a state-by-state analysis of landslide problems in the United States and different ways to evaluate the impact of those problems on each state. This was in contrast to the Radbruch-Hall report, which discussed the spatial occurrence of landsliding within physiographic provinces. A slope map in the 1989 report showed mountainous areas where landslides had occurred or could be expected, but debris flows were not described separately. The purpose of the present map, therefore, is to show where debris flows have occurred in the United States and where these slope movements might be expected in the future.

## PREPARATION OF THIS MAP

 In 1984, Best and Brabb prepared an inventory of past debris flows using data from the reconnaissance field investigations and a list of published and unpublished reports, a list which was eventually published by Alger and Brabb (1985). This information was plotted on 1:500,000-scale USGS state maps and transferred by hand to a 1:2,500,000-scale greenline base map of the United States. In 1997, A. Barron and M. Sinor digitized this greenline base map, but no new information was added to the map at that time.

 In 1998 and 1999, new information was added to bring the map up-to-date. The data were gathered from published and unpublished reports of debris flows primarily covering the years 1984-1999. Many older reports that had been overlooked in the original map were also included. In addition, all state geologists were contacted to find out if they had information on debris flows. Several state geologists and members of their staff provided significant new information.

 No distinction was made between debris flow scars, made shortly after the events, and debris flow deposits, which may be thousands of years old. We believe that all of the debris flows described in this report formed during the past 10,000 years (Holocene), but some of them could be older.

 Mudflows are included even though this term is widely misused by the media and others for debris flows and sediment-laden floods. See the discussion by Campbell and others (1989).

 If a report included a map at a scale larger than that of the compilation (1:2,500,000), the map or a photocopy was scanned. Other reports contained only the names of places where debris flows had occurred, or a map at a scale smaller than 1:2,500,000, or a map with no geographic coordinates. In those cases, the debris flows were located approximately on the appropriate 1:500,000-scale USGS state map or a 1:100,000-scale USGS topographic map and plotted by hand on a Mylar overlay. This overlay was then scanned. Details of the scanning process and a description of other database techniques and data are provided in Appendix 1.

 The inventory map shows the locations of debris flows in two different ways, as points representing the locations of individual flows or small groups of flows, and as areas or polygons containing one or more debris flows. Different symbols are used to indicate uncertainty in location or the identification of the feature as a debris flow. In the digital database, a reference number ties each point and polygon on the map to the bibliography for each state, but these numbers are omitted from the published map for clarity. In those places where detailed debris-flow mapping was available in digital form, such as New Mexico and Utah, we plotted individual flows to illustrate their number and extent. In the San Francisco Bay area (Ellen and Wieczorek, 1988), we used a polygon because the 18,000 debris flows would plot as a large red blob.

 Many of the other polygons represent areas in which less than fifty debris flows have been recognized or in areas where authors of reports have not provided sufficient information to locate the flows. Rectangular boxes represent 7.5-minute quadrangles where one to several hundred debris flows have been mapped at 1: 24,000 scale. Most of these quadrangles are in Appalachian states and in California.

 Only New Mexico has a systematic inventory of debris flows (Cardinali and others, 1990) for the entire state. The comparison of New Mexico with surrounding states having a similar climate and similar steep slopes suggests that most of the mountainous states have not been adequately mapped and that debris flows are far more common than depicted. This idea is reinforced by the large number of debris flows recorded in specific storms in Utah (Brabb and others, 1989b), California (Ellen and Wieczorek, 1988), and Virginia (Morgan and others, 1999).

## SUSCEPTIBILITY

 The incompleteness of the inventory of debris flows makes educating decision-makers and the public about the extent of debris-flow hazard in the United States difficult. Fortunately, Clark (1987) and Corominas and others (1996) have compiled information on the slope angles of debris-flow source areas, indicating that debris flows initiate mainly on slopes steeper than 25 degrees. Therefore, a map showing slopes greater than 25 degrees would be expected to show most debris-flow source areas in the United States.

 A Digital Elevation Model (DEM) released by the National Oceanic and Atmospheric Administration (NOAA) provides convenient nationwide data for the preparation of a slope map. The database consists of ground-surface elevations at 30 arc-second (approximately 1 km by 1 km) grid cells. Apparently these data were derived from the Army Map Service 1:250,000 topographic maps. Several slope maps were prepared from this database using ARC/INFO, a commercial GIS software program. To calculate the slope at each one-kilometer grid cell, the process fits a quadratic surface to the elevation values of a 3 cell by 3 cell box surrounding the grid cell for which the slope is to be calculated. The slope assigned to the middle cell is the maximum slope of the quadratic surface at that point.

 Brabb and others (1989b) have discussed several problems with the database. One of these concerns the average value for the slope over a 9-km-square area. This figure is generally much flatter than the actual value for slopes within the selected area. Map values of one or two degrees may correspond to slopes steeper than the 25- degree value targeted for the susceptibility map. Because of this discrepancy, the map is referred to as a slope index map, giving relative slope rather than actual slope in any specific area.

 Several slope index maps were prepared to try to find slopes steeper than 25 degrees where debris flows might be expected in the future. The maps were adjusted by trial and error to incorporate the largest number of debris-flow points without including large, gently sloping areas where no debris flows are expected. We eventually adopted a map with a slope index steeper than 3 percent, which includes about 75 percent of the debris flows mapped. Only individual debris-flow locations were used to compute the percentage of debris flows in each slope category, because the locations of debris flows within the polygon areas are too uncertain for this purpose. The other debris flows may occur in areas where more gentle average slopes contain steep slopes of limited extent, such as cliffs along rivers and lakes that are too small to be detected in the one-kilometer grid cell. Alternatively, some features mapped as debris flows may not be debris flows.

### SPATIAL RESOLUTION AND POTENTIAL MISUSE OF MAP INFORMATION

 Users of this digital map should not violate the spatial resolution of the data. Although the digital form of the data removes the constraint imposed by the scale of a paper map, the detail and accuracy inherent in map scale are also present in the digital data. The fact that this database was edited at a scale of 1:2,500,000 means that higher resolution information is not present in the data. Plotting at scales larger than 1:2,500,000 will not yield greater real detail, and it may reveal fine-scale irregularities below the intended resolution of the database. Similarly, where this database is used in combination with other data of higher resolution, the resolution of the combined output will be limited by the lower resolution of these data.

 Users are also warned that gently sloping or even flat areas adjacent to steeper slopes where debris flows may occur are not necessarily safe. Debris flows may extend several kilometers from the mountains out into the flat areas.

## CONCLUSIONS

 This map provides a preliminary overview of debris flows and debris-flow susceptibility in the conterminous United States. It is not intended for hazard evaluation or other site-specific work, and should not be used for such. It can be used to determine where debris flow processes may be a problem and where additional information and investigation are warranted.

 Twenty-eight of the forty-eight conterminous United States have documented debris flows. They are most abundant in the Coast Ranges, Rocky Mountains, and Appalachian Mountains but occur in other places where slopes are steep, including bluffs along rivers and the slopes beneath mesas and other escarpments. Moreover, gently sloping or flat areas adjacent to these steep slopes are also at risk. Debris flows are rare or absent on the plains and gently rolling hills of Middle America. In California, Utah, and the Southern Appalachians, debris flows are a common hazard that kills people and causes extensive property damage. References and map locations in the digital database provide a foundation for understanding the extent of the debris flow hazard, but much more systematic mapping of debris flows in every vulnerable state is needed before the full extent of the problem can be determined.

## ACKNOWLEDGEMENTS

 We are grateful to several state geologists and members of their staff who kindly reviewed a preliminary copy of the map and the bibliography and provided new information. We are particularly grateful to M. Lee Allison, State Geologist for Utah, and members of his staff who contributed a digital database of debris flow locations for Utah. We also wish to thank Stephen Ellen, Russell Campbell, Gerald Wieczorek, Carl Wentworth, and David Howell for their reviews and help during various phases of the work. Charles Powell, II, kindly scanned and edited a draft of the bibliography. This project was supported in part by an appointment to the U.S. Geological Survey Earth Science Internship Program administered by Oak Ridge Associated Universities.

## TRADE, PRODUCT, OR FIRM NAMES

 The use of trade, product, or firm names is for descriptive purposes only and does not imply endorsement by the U.S. Government.

#### REFERENCES CITED

Alger, C.S., and Brabb, E.E., 1985, Bibliography of United States landslide maps and reports: U.S. Geological Survey Open-File Report 85-585,119 p.

Baum, R.L., and Fleming, R.W., 1989, Landslides and debris flows in Ephraim Canyon, Central Utah: U.S. Geological Survey Bulletin 1842.

Blackwelder, E., 1928, Mudflow as a geologic agent in semi-arid mountains: Geological Society of America Bulletin, v. 39, p. 465-484.

Brabb, E.E., 1989, Landslides; Extent and economic significance in the United States, *in* Brabb, E.E. and Harrod, B.L., eds., Landslides: Extent and economic significance: International Geological Congress, 28th,Washington, 1989, Proceedings: Rotterdam, Balkema, p. 25-50.

Brabb, E.E., Guzzetti, Fausto, Mark, Robert, and Simpson, R.W. Jr., 1989a, The extent of landsliding in northern New Mexico and similar semi-arid and arid regions: Inland Geological Society, v. 2, p. 163-173.

Brabb, E.E., Wieczorek, G.F., and Harp, E.L., 1989b, Map showing 1983 landslides in Utah: U.S. Geological Survey Miscellaneous Field Studies Map MF-2085, scale 1:500,000.

Campbell, R.H., Fleming, R.W., Prior, D.B., Nichols, D.J., Varnes, D.J., Hampton, M.A., Sangrey, D.A., and Brabb, E.E., 1989, Landslide classification for identification of mud flows and other landslides, *in* Sadler, P.M., and others, eds., Landslides in a semi-arid environment with emphasis on the inland valleys of Southern California: Publications of the Inland Geological Society, p. 1-27.

Cardinali, Mauro, Guzzetti, Fausto, and Brabb, E.E., 1990, Preliminary maps showing landslide deposits and selected features in New Mexico: U.S. Geological Survey Open-File Report 90-293, scale 1:500,000.

Clark, G.M., 1987, Debris slide and debris flow events in the Appalachians south of the glacial border, *in* Costa, J.E., and Wieczorek, G.F. eds., Debris flows/avalanches: process, recognition, and mitigation: Geological Society of America Reviews in Engineering Geology, v. 7, p. 125-138.

Corominas, J., and others, 1996, Debris flow, *in* Dikau, Richard, and others, eds., Landslide recognition: John Wiley and Sons, New York, p. 161-180.

Crandell, D.R., and Waldron, H.H., 1956, A recent volcanic mudflow of exceptional dimensions from Mt. Rainier, Washington: American Journal of Science, v. 254, p. 349-362.

Crandell, D.R., and others, 1984, Catastrophic debris avalanche from ancestral Mount Shasta volcano, California: Geology, v. 12, p. 143-146.

Cruden, D.M., and Varnes, D.J., 1996, Landslide types and processes, *in* Turner, A.K., and Schuster, R.L. eds., Landslides, investigation and mitigation: Transportation Research Board, National Research Council, Special Report 247, p. 36.

Ellen, S.D., and Wieczorek, G.F., 1988, Landslides, floods and marine effects of the storm of January 3-5, 1982, in the San Francisco Bay region: U. S. Geological Survey Professional Paper 1434.

Fairchild, L.H., 1987, The importance of lahar initiation processes, *in* Costa, J.E., and Wieczorek, G.F., eds., Debris flows/avalanches: processes, recognition, and mitigation: Geological Society of America Reviews in Engineering Geology, v. 7, p. 51-61.

Highland, L.M., Ellen, S.D., Christian, S.B., and Brown, W.M., III, 1997, Debris-flow hazards in the United States: U.S. Geological Survey Fact Sheet 176-97.

Jackson, J.A., ed., 1997, Glossary of Geology: American Geological Institute, Alexandria, VA.

Morgan, B.A., Wieczorek, G.F., and Campbell, R.H., 1999, Map showing rainfall, debris flows, and flood effects of the June 27, 1995 storm in Madison County, Virginia: U.S. Geological Survey Geologic Investigations Map I-2623-A, scale 1:24,000.

Neary, D.G., and Swift, L.W. Jr., 1987, Rainfall threshold for triggering a debris avalanching event in the southern Appalachian Mountains: Geological Society of America Reviews in Engineering Geology, v. 7, p. 81 -92.

Radbruch-Hall, D.H., and others, 1982, Landslide overview map of the conterminous United States: U. S. Geological Survey Professional Paper 1183.

Varnes, D.J., 1978, Slope movement and processes, *in* Schuster, R.L., and Krijek, R.J. eds., Landslide analysis and control: National Academy of Sciences,Washington, D.C., p. 11-33.

Webb, R.H., Pringle, P.T., Rink, G.R., 1989, Debris flows from tributaries of the Colorado River, Grand Canyon National Park, Arizona: U.S. Geological Survey Professional Paper 1492.

Wells, W.G., II, 1987, The effects of fire on the generation of debris flows in southern California, *in* Costa, J.E., and Wieczorek, G.F., eds., Debris flows/avalanches: processes, recognition, and mitigation: Geological Society of America Reviews in Engineering Geology, v. 7, p. 105-114.

Williams, G.P., and Guy, H.P., 1973, Debris avalanches, a geomorphic hazard, *in* Coates, D. R., compiler, Environmental Geomorphology: Dowden, Hutchinson and Ross, Stroudsburg, PA, p. 25‑46.

U.S. DEPARTMENT OF THE INTERIOR TO ACCOMPANY MAP MF-2329

U.S. GEOLOGICAL SURVEY

**APPENDIX 1**

#### TECHNICAL DESCRIPTION OF THE DATABASE

SCANNING

 The scanning was done at 400 dpi on either a UMAX color flatbed scanner or a Contex FSC-8000dsp color scanner, depending on the size of the map or tracing. The scanned images were transformed from scanner coordinates to geographic coordinates in ARC/INFO with digital tics placed by hand. The scanned lines and/or points were edited interactively using ALACARTE (Wentworth and Fitzgibbon, 1991), and the database fields (tables 3, 4, and 5) were filled in as appropriate

PROJECTION

 The digital map databases consist of ARC coverages and supporting INFO files, which are stored in a Lambert Azimuthal projection (table 1). Digital tics every 9 degrees of latitude and 20 degrees of longitude define a grid in the coverages. For more information about map projections, see Snyder (1987).

**Table 1.** Map Projection Information

Projection Lambert\_Azimuthal

Datum North American Datum of 1983 (NAD83)

Units Meters

Zunits None

Xshift 0.0000000000

Yshift 0.0000000000

# Parameters

6370997.00000 Radius of the sphere of reference

-100 0 0.000 Longitude of center of projection

45 0 0.000 Latitude at center of projection

0.00000 False easting (meters)

0.00000 False northing (meters)

DATABASE FIELDS

 The content of the geologic database can be described in terms of the points and the areas that compose the map. Descriptions of the database fields in each table are explained in table 2.

**Table 2.** Field Definition Terms in Tables

Item Name Name of the database field (item)

Width Maximum number of digits or characters stored

Output Output width

Type B-binary integer, F-binary floating-point number,
I-ASCII integer, C-ASCII character string

NDP Number of decimal places maintained for floating-point numbers

POINTS

 Data representing information at a single locality (points) are described in the point attribute table (table 3). The identities of the points from compilation sources are recorded in the REF and STATE fields. The STATE field indicates the state under which the source data for that point is referenced, and the REF field indicates the number of the reference for that point. Because several published sources of data can refer to the same geographic location, the REF field may contain multiple entries separated by commas. The subjective quality of the source data for a point is stored in the DFTYPE field (table 4).

**Table 3.** Content of the Point Attribute Tables

# Item Name Width Output Type NDP Explanation

AREA 4 12 F 3 Area of polygon in square meters

PERIMETER 4 12 F 3 Length of perimeter in meters

DFIPTSCMP# 4 5 B Unique internal control number

DFIPTSCMP-ID 4 5 B Unique identification number

STATE 2 2 C Two-letter state abbreviation

REF 45 45 C Reference numbers

DFTYPE 1 1 I Nature of point data (table 4)

**Table 4.** Point Types Recorded in the DFTYPE field.

1. Location of debris flows(s) and related fast-moving landslide(s)

2. Approximate location of debris flow(s) and related fast-moving landslide(s)

3. Identification as debris flow(s) ) and related fast-moving landslide(s) uncertain

4. Approximate location, and uncertain identification as debris flow(s) and related fast-moving landslide(s)

5. Location of debris flow(s) and related fast-moving landslide(s) specific only by county

6. Identification as debris flow(s) and related fast-moving landslide(s) uncertain and specific only by county

7. Location of debris flow(s) and related fast-moving landslide(s) from field investigations

8. Approximate location and uncertain identification as debris flow(s) and related fast-moving landslide(s) from field investigations

AREAS

 The identities of the areas from compilation sources are recorded in the REF and STATE fields. The STATE field indicates the state under which the source data for that area is referenced, and the REF field indicates the number of the reference for that area. Because several published sources of data can refer to the same geographic location, the REF field may contain multiple entries separated by commas. Because the location of individual debris flows is uncertain within the polygon boundary, the information in table 4 is not recorded in a DFTYPE field as it is for point data. Note that ARC/INFO coverages cannot contain both point and polygon information, so only coverages with polygon information will have a polygon attribute table, and those coverages will not have a point attribute table.

**Table 5.** Content of the Polygon Attribute Tables

# Item Name Width Output Type NDP Explanation

AREA 4 12 F 3 Area of polygon in square meters

PERIMETER 4 12 F 3 Length of perimeter in meters

DFIPTSCMP# 4 5 B Unique internal control number

DFIPTSCMP-ID 4 5 B Unique identification number

STATE 2 2 C Two-letter state abbreviation

REF 45 45 C Reference numbers

LINES

 The lines (arcs) are recorded as strings of vectors and are described in the arc attribute table (table 6). They define the boundaries of the areas containing debris flows.

 **Table 6.** Content of the Arc Attribute Tables

# Item Name Width Output Type NDP Explanation

FNODE# 4 5 B Starting node of arc (from node)

TNODE# 4 5 B Ending node of arc (to node)

LPOLY# 4 5 B Polygon to the left of the arc

RPOLY# 4 5 B Polygon to the right of the arc

LENGTH 4 12 F 3 Length of arc in meters

DFIPLYCOMP# 4 5 B Unique internal control number

DFIPLYCOMP-ID 4 5 B Unique identification number

SYMB 3 3 I Symbol number

SEL 3 3 I Select number (1 or 0)

SHADED RELIEF BASE MAP

 The shaded-relief base map was derived from NOAA digital elevation data for northern North America, available from: http://www.ngdc.noaa.gov:80/seg/fliers/se-1104.html. The altitude data were downloaded from the NOAA web site and imported into ARC/INFO by Andrew Barron in the manner described here: Using the .HDR file downloaded, an ARC-compatible .HDR file was created. The raw data was treated as a .BIL image, and IMAGEGRID was used to convert it. For an unknown reason, negative elevation values (for example, elevations at Death Valley in California) were a huge number. By experimenting, this number was determined to be:

 (LARGE\_NUMBER) = 65,536 + (Negative Elevation)

This is intrinsic to the 16 bit data source, 2 to the 16th power (2^16) = 65,536.This problem was fixed by using the following GRID statement, where <ingrid> is the uncorrected elevation data and <outgrid> is the corrected data:

 <outgrid> = con(<ingrid> gt 4500,<ingrid> - 65536, <ingrid>)

 The 'gt 4500' part is related to the maximum elevation in meters, listed as 4328 in the NOAA HDR file. After correcting the grid values, the elevation data was projected using the parameters in Table 1.

The shaded-relief base map was made from the digital elevation model with the HILLSHADE command in ARC/INFO, using sun azimuth 315 degrees and altitude 45 degrees. The resulting grid was then processed to lighten the gray shades but preserve the topographic data, using the procedure described by Graham and Pike (1997). In the procedure described below, ‘ltgrid’ is the original shaded-relief, and ‘final\_grid’ is the lightened version:

 Step 1:

 ltgrid = SLICE(usa-hs\_val, EQINTERVAL, 100)

 Step 2: (use &describe on ltgrid before running this step)

 temp\_grid = (ltgrid - [value GRD$MEAN]) \* 15 / [value GRD$STDV] + 90

 Step 3:

 final\_grid = con(isnull(temp\_grid), 99, temp\_grid <= 60, 60,temp\_grid <=

 99, int(temp\_grid),99)

SUSCEPTIBILITY MAP

 The debris-flow susceptibility areas and the shaded relief background were plotted together using the ARCPLOT command GRIDCOMPOSITE HSV (hue, saturation, and value) to make the base for the final map.

#### REFERENCES CITED

Graham, S.E., and Pike, R.J., 1997, San Francisco Bay Landslide Folio part B - Shaded relief map of the San Francisco Bay region, California: U.S. Geological Survey Open-File Report 97-745 B.

Mark, R.K., 1992, Map of debris-flow probability, San Mateo County, California, U.S. Geological Survey Miscellaneous Investigations Map I-1257-M, scale 1:62,500.

Snyder, J.P., 1987, Map projections – a working manual: U.S. Geological Survey Professional Paper 1395.

Wentworth, C.M., and Fitzgibbon, T.T., 1991, ALACARTE user manual (version 1.0): U.S. Geological Survey Open-File Report 91-587C.

U.S. DEPARTMENT OF THE INTERIOR TO ACCOMPANY MAP MF-2329

U.S. GEOLOGICAL SURVEY

**APPENDIX 2**

**BIBLIOGRAPHY OF DEBRIS FLOWS BY STATE**

 References listed below are the data sources for each landslide or group of landslides in each state. References for individual landslides are shown as points on the map and references for groups of landslides are shown as areas or quadrangles on the map. Each reference is provided with a number in the order the material was received. This reference number is also provided in the digital database so that the sources of data can be linked to the individual landslide or group of landslides. The numbers are not shown on the plot for the map because they would overwhelm the data in several areas. The numbers in parentheses and brackets following each reference indicate the number of points or polygons in the database for that reference and the actual reference number(s) in the database for that point or polygon. For example, reference number 27 for California is: [6 PT (27), 1 PT (25,27,85)]. This means that 7 debris flow locations in the point database are from reference 27 and one is also mentioned in references 25 and 85.

 Nearly all the references are in the files of the U. S. Geological Survey Landslide Information Center in Golden, Colorado. The current curator of these files is Lynn Highland, P.O. Box 25046, MS 966, Lakewood, CO 80225, phone 303-273-8588. Email: highland@usgs.gov.

**Alabama**

1. Pomeroy, J.S., 1983, Relict debris flows in northeastern Pennsylvania: Northeastern Geology, v. 5, no. 1. [1PT (1)]

**Arizona**

1. Cooley, M.E., Aldridge, B.N., Euler, R.C., 1966, Effects of catastrophic flood of December 1966, North Rim area, eastern Grand Canyon, Arizona: U. S. Geological Survey Professional Paper 980, p. 43. [7 PT (1), 1 PT (1,5)]

3. Hereford, R., Thompson, K.S., and Burke, K.J., 1997, Dating prehistoric debris fans, Colorado River, Grand Canyon National Park, Arizona, with implications for channel evolution and river navigability: U.S. Geological Survey Open-File Report 97-167. [12 PT (3), 1 POLY (3)]

2. Moosburner, O., Glancy, P.A., 1978, Potential flood and debris hazards at Willow Beach, Lake Mead National Recreation area, Arizona: unpublished report. [1 POLY, (2)]

8. Murphy, B.J., and Moore, R.T., 1980, Maps showing relative slope stability and relative erodibility, central Santa Cruz river valley, Tucson area, Arizona: U.S. Geological Survey Miscellaneous Investigations Series Map I-844-O, 2 map sheets, scale 1:125,000. [6 PT (8)]

7. Realmuto, V.J., 1985, Preliminary map of selected mass movement events in Arizona: Arizona Bureau of Geology and Mineral Technology (written commun.), 10 p. [1 PT (7)]

4. Webb, R.H., Pringle, P.T., Reneau, P.T., and Rink, G.R., 1987, Monument Creek Debris flow, 1984-Implications for formation of rapids on the Colorado River in Grand Canyon National Park: Geology, v. 16, no. 1, p. 50-54. [1 POLY (4)]

5. Webb, R.H., Pringle, P.T., and Rink, G.R., 1987, Debris flows from tributaries of the Colorado River, Grand Canyon National Park, Arizona: U.S. Geological Survey Open File Report 87-118. [2 PT (5), 1 PT (1,5)]

6. Wohl, E.E., and Peartree, P.A., 1991, Debris flows as geomorphic agents in the Huachuca Mountains of Southeastern Arizona: Geomorphology, v. 4, no. 3-4, p. 273-292. [1 PT (6)]

**Arkansas**

1. McFarland, J.D., 1992, Landslide features of Crowley's Ridge: Arkansas Geological Commission Information Circular 31, 30 p. [2 POLY (1)]

**California**

2. Applied Earth Sciences, Inc., no date, Landslide inventory maps for Six Rivers National Forest: unpublished report. [1 PT (2)]

219. Barrows, A.G., 1986, Landslide hazards in the east half of the Val Verde quadrangle, Los Angeles County, California: California Division of Mines and Geology, Open-File Report 86-9LA (Landslide Hazard Identification Map No. 5), scale 1:24,000. [1 POLY (160, 219)]

136. Bawcom, J.A., and Spittler, T.E., 1995, The Floodgate landslide failure due to the March 1995 storms, Navarro River, Mendocino County, California: California Division of Mines and Geology, unpublished memo to J. Teie, California Department of Forestry, October 30. [1 PT (136)]

137. \_\_\_1997, Engineering geologic review of the Rancheria Creek landslide: California Division of Mines and Geology, unpublished memo to C.E., Anthony, California Department of Forestry, January 17. [1 PT (137)]

134. \_\_\_1997, Engineering review of two landslides in Jackson Demonstration State Forest: California Division of Mines and Geology, unpublished memo to C.E., Anthony, California Department of Forestry, February 2. [1 PT (134)]

4. Beaty, C.B., 1959, Desert flooding and debris‑flow deposition, California‑Nevada [abs.]: Geological Society of America Bulletin, v. 70, no 12, pt. 2, p. 1774. [1 POLY (4,5)]

3. \_\_\_1970, Age and estimated rate of accumulation of an alluvial fan, White Mountains, California: American Journal of Science, v. 268, no. 1, p. 50-77. [1 PT (3)]

5. \_\_\_1974, Debris flows, alluvial fans, and a revitalized catastrophism: Zeitschrift fur Geomorphologie, Supplementband 21, p. 39‑51. [1 POLY (4,5)]

7. Bedrossian, T.L., 1978, Geology and slope stability in the Geysers geothermal resources area: California Geology, v. 31, no. 7, p. 151‑159. [1 PT (7)]

141. \_\_\_1995, Boulder Creek debris flow: California Division of Mines and Geology, unpublished memo to N. Carr-Gordon, County of Santa Cruz Office of Emergency Services. [1 PT (141)]

6. Blackwelder, E., 1928, Mudflow as a geologic agent in semi‑arid mountains: Geological Society of America Bulletin, v. 39, no. 2, p. 465‑484. [1 PT (6)]

210. Bortugno, E.J., 1987, Landslide hazards in Benicia-Vallejo area, Solano County, California: California Division of Mines and Geology, Open-File Report 86-17SF (Landslide Hazard Identification Map no. 8), scale 1:24,000. [1 POLY (210), 1 POLY (128,210), 1 POLY (128,210,211)]

119. Brabb, E.E., Reconnaissance field investigations in California, 1982, 1983, 1984, 1985. [4 PT (119)]

10. Campbell, R.H., 1969, Rapid debris flows in the central Santa Monica Mountains, California [abs.]: Association of Engineering Geologists, Annual Meeting, San Francisco, Program Abstracts, p. 20‑21. [1 PT (10)]

11. \_\_\_1974, Debris flows originating from soil slips during rainstorms in southern California: Quarterly Journal of Engineering Geology, v. 7, no. 4, p. 339‑349. [1 POLY (11,12), 1 POLY (11,12,154), 1 POLY (11,12,218), 1 POLY (11,12,217,218), 1 POLY (11,12,154,217,218)]

12. \_\_\_1975, Soil slips, debris flows, and rainstorms in the Santa Monica Mountains and vicinity, Southern California: U.S. Geological Survey Professional Paper 851, p. 51‑70. [1 POLY (11,12), 1 POLY (11,12,154), 1 POLY (11,12,218), 1 POLY (11,12,217,218), 1 POLY (11,12,154,217,218)]

13. \_\_\_1980, Landslide maps showing field classification, Point Dume Quadrangle, California: U.S. Geological Survey Miscellaneous Field Studies Map MF‑1167, scale 1:24,000. [1 POLY (13), 1 POLY (13,218), 1 POLY (13,217,218)]

14. Cleveland, G.B., 1973, Fire + rain = mudflows; Big Sur, 1972: California Geology, v. 26, no. 6, p. 127‑139. [1 PT (14)]

15. Colman, S.M., 1973, History of mass movement processes in the Redwood Creek Basin, Humboldt County, California: Pennsylvania State University, unpublished Master’s thesis, 180 p. [1 POLY (15,69)]

16. Conwell, F.R., and Fuqua, W.D., 1960, Engineering geology of debris flows along the southwest side of the San Joaquin Valley, California, 1957‑59, *in* Regional subsidence exploration, debris flow study: California Department of Water Resources, Division of Design and Construction Engineering Laboratories, Exploration Section Report no. E‑3, 30 p. [1 POLY (16)]

17. Crandell, D.R., Mullineaux, D.R., Sigafoos, R.S., and Rubin, M., 1974, Chaos Crags eruptions and rockfall‑avalanches, Lassen Volcanic National Park, California: U.S. Geological Survey, Journal of Research, v. 2, no. 1, p. 49‑60. [1 PT (17,34)]

224. Crandell, D.R., Miller, C.D., Glicken, H.X., Christiansen, R.L., Newhall, C.G., 1984, Catastrophic debris avalanches from Mount Shasta volcano, California: Geology, v. 12, p. 143-146. [1 POLY (39,124, 146, 224)]

18. Crippen, J.R., 1979, Potential hazards from mudflows and debris movement in the Furnace Creek area, Death Valley National Monument, California-Nevada: U.S. Geological Survey Open-File Report 79‑991, 20 p. [1 PT (18)]

125. Cronin, V.S., Slosson, J.E., Slosson, T.L., and Shuirman, G., 1992, Deadly debris flows on I-5 near Grapevine, CA, *in* French, R. H., ed., Hydraulics, Hydrology of Arid Lands, Proceedings of the International Symposium: New York, American Society of Civil Engineers, p. 78-83. [1 PT (125)]

120. Davenport, C.W., 1982, Geology and geomorphic features related to landsliding, Smith River 7 1/2‑minute Quadrangle, Del Norte County, California: California Division of Mines and Geology, Open-File Report 83‑19 SF, scale 1:24,000. [1 POLY (44,109)]

19. \_\_\_1983, Geology and geomorphic features related to landsliding, High Divide 7.5‑minute quadrangle, Del Norte County, California: California Division of Mines and Geology Open-File Report 83‑18 SF, scale 1:24,000. [1 POLY (19)]

164. \_\_\_1983, Geology and geomorphic features related to landsliding, Hiouchi 7.5’ quadrangle, Del Norte County, California: California Division of Mines and Geology, Open-File Report 83-4 SF, scale1:24,000. [1 POLY (164)]

165. \_\_\_1983, Geology and geomorphic features related to landsliding, Leggett 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 83-40 SF, scale 1:24,000. [1 POLY (165)]

166. \_\_\_1984, Geology and geomorphic features related to landsliding, Tan Oak Park 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-17 SF, scale 1:24,000. [1 POLY (166)]

167. \_\_\_1984, Geology and geomorphic features related to landsliding, Point Arena 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-46 SF, scale 1:24,000. [1 POLY (167)]

168. \_\_\_1984, Geology and geomorphic features related to landsliding, Point Arena NE 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-47 SF, scale 1:24,000. [1 POLY (168)]

169. \_\_\_1984, Geology and geomorphic features related to landsliding, Gualala 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-48 SF, scale 1:24,000. [1 POLY (169)]

20. \_\_\_1984, Geology and geomorphic features related to landsliding, Noble Butte 7 1/2‑minute Quadrangle, Mendocino County, California: California Division of Mines and Geology Open‑File Report 83‑41 SF, scale 1:24,000. [1 POLY (20)]

21. \_\_\_1984, Geology and geomorphic features related to landsliding, Requa 7 1/2‑minute Quadrangle, Del Norte County, California: California Division of Mines and Geology Open‑File Report 84‑8 SF, scale 1:24,000. [1 POLY (21)]

22. \_\_\_1984, Geology and geomorphic features related to landsllding, Childs Hill 7 1/2‑minute Quadrangle, Del Norte County, California: California Division of Mines and Geology Open‑File Report 84‑7 SF, scale 1:24,000. [1 POLY (22)]

214. \_\_\_1984, An analysis of slope failures in eastern Marin County, California, resulting from the January 3rd and 4th, 1982, storm: California Division of Mines and Geology, OpenFileReport 84-22SF, scale 1:62,500. [1 POLY (128,212,213,214,222)]

140. \_\_\_1983, Sandy Beach road landslides, Solano County, California: California Division of Mines and Geology, unpublished memo to R.H. Sydnor, April 20. [1 PT (140)]

122. Degraff, J.V., 1994, The geomorphology of some debris flows in the southern Sierra Nevada, California: Geomorphology, v. 1, no. 4, p. 231-252. [29 PT (122)]

24. Durgan, P.B., 1977, Landslides and the weathering of granitic rocks: Geological Society of America, Reviews in Engineering Geology, v. 3, p. 127‑131. [1 PT (24)]

23. Dwyer, M.J., 1972, Landslides and related processes in the Round Valley‑Little Lake Valley and Fort Bragg region, Mendocino County, California, *in*  Geologic guide to the northern Coast Ranges; Lake, Mendocino, and Sonoma Counties, California: Geological Society of Sacramento, p. 33‑49. [1 PT (23)]

25. Ellen, S.M., Peterson, D.M., and Reid, G.O., 1982, Areas susceptible to shallow landsliding, Marin and Sonoma Counties, California: U.S. Geological Survey Miscellaneous Field Studies Map ME‑1406, scale 1:62,500. [1 PT (25,27,85)]

26. Ellen, S.M., Peterson, D.M., Reid, G.O., and Savina, M.E., 1979, Hillslope forms and landslide processes in erosional terrain on Franciscan rocks of the Marin Peninsula, California [abs. ]: Geological Society of America, Abstracts with Programs, v. 11, no. 3, p. 77. [1 PT (26)]

128. Ellen, S.D., Mark, R.K., Wieczorek, G.F., Wentworth, C.M., Ramsey, D.R., and May, T.E., 1997, Map of debris flow source areas in the San Francisco Bay Region, California: U.S. Geological Survey Open-File Report 97-745E (18,000 + debris flows from digital data). [3 POLY (128), 1 POLY (113, 128), 1 POLY (128,203), 1 POLY (128,204), 1 POLY (128,205), 2 POLY (128,206), 1 POLY (128,209), 1 POLY (128,210), 1 POLY (128,211), 1 POLY (128,210,211), 1 POLY (128,212,213,214,222)]

1. EOS, 1979, Predictable mudflows: EOS, v. 60, no. 11, p. 159. [1 PT (1,57,66,68,83)]

139. Falls, J.N., and Spittler, T.E., 1997, Preliminary engineering geologic review of debris flow at Stafford, Humboldt County, California: California Division of Mines and Geology, unpublished memo to C.E. Anthony, California Department of Forestry, March 12. [1 PT (139)]

152. Fife, D.L., 1974, Geology of the south half of the El Toro quadrangle, Orange County, California: California Division of Mines and Geology, Special Report 110, scale 1:12,000. [1 POLY (152), 1 POLY (152,215)]

27. Foggin, G.T., III, and Rice, R.M., 1979, Predicting slope stability from aerial photos: Journal of Forestry, v. 77, no. 2, p. 152‑155. [6 PT (27), 1 PT (25,27,85)]

31. Harp, E.L., and Herd, D.G., 1982, Debris flows induced by the January 3‑4, 1982, storm in Santa Cruz County, California [abs.]: Geological Society of America, Abstracts with Programs, v. 14, no. 7, p. 507‑508. [1 PT (31)]

211. Haydon, W.D., 1995, Landslide hazards in the Martinez-Orinda-Walnut Creek area, Contra Costa County, California: California Division of Mines and Geology, Open-File Report 95-12 (Landslide Hazard Identification Map no. 32), scale 1:24,000. [1 POLY (128,211), 1 POLY (128,210,211)]

131. Haydon, W.D., and Bedrossian, T.L., 1998, Engineering review of Rio Nido landslide, Sonoma County, California: California Division of Mines and Geology, unpublished memo to S. Covall, Sonoma County Emergency Services Coordinator, February 27. [1 PT (131)]

34. Heath, J.P., 1959, Dating chaos jumbles and avalanche‑deposits in Lassen National Park (California): American Journal of Science, v. 257, no. 7, p. 537-538. [1 PT (17,34)]

37. Highway research board #3, unpublished report. [1 PT (37)]

38. Highway research board #56, unpublished report. [1 PT (38)]

39. Hill, M., Egenhoff, E.L., 1977, A California Jokulhlaup: Earthquake Information Bulletin, v. 9, no. 1, p. 27‑31. [1 POLY (39,124, 146, 224)]

41. Holzhausen, G.R., 1974, The Lerida Court landslide of 1973: renewed failure within a prehistoric landslide system in Ladera, California: Stanford University, unpublished Master’s thesis. [1 PT (41)]

42. Hooke, R.L., 1967, Process on arid‑region alluvial fans: Journal of Geology, v. 75, p. 438‑460. [2 PT (42)]

43. Hsu, E.Y., 1982, Investigation and inventory of slope failures that occurred in 1978 and 1980 in the Los Angeles 7 1/2‑minute Quadrangle, Los Angeles County, California: California Division of Mines and Geology, Open‑File Report 82‑26 LA, 85 p. [1 POLY (43), 1 POLY (43,217)]

153. Hsu, E.Y., Saul, R.B., Tan, S.S., Treiman, J.A., and Weber, F.H., Jr., 1982, Slope stability and Geology of the Baldwin Hills, Los Angeles County, California: California Division of Mines and Geology, Special Report 152, 93 p. [1 POLY (153)]

127. Hubert, J.F., and Filipov, A.J., 1989, Debris-flow deposits in alluvial fans on the west flank of the White Mountains, Owens Valley, California, U.S.A: Sedimentary Geology, v. 61, p. 177-205. [7 PT (127)]

124. Hupp, C.R., Osterkamp, W.R., and Thornton, J.L., 1987, Dendrogeomorphic evidence and dating of recent debris flows on Mount Shasta, Northern California: U.S. Geological Survey Professional Paper, 1396-B. [1 POLY (39,124, 146, 224)]

154. Irvine, P.J., 1989, Landslide hazards in the north half of the Calabasas quadrangle, Los Angeles and Ventura Counties, California: California Division of Mines and Geology, Open-File Report 89-18 (Landslide Hazard Identification Map No. 20), scale 1:24,000. [1 POLY (154), 1 POLY (11,12,154), 1 POLY (154,218), 1 POLY (154,217,218), 1 POLY (11,12,154,217,218)]

155. \_\_\_1990, Landslide hazards in the Simi Valley area, Los Angeles and Ventura Counties, California: California Division of Mines and Geology, Open-File Report 90-17(Landslide Hazard Identification Map No. 22), scale 1:24,000. [1 POLY (155), 1 POLY (155,159), 1 POLY (155,160), 1 POLY (155,218)]

156. \_\_\_P.J., 1995, Landslide Hazards in the Moorpark and Santa Paula quadrangles, Ventura County, California: California Division of Mines and Geology, Open-File Report 95-07 (Landslide Hazard Identification Map No. 26), scale 1:24,000. [1 POLY (156,161), 1 POLY (156,159)]

142. \_\_\_P.J., and Bedrossian, T.L., 1995, Debris-flow activity resulting from January 1995 rainstorms in the city of Fillmore, Ventura County, California: California Division of Mines and Geology, unpublished memo to S.E. Jewett, U.S. Department of Agriculture, January 23, 1995. [1 PT (142)]

44. Jackson, L.E., 1977, Dating and recurrence frequency of prehistoric mudflows near Big Sur, Monterey County, California: U.S. Geological Survey, Journal of Research, v. 5, no. 1, p. 17‑32. [1 POLY (44,109)]

45. Lowney, J.V. and Associates, Phase II report, investigations of landslides, Six Rivers National Forest, Contract no. 39‑3327. [2 PT (45)]

46. Kelly, F.R., 1983, Geology and geomorphic features related to landsliding, Westport 7.5‑minute Quadrangle, Mendocino County, California: California Division of Mines and Geology, Open‑file Report 83‑32 SF, scale 1:24,000. [1 POLY (46)]

47. \_\_\_1983, Geology and geomorphic features related to landsliding, Dutchmans Knoll 7 1/2‑minute Quadrangle, Mendocino County, California: California Division of Mines and Geology, Open‑file Report 83‑33 SF, scale 1:24,000. [1 POLY (47)]

48. \_\_\_1983, Geology and geomorphic features related to landsliding, Lincoln Ridge 7 1/2‑minute Quadrangle, Mendocino County, California: California Division of Mines and Geology, Open‑file Report 83‑14 SF, scale 1:24.000. [1 POLY (48)]

170. \_\_\_1984, Geology and geomorphic features related to landsliding, Hales Grove 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-15 SF, scale 1:24,000. [1 POLY (170)]

171. \_\_\_1984, Geology and geomorphic features related to landsliding, Piercy 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-16 SF, scale 1:24,000. [1 POLY (171)]

172. \_\_\_1983, Geology and geomorphic features related to landsliding, Inglenook 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 83-315 SF, scale 1:24,000. [1 POLY (172)]

173. \_\_\_1984, Geology and geomorphic features related to landsliding, Arcata North 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-38 SF, scale 1:24,000. [1 POLY (173)]

174. \_\_\_1984, Geology and geomorphic features related to landsliding, Arcata South 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-39 SF, scale 1:24,000. [1 POLY (174)]

50. Kelsey, H.M., 1978, Earthflows in Franciscan melange, Van Duzen River basin, California: Geology, v. 6, no. 6, p. 361‑364. [1 POLY (49,50,51), 1 POLY (49,50,51,95), 1 POLY (49,50,51,186)]

51. \_\_\_1980, A sediment budget and an analysis of geomorphic process in the Van Duzen River basin, north coastal California, 1941‑1975: Geological Society of America Bulletin, vol. 91, no. 4, p. 1119‑1216. [1 POLY (49,50,51), 1 POLY (49,50,51,95), 1 POLY (49,50,51,186)]

49. \_\_\_1982, Hillslope evolution and sediment movement in a forested headwater basin, Van Duzen River, north coastal California, *in* Swanson, F. J., Janda, R. J., Dunne, T., and Swanston, D. N., eds., Sediment budgets and routing in forested drainage basins: U.S. Forest Service Pacific Northwest Forest and Range Experimental Station, General Technical Report PNW‑141. [1 POLY (49,50,51), 1 POLY (49,50,51,95), 1 POLY (49,50,51,186)]

52. Kilbourne, R.I., 1982, Geology and geomorphic features related to landsliding, Glenblair NW [Noyo Hill] 7.5‑minute Quadrangle, Mendocino County, California: California Division of Mines and Geology, Open file Report 82‑25 SF, scale 1:24,000. [1 POLY (52), 1 POLY (52,198)]

53. \_\_\_1983, Geology and geomorphic features related to landsliding, Glenblair SE [Comptche] 7 1/2 minute Quadrangle, Mendocino County, California: California Division of Mines and Geology, Open File Report 83‑21 SF, scale 1:24,000. [1 POLY (53)]

118. \_\_\_1983, Geology and geomorphic features related to landsliding, Fort Bragg 7 1/2‑minute Quadrangle, California: California Division of Mines and Geology, Open-File Report 83-55 SF, scale 1:24,000. [1 POLY (118)]

175. \_\_\_1983, Geology and geomorphic features related to landsliding, Mendocino 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 83-55 SF, scale 1:24,000. [1 POLY (175), 1 POLY (175,198)]

176. \_\_\_1984, Geology and geomorphic features related to landsliding, Longvale 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-18 SF, scale 1:24,000. [1 POLY (176)]

177. \_\_\_1984, Geology and geomorphic features related to landsliding, Willits [Burbeck] 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-19 SF, scale 1:24,000. [1 POLY (177)]

178. \_\_\_1984, Geology and geomorphic features related to landsliding, Willits SW [Greenough Ridge] 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-20 SF, scale 1:24,000. [1 POLY (178)]

179. \_\_\_1984, Geology and geomorphic features related to landsliding, Iron Peak 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-40 SF, scale 1:24,000. [1 POLY (179)]

180. \_\_\_1984, Geology and geomorphic features related to landsliding, Laytonville 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-41 SF, scale 1:24,000. [1 POLY (180)]

181. \_\_\_1984, Geology and geomorphic features related to landsliding, Boonville NW [Bailey Ridge] 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-42 SF, scale 1:24,000. [1 POLY (181)]

54. \_\_\_1984, Geology and geomorphic features related to landsliding, Sherwood Peak 7 1/2‑minute Quadrangle, Mendocino County, California: California Division of Mines and Geology, Open‑file Report 83‑38 SF, scale 1:24,000. [1 POLY (54)]

55. \_\_\_1984, Geology and geomorphic features related to landsliding, Cahto Peak 7 1/2‑minute Quadrangle, Mendocino County, California: California Division of Mines and Geology, Open‑file Report 83‑39 SF, scale 1:24,000. [1 POLY (55)]

192. \_\_\_1985, Geology and geomorphic features related to landsliding, Fortuna 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 85-1 SF, scale 1:24,000. [1 POLY (192)]

193. \_\_\_1985, Geology and geomorphic features related to landsliding, Hydesville 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 85-2 SF, scale 1:24,000. [2 POLY (193), 1 POLY (49,50,51,193)]

194. \_\_\_1985, Geology and geomorphic features related to landsliding, McWhinney Creek 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 85-3 SF, scale 1:24,000. ), [1 POLY (194), 1 POLY (49,50,51,194)]

195. \_\_\_1985, Geology and geomorphic features related to landsliding, Korbel 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 85-5 SF, scale 1:24,000. [1 POLY (195)]

56. Kilbourne, R.T., and Mata‑Sol, A.R., 1983, Geology and geomorphic features related to landsliding, Glenblair SW 7 1/2‑minute Quadrangle, Mendocino County, California: California Division of Mines and Geology, Open‑File Report 83‑20 SF, scale 1:24,000. [1 POLY (56), 1 POLY (56,198)]

196. Kilbourne, R.T., and Morrison, S.D., 1985, Geology and geomorphic features related to landsliding, Field’s Landing 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 85-4 SF, scale 1:24,000. [1 POLY (196)]

57. Kojan, E., 1979, The mudflow‑landslide hazard at Wrightwood, San Bernardino County, California: U.S. Forest Service, San Bernardino National Forest, California, Project no. O1601, 10 p. [1 PT (1,57,66,68,83)]

58. Lehre, A.K., 1982, Sediment mobilization and production from a small Coast Range catchment, Lone Tree Creek, Marin County, California: Unpublished Doctorate thesis, University of California, Berkeley, 235 p. [1 PT (58,59)]

59. \_\_\_1982, Sediment budget of a small Coast Range drainage basin in north‑central California, *in* Swanson, F.J., Janda, R.J., Dunne, T., and Swanston, D.N., eds., Sediment budgets and routing in forested drainage basins: U.S. Forest Service Pacific Northwest Forest and Range Experimental Station, General Technical Report PNW‑141. [1 PT (58,59)]

201. Majmundar, H.H., 1994, Landslide hazards in the Hollister area, San Benito County, California: California Division of Mines and Geology, Open-File Report 94-2 (Landslide Hazard Identification Map no. 30), scale 1:24,000. [1 POLY (201)]

202. \_\_\_1994, Landslide hazards in the Tres Pinos and Paicines area, San Benito County, California: California Division of Mines and Geology, Open-File Report 94-3 (Landslide Hazard Identification Map no. 31), scale 1:24,000. [1 POLY (202)

203. \_\_\_1995, Landslide hazards in the Hayward quadrangle and parts of the Dublin quadrangle, Alameda and Contra Costa Counties, California: California Division of Mines and Geology, Open-File Report 95-14 (Landslide Hazard Identification Map no. 37), scale 1:24,000. [1 POLY (203), 1 POLY (128,203)]

204. \_\_\_1995, Landslide hazards in the Las Trampas Ridge quadrangle and parts of the Diablo quadrangle, Alameda and Contra Costa Counties, California: California Division of Mines and Geology, Open-File Report 95-15 (Landslide Hazard Identification Map no. 38), scale 1:24,000. [1 POLY (128,204)]

205. \_\_\_1991, Landslide hazards in the Tassajara and Byron Hot Springs 7.5’ quadrangles, Alameda and Contra Costa Counties, California: California Division of Mines and Geology, Open-File Report 92-5, scale 1:24,000. [1 POLY (205), 1 POLY (128,205)]

206. \_\_\_1995, Landslide hazard in the Livermore Valley and vicinity, Alameda and Contra Costa Counties, California: California Division of Mines and Geology, Open-File Report 91-2 (Landslide Hazard Identification Map no. 21), scale 1:24,000. [1 POLY (206), 2 POLY (128,206)]

207. \_\_\_1989, Landslide hazards in the Vacaville area, Solano County, California: California Division of Mines and Geology, Open-File Report 89-17 (Landslide Hazard Identification Map no. 14), scale 1:24,000. [1 POLY (207)]

208. \_\_\_1987, Landslide hazards in south half of the Fairfield North quadrangle, Solano County, California: California Division of Mines and Geology, Open-File Report 87-9 (Landslide Hazard Identification Map no. 11), scale 1:24,000. [1 POLY (208)]

182. Manson, M.W., 1984, Geology and geomorphic features related to landsliding, Navarro NE [Navarro] 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-44 SF, scale 1:24,000. [1 POLY (182)]

183. \_\_\_1984, Geology and geomorphic features related to landsliding, Navarro SE [Cold Spring] 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-45 SF, scale 1:24,000. [1 POLY (183)]

184. \_\_\_1984, Geology and geomorphic features related to landsliding, Mallo Pass Creek 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-13 SF, scale 1:24,000. [1 POLY (184)]

185. \_\_\_1984, Geology and geomorphic features related to landsliding, Boonville SW [Philo] 7.5’ quadrangle, Mendocino County, California: California Division of Mines and Geology, Open-File Report 84-43 SF, scale 1:24,000. [1 POLY (185)]

61. \_\_\_1984, Geology and geomorphic features related to landsliding, Elk 7 1/2‑minute Quadrangle, Mendocino County, California: California Division of Mines and Geology, Open‑File Report 84‑12 SE, scale 1:24,000. [1 PT (61)]

209. \_\_\_1988, Landslide hazards in the Cordelia-Vallejo area, Solano and Napa Counties, California: California Division of Mines and Geology, Open-File Report 88-22 (Landslide Hazard Identification Map no. 13), scale 1:24,000. [2 POLY (209), 1 POLY (128,209)]

197. \_\_\_ 1989, Landslide hazards in the eastern Clear Lake area, Lake County, California: California Division of Mines and Geology, Open-File Report 89-27, scale 1:24,000. [1 POLY (197)]

62. Matthews, R.A., 1968, Geological hazards of Lake Tahoe Basin area, California and Nevada, *in* Evans, J.A., and Mathews, R.A., eds., Geological Society of Sacramento, Annual Field Trip Guidebook, p. 14-26. [1 POLY (62)]

63. McCaffrey, W.F., and DeGraff, J.V., 1982, Geologic resources inventory, geologic reconnaissance of surficial features Sierra National Forest: U.S. Forest Service, Sierra National Forest, California, 21 maps, scale 1:24,000. [2 POLY (63)]

199. McKittrick, M.A., 1995, Geology and geomorphic features related to landsliding, and relative landslide susceptibility categories, North Fork Mokelumne River, Amador County, California: California Division of Mines and Geology, Open-File Report 95-6, scale 1:24,000.

200. \_\_\_1995, Geology and geomorphic features related to landsliding, and relative landslide susceptibility categories, North Fork Gualala River, Mendocino County, California: California Division of Mines and Geology, Open-File Report 95-5, scale 1:24,000.

65. Merifield, P.M., 1984, Observations on slope failure associated with the rainstorms of 1978, 1980 and 1983 in southern California [abs.], *in* Bowles, D. S., ed., Delineation of landslide, flash flood and debris flow hazards in Utah; Proceedings of a specialty conference: Utah Water Research Laboratory, Logan, Utah, June 14‑15, 1984, p. 163-177. [1 PT (65,84)]

157. Miller, R.V., and Morton, P.K., 1984, Engineering geology of part of the western half of the Santiago Peak quadrangle, Orange County, California: California Division of Mines and Geology, Open-File Report 84-58LA, scale 1:12,000. [1 POLY (157), 1 POLY (157,215)]

158. Miller, R.V., and Siang, S.T., 1983, Geologic map of part of the south half of the Black Star Canyon Quadrangle, Orange County, California: California Division of Mines and Geology, Open-File Report 83-34LA, scale 1:12,000. [1 POLY (158), 1 POLY (158, 215)]

66. Morton, D.M., 1970, 1969 mudflows at Wrightwood, San Bernardino County, California [abs.]: Geological Society of America, Abstracts with Programs, v. 2, no. 2, p. 121‑122. [1 PT (1,57,66,68,83)]

67. \_\_\_1971, Seismically triggered landslides in the area above the San Fernando Valley: U.S. Geological Survey Professional Paper 733, p. 99‑104. [1 PT (67)]

159. \_\_\_1976, Reconnaissance surficial geologic maps of the Fillmore, Moorpark, Piru, and Simi 7.5’ quadrangles, Ventura County, southern California: U.S. Geological Survey Open-File Report 76-210, scale 1:24,000. [3 POLY (159), 1 POLY (155,159), 1 POLY (156,159)]

160. \_\_\_1976, Reconnaissance surficial geologic maps of the Newhall, Oat Mountain, Santa Susana, and Val Verde 7.5’ quadrangles, Los Angeles and Ventura Counties, southern California: U.S. Geological Survey Open-File Report 76-211, scale 1:24,000. [4 POLY (160), 1 POLY (155,160), 2 POLY (160,217), 1 POLY (160, 219), 1 POLY (160,220), 1 POLY (160,221), 1 POLY (160,217,221)]

161. \_\_\_1976, Reconnaissance surficial geologic maps of the Santa Paula, Santa Paula Peak, Saticoy, and Ojai 7.5’ quadrangles, Ventura County, southern California: U.S. Geological Survey Open-File Report 76-212, scale 1:24,000. [3 POLY (161), 1 POLY (156,161)]

68. Morton, D.M, and Campbell, R.H., 1974, Spring mudflows at Wrightwood, southern California: Quarterly Journal of Engineering Geology, v. 7, no. 4, p. 377‑384. [1 PT (1,57,66,68,83)]

162. Morton, P.K., 1974, Geology and engineering geologic aspects of the south half of the Canada Gobernadora quadrangle, Orange County, California: California Division of Mines and Geology, Special Report 111, scale 1:12,000. [1 POLY (162), 1 POLY (162, 215)]

163. Morton, P.K., Edgington, W.J., and Fife, D.L., 1974, Geology and engineering geologic aspects of the San Juan Capistrano quadrangle, Orange County, California: California Division of Mines and Geology, Special Report 112, scale 1:12,000. [1 POLY (163), 1 POLY (163, 215)]

215. Morton, P.K., Miller, R.V., and Fife, D.L., 1973, Geo-Environmental maps of Orange County, California: California Division of Mines and Geology, Preliminary Report 15, scale 1:48,000. [2 POLY (215), 1 POLY (152,215), 1 POLY (157,215), 1 POLY (158, 215), 1 POLY (162, 215), 1 POLY (163, 215), 1 POLY (215,216)]

69. Nolan, K.M., Harden, D.R., and Colman, S.M., 1976, Erosional landform map of the Redwood Creek drainage basin, Humboldt County, California, 1947-74: U.S. Geological Survey, Water Resources Investigations Open File Report OF-76-42, scale 1:62,500. [1 POLY (15,69)]

146. Osterkamp, W.R., Hupp, C.R., and Blodgett, J.C., 1986, Magnitude and frequency of debris flows, and areas of hazard on Mount Shasta, California: U.S. Geological Survey Professional Paper 1396-C, 21 p. [1 POLY (39,124, 146, 224)]

70. Pascocci, V.N., 1985, 475 landslides in the city of Pacifica, California [abs.], *in* Bowles, D. S., ed., Delineation of landslide, flash flood and debris flow hazards in Utah; Proceedings of a specialty conference: Utah Water Research Laboratory, Logan, Utah, June 14‑15, 1984, p. 99-112. [1 PT (70,87,150)]

72. Rantz, S.E., 1970, Urban sprawl and flooding in southern California: U.S. Geological Survey Circular 601‑B, 11 p. [1 PT (72)]

149. Reneau, S.E., and Dietrich, W.E., 1987, The importance of hollows in debris flow studies; Examples from Marin County, California: Geological Society of America Reviews in Engineering Geology, v. 7, p. 165-180. [3 PT (149)]

73. Renwick, H., Brumbaugh, R., and Loeher, L., 1982, Landslide morphology and processes on Santa Cruz Island, California: Geografiska Annaler, v. 64A, nos. 3-4, p. 149‑159. [1 PT (73)]

74. Rice, S.J., and Chase, G.B., 1973, Geology and geologic hazards of the Novato area, Marin County, California: California Division of Mines and Geology, Preliminary Report 21: 47 p., scale 1:12,000. [1 PT (74)]

222. Rice, S.J., and Strand, R.G., 1972, Geologic and slope stability maps of the Tennessee Valley, Lucas Valley, and north coastal areas, Marin County, California: California Division of Mines and Geology, Open-File Report 72-22, scale 1:12,000. [1 POLY (128,212,213,214,222)]

213. Rice, S.J., Smith, T.C., and Strand R.G., 1976, Geology for planning central and southeastern Marin County, California: California Division of Mines and Geology, Open-File Report 76-2, scale 1:12,000. [1 POLY (128,212,213,214,222)]

75. Richards, C.A., 1953, The mudflows of Mosaic Canyon, Death Valley National Monument, California: Compass of the Sigma Gamma Epsilon, v. 30, no. 4, p. 238-243. [1 PT (75)]

77. Rodine, J.D., 1975, Analysis of the mobilization of debris flows: Stanford University, unpublished Ph.D. thesis: 235 p. [1 PT (77,78)]

78. Rodine, J.D., and Johnson, A.M., 1976, The ability of debris, heavily freshened with coarse material, to flow on gentle slopes: Sedimentology, v. 23, no, p. 213-234. [1 PT (78), 1 PT (77,78)]

79. Saul, R. B., 1977, Geologic hazards, Mt. Wilson Quadrangle: California Geology, v. 30, no. 2, p. 35-36. [1 POLY (79). 1 POLY (79,217)]

150. Shlemon, R.J., Wright, R.H., and Montgomery, D.R., 1987, Anatomy of a debris flow, Pacifica, California: Geological Society of America Reviews in Engineering Geology, v. 7, p. 181-199. [1 PT (70, 87, 150)]

80. Schlocker, J., 1974, Geology of the San Francisco North Quadrangle, California: U.S. Geological Survey Professional Paper 782, 109 p., scale, 1:24,000. [1 POLY (80)]

138. Schlosser, J.P., and Spittler, T.E., 1995, Preliminary engineering geologic review of Snow Creek debris slide - on site of former THP 2-84-396 SIS (6): California Division of Mines and Geology, unpublished memo to L.I. Keefer, California Department of Forestry, August 4. [1 PT (138)]

81. Scott, K.M., 1971, Origin and sedimentation of 1969 debris flows near Glendora, California: U.S. Geological Survey Professional Paper 750‑C, p. C242-C247. [1 PT (81,104)]

82. Scott, K.M., and Williams, R.P., 1978, Erosion and sediment yield in the Transverse Range: U.S. Geological Survey Professional Paper 1030, 38 p. [1 PT (82)]

83. Sharp, R.P., and Nobles, L.H., 1953, Mudflow of 1941 at Wrightwood, southern California: Geological Society of America Bulletin, v. 64, no. 4, p. 547-560. [1 PT (1,57,66,68,83)]

84. Shuirman, G., Slosson, J.E., and Yoakum, D., 1985, Relationship of fire/flood to debris flows [abs.], *in* Bowles, D. S., ed., Delineation of landslide, flash flood and debris flow hazards in Utah; Proceedings of a specialty conference: Utah Water Research Laboratory, Logan, Utah, June 14‑15, 1984, p. 178-194. [1 PT (65,84)]

85. Siederman, D.J., Borum, J.D., 1983, Hillslope processes and urban planning, Larkspur, California: Siederman and Associates, Lafayette, CA, unpublished report. [1 PT (25,27,85)]

126. Slosson, J.E., and Slosson, T.E., 1992, Olancha debris flow: An example of an isolated damaging event, *in* French, Richard H. ed., Hydraulics, Hydrology of Arid Lands, Proceeding of the International Symposium: New York, American Society of Civil Engineers, p. 72-77. [1 PT (126)]

87. Smith, T.C., 1977, The debris avalanche; a commonly overlooked geologic hazard [abs.]: Geological Society of America Abstracts with Programs, v. 9, no. 4, p. 502. [1 PT (70,87,150)]

88. Smith, T.C., Hart, E.R., Baldwin, J.E., and Rodrigues, R.J., 1982, Landslides and related storm damage January 1982, San Francisco Bay Region: California Geology, v. 35, no. 7, p. 139‑152. [1 PT (88)]

147. Smith, T.C., 1985, Landslide hazards in the southeastern part of the Petaluma dairy belt, Sonoma County, California: California Division of Mines and Geology Open-File Report 85-5 SF, scale 1:24,000. [1 POLY (147)]

89. Spittler, T.E., 1983, Geology and geomorphic features related to landsllding, Scotia 7 1/2‑minute Quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 82‑20 SF, scale 1:24,000. [1 POLY (89)]

90. \_\_\_1983, Geology and geomorphic features related to landsliding, Bull Creek 7 1/2‑minute Quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 83‑3 SF, scale 1:24,000. [1 POLY (90)]

91. \_\_\_1983, Geology and geomorphic features related to landsliding, Miranda 7 1/2‑minute Quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 83‑25 SF, scale 1:24,000. [1 POLY (91)]

92. \_\_\_1983, Geology and geomorphic features related to landsliding, Garberville 7 1/2‑minute Quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 83‑26 SF, scale 1:24,000. [1 POLY (92)]

93. \_\_\_1983, Geology and geomorphic features related to landsliding, Weott 7 1/2‑minute Quadrangle, Humboldt County, California: California Division of Mines and Geology, Open File Report 83‑6 SF, scale 1:24,000. [1 POLY (93)]

94. \_\_\_1983, Geologic and geomorphic features related to landsliding, Myers Flat 7 1/2‑minute Quadrangle, Humboldt County, California: California Division of Mines and Geology, Open‑File Report OFR‑83‑22 SF, scale 1:24,000. [1 POLY (94)]

95. \_\_\_1983, Geologic and geomorphic features related to landsliding, Bridgeville 7 1/2‑minute Quadrangle, Humboldt County, California: California Division of Mines and Geology, Open‑File Report OFR‑83‑23 SE, scale 1:24,000. [1 POLY (95)]

186. \_\_\_1983, Geology and geomorphic features related to landsliding, Redcrest 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 83-17 SF, scale 1:24,000. [1 POLY (186), 1 POLY (49,50,51,186)]

187. \_\_\_1984, Geology and geomorphic features related to landsliding, Honeydew 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 84-11 SF, scale 1:24,000. [1 POLY (187)]

188. \_\_\_1984, Geology and geomorphic features related to landsliding, Capetown 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 84-34 SF, scale 1:24,000. [1 POLY (188)]

189. \_\_\_1984, Geology and geomorphic features related to landsliding, Ferndale 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 84-35 SF, scale 1:24,000. [1 POLY (189)]

190. \_\_\_1984, Geology and geomorphic features related to landsliding, Taylor Peak 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 84-36 SF, scale 1:24,000. [1 POLY (190)]

191. \_\_\_1984, Geology and geomorphic features related to landsliding, Buckeye Mountain 7.5’ quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 84-37 SF, scale 1:24,000. [1 POLY (191)]

96. \_\_\_1984, Geology and geomorphic features related to landsliding, Briceland 7 1/2‑minute Quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 84‑10 SF, scale 1:24,000. [1 POLY (96)]

117. \_\_\_1984 Geology and Geomorphic features related to landsliding, Harris 7 1/2‑minute Quadrangle, Humboldt County, California: California Division of Mines and Geology, Open-File Report 84‑9 SF, scale 1:24,000. [1 POLY (117)]

130. Spittler, T.E., and Bedrossian, T.L., 1995, Freezout road landslide - Sonoma County landslide evaluations: California Division of Mines and Geology, unpublished memo to A. Vellutini, Sonoma County Public Works, April 15. [1 PT (130)]

132. \_\_\_1995, Engineering reinspection of THP 1-93-315 SON: California Division of Mines and Geology, unpublished memo to L.I. Keefer, California Department of Forestry, March 13. [1 PT (132)]

135. \_\_\_1995, Geologic review inspection of THP 1-90-701 MEN: California Division of Mines and Geology, unpublished memo to L.I. Keefer, California Department of Forestry, January 30. [1 PT (135)]

133. \_\_\_1997, Engineering geologic reinspection review of THP 1-96-524 SON - Fisher Conversion landslides: California Division of Mines and Geology, unpublished memo to C.E. Anthony, California Department of Forestry, January 9. [1 PT (133)]

143. Spittler, T.E., Haydon, W.D., Bedrossian, T.E., 1995, Emergency review of landsliding along Big Sulphur Creek, Sonoma County, California: California Division of Mines and Geology, unpublished memo to R. King, U.S. Department of Agriculture, January 31. [1 PT (143)]

198. Spittler, T.E., and McKittrick, M.A., 1995, Geology and geomorphic features related to landsliding, North and South Forks of Caspar Creek, Mendocino County, California: California Division of Mines and Geology, Open-File Report 95-8, scale 1:12,000. [1 POLY (52,198), 1 POLY (56,198), 1 POLY (175,198)]

97. Swanston, D.N., Shanson, F.J., Coates, D.R., 1976, Timber harvesting, mass erosion, and steepland forest geomorphology in the Pacific Northwest, *in* Geomorphology and Engineering: Dowden, Hutchinson and Ross, Inc., p. 199‑221. [1 PT (97)]

144. Tan, S.S., and Bedrossian, T.L., 1998, Debris-flow and landslide hazards in the city of Laguna Beach, Orange County, California: California Division of Mines and Geology, unpublished memo to K.C. Frank, City Manager, Laguna Beach, California, April 17, 1998. [1 PT (144)]

216. Tan, S.S., and Edgington, W.J., 1976, Geology and engineering geologic aspects of the Laguna Beach quadrangle, Orange County, California: California Division of Mines and Geology, Special Report 127, scale 1:12,000. [1 POLY (216), 1 POLY (215,216)]

220. Treiman, J.A., 1986, Landslide hazards in the west half of the Newhall quadrangle, Los Angeles County, California: California Division of Mines and Geology, Open-File Report 86-6 LA (Landslide Hazard Identification Map No. 2), scale 1:24,000. [1 POLY (160,220)]

221. \_\_\_1987, Landslide hazards in the north half of the Oat Mountain quadrangle, Los Angeles County, California: California Division of Mines and Geology, Open-File Report 87-8 LA (Landslide Hazard Identification Map No. 10), scale 1:24,000. [1 POLY (160,221), 1 POLY (160,217,221)]

30. Troxell, H.C., and Peterson, J.Q., 1937, Flood in La Cãnada Valley, California, *in* Grover, N. C. (ed.), Contributions to the hydrology of the United States: U.S. Geological Survey Water Supply Paper 796. [1 POLY (30), 1 POLY (30,217)]

98. U.S. Forest Service, Klamath National Forest, Timber sales report, 7/23/74; Oak Knoll Ranger District: Klamath National Forest, CA. [1 PT (98)]

100. U.S. Forest Service, Klamath National Forest, 1970, Timber sales report, 12/4/70; Klamath National Forest, CA. [1 PT (100)]

101. U.S. Forest Service, Klamath National Forest, 1977, Timber sales report, 1977; Klamath National Forest, CA. [1 PT (101)]

103. U.S. Forest Service, Klamath National Forest, 1970, Timber sales report, 1/19/70 (debris flows inferred); Klamath National Forest, CA. [1 PT (103)]

123. U.S. Forest Service, Region 5, Debris flows near Lake Tahoe: Earth Resources Monograph 14. [2 PT (123)]

212. Wagner, D.L., 1977, Geology for planning in Western Marin County, California: California Division of Mines and Geology, Open-File Report 77-15 SF, scale 1:12,000. [1 POLY (128,212,213,214,222)]

104. Washington Post, 1969, Floods in California kill at least 11: The Washington Post, Washington, D.C., January 26, 1969, p. A1. [1 PT (81,104)]

105. \_\_\_1972, Huge mudslide wipes out center of Big Sur: The Washington Post, Washington D. C., November 17, 1972, p. A3. [1 PT (105)]

223. Weber, F.H., 1980, Landsliding and flooding in Southern California during the winter of 1979-80, California Division of Mines and Geology, Open-File Report 80-3 LA. [15 PT (223)]

217. Weber, F.H., Treiman, J.A., Tan, S.S., Miller, R.V., 1979, Landslides in the Los Angeles Region, California- Effects of February-March 1978 rains: California Division of Mines and Geology, Open-File Report 79-4 LA. [4 POLY (217), 1 POLY (30,217), 1 POLY (43,217), 1 POLY (79,217), 2 POLY (160,217), 2 POLY (217,218), 1 POLY (13,217,218), 1 POLY (11,12,217,218), 1 POLY (154,217,218), 1 POLY (11,12,154,217,218), 1 POLY (160,217,221)]

218. Weber, F.H., and Wills, C.J., 1983, Map showing landslides of the central and western Santa Monica Mountains, Los Angeles and Ventura Counties, California: California Division of Mines and Geology, Open-File Report 83-16, scale 1:48,000. 1 POLY (218), 1 POLY (11,12,218), 1 POLY (13,218), 1 POLY (154,218), 1 POLY (155,218), 2 POLY (217,218), 1 POLY (13,217,218), 1 POLY (11,12,217,218), 1 POLY (154,217,218), 1 POLY (11,12,154,217,218)]

151. Wells, W.G. II, 1987, The effects of fire on the generation of debris flows in southern California: Geological Society of America Reviews in Engineering Geology, v. 7, p. 105-124. [1 POLY (151)]

121. Wieczorek, G.F., 197, Landslide susceptibility evaluation in the SantaCruz Range, San Mateo County, California: University of California, Berkeley, Ph. D. thesis, 223 p. [1 PT (110,111,121,129,148)]

110. \_\_\_1982, Map showing recently active and dormant landslides near La Honda, central Santa Cruz Mountains, CA: U.S. Geological Survey, Miscellaneous Field Studies Map MF-1422, scale 1:4,800. [1 PT (110,111,121,129,148)]

109. \_\_\_1983, Written communication (air photos, 3/25/83). [1 POLY (44,109,120)]

148. \_\_\_1987, Effect of rainfall intensity and duration on debris flows in central Santa Cruz Mountains, California: Geological Society of America Reviews in Engineering Geology, v. 7, p. 93-104.

 [1 PT (110,111,121,129,148)]

111. Wieczorek, G.F., Sarmiento, J., 1983, Significance of storm intensity‑duration for triggering debris flows near La Honda, California: Geological Society of America Abstracts with Programs, v. 15, no. 5. [1 PT (110,111,121,129,148)]

113. Williamson, J.A., 1975, Landslide susceptibility near Tomales Bay, California: San Francisco State University, unpublished Master’s thesis, 113 p. [1 POLY (113)]

145. Wills, C., 1999, written communication: unpublished field notes from 1995. [3 PT (145)]

129. Wilson, R.C., and Wiezorek, G.F., 1995, Rainfall Thresholds for the initiation of debris flows at La Honda, California: Environmental and Engineering Geoscience, v. 1, no. 1, p. 11-27. [1 PT (110,111,121,129,148)]

114. Wright, R.H., and Reid, G.O., 1975, Photointerpretlve map of landslides and surficial deposits of northernmost Napa County, California: U.S. Geological Survey, Miscellaneous Field Studies Map MF‑677, scale 1:24,000. [1 POLY (114)]

116. Zielbauer, E.J., 1966, Flood control problems encountered in southern California, *in* Lung, R., and Proctor, R., eds.,Engineering geology in southern California, Association of Engineering Geologists Special Report. [1 PT (116)]

**Colorado**

2. Brabb, E.E., Reconaissance field investigations in Colorado, 1982, 1983, 1985, 1987. [6 PT (2)]

29. Cannon, S.H., Powers, P.S., Pihl, R.A., Rogers, W.P., 1995, Preliminary evaluation of fire-related debris flows on Storm King Mountain, Glenwood Springs, CO: U.S. Geological Survey, Open File Report 95-508. [1 PT (29)]

30. Chleborad, A.F., Ellis, W.L., and Kibler, D., 1997, Results of site investigation and instrumentation of the Keno gulch landslide/debris-flow source area, Aspen, CO: U.S. Geological Survey, Open File Report 97-717. [1 PT (30)]

3. Clark, J.A., 1974, Mudflows in the San Juan Mountains, Colorado; controls and work: University of Colorado, unpublished Master's thesis. [1 POLY (3) 1 POLY (3,9,23)]

44. Coe, J.A., and Godt, J.W., 1997, Characteristics of alluvial fans from tributaries of Clear Creek, Floyd Hill, Colorado: Geological Society of America Abstracts with Programs, 1997. [1 POLY (44)]

5. Costa, J.E., and Jarrett, R.D., 1981, Debris flows in small mountain stream channels of Colorado and their hydrologic implications: Association of Engineering Geologists Bulletin, v. 18, no. 3, p. 309‑322. [7 PT (5)]

6. Curry, R.R., 1966, Observations of an alpine mudflow in the Tenmile Range, central Colorado: Geological Society of America Bulletin, v. 77, no. 7, p. 771-776. [1 PT (6)]

7. Fleming, R.W., 1975, Debris flows and debris fans: Colorado Geological Survey Special Publication 8, p. 27-31. [2 PT (7)]

33. Hammack, L., and Wohl, E., 1996, Debris-fan formation and rapid modification at Warm Springs Rapid, Yampa River, Colorado: Journal of Geology, v. 104, no. 6, p. 729-740. [1 PT (33)]

8. Hansen, W.R., 1973, Effects of the May 5‑6, 1973, storm in the greater Denver area, Colorado: U.S. Geological Survey Circular 689, 20 p. [2 PT (8)]

9. Ives, J.D., and Bovis, M.J., 1978, Natural hazards maps for land‑use planning, San Juan Mountains, Colorado, USA, *in* Ives, J.D., and Zimina, R.P., eds., Mountain geoecology and land‑use implications: Arctic and Alpine Research, v. 10, no. 2, p. 185-212 (debris fans). [1 POLY (9)]

10. Ives, J.D., Mears, A.I., Carrara, P.E., and Bovis, M.J., 1976, Natural hazards in mountainous Colorado: Association of American Geographers Annals, v. 66, no. 1, p. 129-144. [1 PT (10)]

31. Jochim, C.L., 1986, Debris flow hazard in the immediate vicinity of Ouray, Colorado: Colorado Geological Survey, Special Publication 30, 63 p., 1 pl., scale 1:24000. [1 POLY (31)]

12. Junge, W.R.,1978, Geologic hazards upper Crystal River area, Gunnison County, Colorado: Colorado Geological Survey, Open‑File Report 78‑11, scale 1:24,000. [1 POLY (12,16)]

13. Mears, A.I., 1977, Debris‑flow hazard analysis and mitigation; an example from Glenwood Springs, Colorado: Colorado Geological Survey, Information Series, v. 8, 45 p. [1 PT (13,14,45)]

45. Mejia-Navarro, M., Wohl, E.E. , and Oaks, S.D., 1994, Geological hazards, vulnerability, and risk assesment using GIS, a model for Glenwood Springs, Colorado: Geomorphology, v. 10, p. 331-354. [1 PT (13,14,45)]

34. Montezuma Valley Journal, 1979, Slides on Mesa Verde: Cortez, Colorado, April 20, *in* Chleborad, A.F., 1997, Temperature, snowmelt, and the onset of spring season landslides in the central Rocky Mountains: U.S. Geological Survey Open-File Report 97-27, p. 3. [1 PT (34,35)]

35. \_\_\_ 1979, Mesa Verde remains closed: Cortez, Colorado, May 2, *in* Chleborad, A.F., 1997, Temperature, snowmelt, and the onset of spring season landslides in the central Rocky Mountains: U.S. Geological Survey Open-File Report 97-27, p. 3 [1 PT (34,35)]

14. Morris, R.N., and Weaver, M.T., 1978, Geologic hazards of the Glenwood Springs metropolitan area, Garfield County, Colorado: Colorado Geological Survey, Open‑File Report 78‑10, 27 p. [1 PT (13,14,45)]

32. Pendleton, J.A., 1987, The Boulder area debris flows, *in* Atkinson, William A. ed., Urban Geology hazards of the Boulder area: Geological Society of America, Rocky Mountain Section Annual Meeting, 40th, Field Trip #6 Guide Book, May 6, 1987. [1 PT (32)]

43. Rocky Mountain News, 1983, Mudslide blocks I-70 as rain sweeps state: Denver, Colorado, Aug. 15. [1 PT (44)]

16. Rogers, W.P., and Rold, J.W., 1972, Engineering geologic factors of the Marble area, Gunnison County, Colorado: Colorado Geological Survey, 44 p. [1 POLY (12,16)]

19. \_\_\_1975, Geologic hazards map, Idaho Springs, Clear County, Colorado. [1 PT (19)]

20. \_\_\_1976, Geologic hazards in the Crested Butte‑Gunnison area, Gunnison County, Colorado: Colorado Geological Survey, Information Service 5, 34 p. [2 PT (20)]

21. \_\_\_1976, Geomorphology of geologic hazards in the Big Thompson Canyon area, Larimer County, Colorado, *in* The Big Thompson Flood of 1976: Geological Society of America, Annual Meeting, Field Trip Guidebook, Denver, CO, May 8-11. [1 POLY (21)]

22. Soule, J.M., and Fleming, R.W., 1977, Debris avalanches and debris flows in Douglas County, Colorado; processes and hazards [abs.]: Geological Society of America Abstracts with Programs, v. 9, no. 6, p. 765. [1 PT (22)]

36. Steamboat Pilot, 1982, Mud slides damage ski jumps: Steamboat Springs, Colorado, May 13, p. 1 *in* Chleborad, A.F., 1997, Temperature, snowmelt, and the onset of spring season landslides in the central Rocky Mountains: U.S. Geological Survey Open-File Report 97-27, 35 p. [1 PT (36)]

37. \_\_\_1982, See me, see mudslide: Steamboat Springs, Colorado, May 27, p. 1 *in* Chleborad, A.F., 1997, Temperature, snowmelt, and the onset of spring season landslides in the central Rocky Mountains: U.S. Geological Survey Open-File Report 97-27, 35 p. [1 PT (37)]

38. \_\_\_1984, Rising waters flood Route County: Steamboat Springs, Colorado, May 17, p. 1 *in* Chleborad, A.F., 1997, Temperature, snowmelt, and the onset of spring season landslides in the central Rocky Mountains: U.S. Geological Survey Open-File Report 97-27, 35 p. [1 PT (38)]

39. \_\_\_1993, "...mudslide... won't be the last one of the spring" [Photo Caption]: Steamboat Springs, Colorado, May 6, p. 1 *in* Chleborad, A.F., 1997, Temperature, snowmelt, and the onset of spring season landslides in the central Rocky Mountains: U.S. Geological Survey Open-File Report 97-27, 35 p. [1 PT (39)]

40. \_\_\_ 1993, Mud slides run down ski area: Steamboat Springs, Colorado, May 27, p. 1 *in* Chleborad, A.F., 1997, Temperature, snowmelt, and the onset of spring season landslides in the central Rocky Mountains: U.S. Geological Survey Open-File Report 97-27, 35 p. [1 PT (40)]

42. Stover, B.K., Cannon, S.H., and Junge, R.W., 1987, The April 30, 1987 Telluride Airport landslides and resultant debris flows: Colorado Geological Survey Department of Natural Resources Open-File Report 87-2, 14 p., *in* Chleborad, A.F., 1997, Temperature, snowmelt, and the onset of spring season landslides in the central Rocky Mountains: U.S. Geological Survey Open-File Report 97-27, 35 p. [1 PT (42)]

23. Summer, R.M., 1976, Role of avalanches and debris flows in soil development, San Juan Mountains, Colorado [abs.]: Geological Society of America, Abstracts with Programs, v. 8, no. 5, p. 638. [1 POLY (23)]

41. Telluride Times, 1984, Woman dies in mud slide; melting snow wrecks county roads: Telluride, Colorado, May 17, p. 1 *in* Chleborad, A.F., 1997, Temperature, snowmelt, and the onset of spring season landslides in the central Rocky Mountains: U.S. Geological Survey Open-File Report 97-27, 35 p. [1 PT (41)]

24. U.S. Forest Service, 1982, Index of landslide problems in the San Juan National Forest: written commun. [1 PT (24)]

25. \_\_\_1982, Index of landslide problems in the White River National Forest: written commun. [2 PT (25)]

26. \_\_\_1982, Index of landslide problems in the Arapaho National Forest: written commun. [1 PT (26)]

27. Wallace, R.G., 1968, Types and rates of alpine mass movement, west edge of Boulder County, Colorado Front Range [abs.]: Dissertation Abstracts International, v. 28, no. 12, pt. 1, p. 5086B. [1 POLY (27)]

28. Yeend, W.E., 1973, Slow‑sliding slumps, Grand Mesa, Colorado: The Mountain Geologist, v. 10, no. 1, p. 25‑28. [1 PT (28)]

**Georgia**

1. Brabb, E.E., Reconnaissance field investigations in Georgia, 1982, 1983. [1 PT (1)]

3. Clark, G.M., 1987, Debris slide and debris flow events in the Appalachians south of the glacial border: Geological Society of America Reviews in Engineering Geology, v. 7, p. 125 - 129. [2 PT (3)]

2. Shadburn, M.L., 1982, Results of a Highway Research Board Questionnaire, 1953: Georgia Dept. of Highways, written commun. [1 PT (2)]

4. Thomas, R.E., 1979, Landslides and related features of the New Home and Trenton Quadrangles, Georgia, Alabama, and Tennessee: U.S. Geological Survey Open-File Report 79-944. [1 POLY (4)]

**Idaho**

1. Brabb, E.E., Reconaissance field investigations in Idaho, 1982, 1983, 1984. [11 PT (1)]

6. Breckenridge, R.M., and Adams, W.C., 1988, The Landslide Inventory of Idaho: Idaho Geological Survey: unpublished report. [91 PT (6)]

3. Day, N.F., and Megahan, W.F., 1975, Landslide occurrence on the Clearwater National Forest: U.S. Forest Service, Clearwater National Forest, Idaho, 6 p., appendices. [6 POLY (3)]

4. \_\_\_1976, Landslide occurrence on mountainous terrain in north‑central Idaho; a progress report, 1974‑1975: 14th Annual Engineering Geology and Soils Symposium, Proceedings, p. 85‑97. [1 PT (4)]

**Illinois**

1. Hester, N.C., and DuMontelle, P.B., 1971, Pleistocene mudflow along the Shelbyville Moraine Front, Macon County, Illinois, *in* Till; a Symposium: Ohio State University Press, Columbus, OH, p. 367-382. [1 PT (1)]

2. Hunt, S.R., Regional geologic control in a landslide area along the Illinois River Valley [abs.]: Geological Society of America, Abstracts with Programs, v. 6, no. 6, p. 517. [3 PT (2)]

**Kentucky**

1. Clark, G.M., 1987, Debris slide and debris flow events in the Appalachians south of the glacial border: Geological Society of America Reviews in Engineering Geology, v. 7, p. 125 - 129. [2 PT (1)]

2. Outerbridge, W.F., 1982, Landslides and related features of the Artemus, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (2)]

3. \_\_\_1979, Landslides and related features of the Bar Creek, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (3)]

9. \_\_\_1979, Landslides and related features of the Big Creek, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (9)]

10. \_\_\_1979, Landslides and related features of the Blackwater, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (10)]

11. \_\_\_1979, Landslides and related features of the Blackey, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (11)]

13. \_\_\_1979, Landslides and related features of the Booneville, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (13)]

15. \_\_\_1979, Landslides and related features of the Buckhorn, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (15)]

18. \_\_\_1979, Landslides and related features of the Canoe, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (18)]

19. \_\_\_1979, Landslides and related features of the Carrie, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (19)]

20. \_\_\_1979, Landslides and related features of the Cowcreek, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (20)]

21. \_\_\_1979, Landslides and related features of the Creekville, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (21)]

22. \_\_\_1979, Landslides and related features of the Cutshin, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (22)]

25. \_\_\_1979, Landslides and related features of the Dorton, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (25)]

26. \_\_\_1979, Landslides and related features of the Elkhorn City, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (26)]

39. \_\_\_1979, Landslides and related features of the Lick Creek, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (39)]

40. \_\_\_1979, Landslides and related features of the Leatherwood, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (40)]

41. \_\_\_1979, Landslides and related features of the Krypton, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (41)]

42. \_\_\_1979, Landslides and related features of the Kite, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (42)]

43. \_\_\_1979, Landslides and related features of the Jenkins West, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (43)]

44. \_\_\_1979, Landslides and related features of the Jamboree, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (44)]

45. \_\_\_1979, Landslides and related features of the Hyden West, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (45)]

46. \_\_\_1979, Landslides and related features of the Hyden East, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (46)]

47. \_\_\_1979, Landslides and related features of the Hazard South, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (47)]

48. \_\_\_1979, Landslides and related features of the Hoskinston, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (48)]

49. \_\_\_1979, Landslides and related features of the Hindman, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (49)]

50. \_\_\_1979, Landslides and related features of the Hima, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (50)]

51. \_\_\_1979, Landslides and related features of the Hellier, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (51)]

52. \_\_\_1979, Landslides and related features of the Hazard North, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (52)]

53. \_\_\_1979, Landslides and related features of the Handshoe, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (53)]

54. \_\_\_1979, Landslides and related features of the Haddix, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (54)]

68. \_\_\_1979, Landslides and related features of the Portersburg, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (68)]

69. \_\_\_1979, Landslides and related features of the Pikeville, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (69)]

70. \_\_\_1979, Landslides and related features of the Oneida, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (70)]

71. \_\_\_1979, Landslides and related features of the Ogle, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (71)]

72. \_\_\_1979, Landslides and related features of the Noble, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (72)]

73. \_\_\_1979, Landslides and related features of the Mistletoe, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (73)]

74. \_\_\_1979, Landslides and related features of the Millard, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (74)]

75. \_\_\_1979, Landslides and related features of the McKee, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (75)]

76. \_\_\_1979, Landslides and related features of the McDowell, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (76)]

77. \_\_\_1979, Landslides and related features of the Maulden, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (77)]

78. \_\_\_1979, Landslides and related features of the Mayking, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (78)]

79. \_\_\_1979, Landslides and related features of the Manchester, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (79)]

104. \_\_\_1979, Landslides and related features of the Whitesburg, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (104)]

105. \_\_\_1979, Landslides and related features of the Wheelwright, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (105)]

106. \_\_\_1979, Landslides and related features of the Wayland, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (106)]

107. \_\_\_1979, Landslides and related features of the Vicco, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (107)]

108. \_\_\_1979, Landslides and related features of the Vest, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (108)]

109. \_\_\_1979, Landslides and related features of the Tyner, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (109)]

110. \_\_\_1979, Landslides and related features of the Tilford, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (110)]

111. \_\_\_1979, Landslides and related features of the Sturgeon, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (111)]

112. \_\_\_1979, Landslides and related features of the Roxana, KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (112)]

4. \_\_\_1982, Landslides and related features of the Barbourville, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (4)]

5. \_\_\_1982, Landslides and related features of the Balkan, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (5)]

6. \_\_\_1982, Landslides and related features of the Beattyville, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (6)]

7. \_\_\_1982, Landslides and related features of the Bellfry, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (7)]

8. \_\_\_1982, Landslides and related features of the Beverly, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (8)]

12. \_\_\_1982, Landslides and related features of the Bledsoe, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (12)]

14. \_\_\_1982, Landslides and related features of the Broad Bottom, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (14)]

16. \_\_\_1982, Landslides and related features of the Campton, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (16)]

17. \_\_\_1982, Landslides and related features of the Cannel City, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (17)]

23. \_\_\_1982, Landslides and related features of the David, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (23)]

24. \_\_\_1982, Landslides and related features of the Dingus, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (24)]

27. \_\_\_1982, Landslides and related features of the Ezel, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (27)]

28. \_\_\_1982, Landslides and related features of the Louellen, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (28)]

29. \_\_\_1982, Landslides and related features of the Levee, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (29)]

30. \_\_\_1982, Landslides and related features of the Lenox, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (30)]

31. \_\_\_1982, Landslides and related features of the Leighton, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (31)]

32. \_\_\_1982, Landslides and related features of the Lee City, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (32)]

33. \_\_\_1982, Landslides and related features of the Landsaw, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (33)]

34. \_\_\_1982, Landslides and related features of the Lancer, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (34)]

35. \_\_\_1982, Landslides and related features of the Jackson, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (35)]

36. \_\_\_1982, Landslides and related features of the Ivyton, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (36)]

37. \_\_\_1982, Landslides and related features of the Irvine, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (37)]

38. \_\_\_1982, Landslides and related features of the Inez, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (38)]

55. \_\_\_1982, Landslides and related features of the Helton, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (55)]

56. \_\_\_1982, Landslides and related features of the Frakes, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (56)]

57. \_\_\_1982, Landslides and related features of the Heidelberg, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (57)]

58. \_\_\_1982, Landslides and related features of the Hazel Green, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (58)]

59. \_\_\_1982, Landslides and related features of the Harold, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (59)]

60. \_\_\_1982, Landslides and related features of the Guage, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (60)]

61. \_\_\_1982, Landslides and related features of the Frenchburg, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (61)]

62. \_\_\_1982, Landslides and related features of the Quicksand, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (62)]

63. \_\_\_1982, Landslides and related features of the Prestonburg, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (63)]

64. \_\_\_1982, Landslides and related features of the Pomeroyton, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (64)]

65. \_\_\_1982, Landslides and related features of the Paintsville, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (65)]

66. \_\_\_1982, Landslides and related features of the Oil Springs, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (66)]

67. \_\_\_1982, Landslides and related features of the Offutt, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (67)]

80. \_\_\_1982, Landslides and related features of the Nolansburg, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (80)]

81. \_\_\_1982, Landslides and related features of the Middlesboro North, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (81)]

82. \_\_\_1982, Landslides and related features of the Pineville, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (82)]

83. \_\_\_1982, Landslides and related features of the Milo, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (83)]

84. \_\_\_1982, Landslides and related features of the Meta, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (84)]

85. \_\_\_1982, Landslides and related features of the Means, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (85)]

86. \_\_\_1982, Landslides and related features of the Martin, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (86)]

87. \_\_\_1982, Landslides and related features of the White Oak, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (87)]

88. \_\_\_1982, Landslides and related features of the West Liberty, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (88)]

89. \_\_\_1982, Landslides and related features of the Varney, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (89)]

90. \_\_\_1982, Landslides and related features of the Tiptop, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (90)]

91. \_\_\_1982, Landslides and related features of the Thomas, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (91)]

92. \_\_\_1982, Landslides and related features of the Tallega, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (92)]

93. \_\_\_1982, Landslides and related features of the Stanton, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (93)]

94. \_\_\_1982, Landslides and related features of the Slade, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (94)]

95. \_\_\_1982, Landslides and related features of the Sitka, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (95)]

96. \_\_\_1982, Landslides and related features of the Seitz, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (96)]

97. \_\_\_1982, Landslides and related features of the Scranton, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (97)]

98. \_\_\_1982, Landslides and related features of the Salyersville South, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (98)]

99. \_\_\_1982, Landslides and related features of the Salyersville North, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (99)]

100. \_\_\_1982, Landslides and related features of the Richardson, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (100)]

101. \_\_\_1982, Landslides and related features of the Wallins Creek, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (101)]

102. \_\_\_1982, Landslides and related features of the Varilla, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (102)]

103. \_\_\_1982, Landslides and related features of the Scalf, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (103)]

113. \_\_\_1982, Landslides and related features of the Fount, KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (113)]

114. \_\_\_1982, Landslides and related features of the Cobhill, KY quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (114)]

**Massachusetts**

1. Cleland, H.F., 1902, The Landslides of Mt. Greylock and Briggsville, Mass: Geology, vol. 10, p. 513. [1PT (1)]

**Montana**

1. Brabb, E.E., Reconaissance field investigations in Montana, 1982, 1985. [4 PT (1)]

2. Bartholomew, M.J., 1984, compilation of 1004 landslides from the literature pertaining to western Montana: Montana Bureau of Mines and Geology, unpublished report. [17 PT (2)]

3. Butler, D.R., 1976, Aerial‑photo interpretation of mass‑wasting deposits, Glacier National Park, Montana [abs.]: American Quaternary Association, National Conference Abstracts, v. 4, p. 127. [1 PT (3)]

4. \_\_\_1983, Observations of historic high magnitude mass movements, Glacier National Park, Montana: The Mountain Geologist, v. 20, no. 2, p. 59‑62. [1 PT (4)]

8. \_\_\_1989, Glacial hazards in Glacier National Park, Montana: Physical Geography v. 10, no. 1, p. 53-71. [1 PT (8)]

5. Cox, W.E., 1977, The 1975 Goldcreek, Montana, landslide: 15th Annual Engineering Geology, Soils Engineering Symposium, Proceedings, p. 149‑159. [1 PT (5)]

6. Padden, J.W., 1982, Map showing two landslides in the Helena National Forest: written commun. 8/17/82. [1 PT (6)]

7. Parret, C., 1988, Fire-related debris-flows in the Beaver Creek drainage, Lewis and Clark County, Montana, *in* Subitzky, S., ed., Selected Papers in the hydrologic sciences: U.S. Geological Survey Water-Supply Paper 2330, p. 57-67. [1 POLY (7)]

**Nevada**

1. Bell, J., 1976, notes on the Hidden Valley mudflow of August, 1976, written commun. [1 PT (1)]

2. Blackwelder, E., 1928, Mudflow as a geologic agent in semiarid mountains: Geological Society of America Bulletin, v. 39, no. 2, p. 465-484. [1 PT (2)]

3. Brabb, E.E., Reconaissance field investigations in Nevada, 1982, 1983, 1984, 1987. [15 PT (3), 1 POLY (3)]

4. Bluck, B.J., 1964, Sedimentation of an alluvial fan in southern Nevada: Journal of Sedimentary Petrology, v. 34, no. 2, p. 395-400 (mud flow). [1 PT (4)]

10. Coe, J.A., Glancy, PA, and Whitney, J.W., 1997, Volumetric analysis and hydrologic characterization of a modern debris flow near Yucca Mountain, Nevada: Geomorphology, v. 20, p. 11-28. [1 PT (10)]

5. Glancy, P.A., 1969, A mudflow in the Second Creek drainage, Lake Tahoe basin, Nevada, and its relation to sedimentation and urbanization: U.S. Geological Survey Professional Paper 650‑C, p. C195‑C200. [1 PT (5)]

6. \_\_\_1985, The Ophir Creek debris flood of May 30, 1983; a real test of geohydrologic hazard mapping [abs.], *in* Bowles, D. S., ed., Delineation of landslide, flash flood and debris flow hazards in Utah; Proceedings of a specialty conference: Utah Water Research Laboratory, Logan, Utah, June 14‑15, 1984, p. 195-196. [1 PT (6,8)]

9. Grose, T.L.T., 1984, Geologic Map of the State Line Peak Quadrangle, Nevada - California: Nevada Bureau of Mines and Geology, Map 82, scale 1:24,000. [1 PT (9)]

7. Katzer, T.J., and Schroer, C.V., 1981, Flood and related debris flow hazards map, Carson City Quadrangle: Nevada Bureau of Mines and Geology, Urban Map, scale 1:24,000. [1 POLY (7)]

8. Watters, R.J., 1983, A landslide induced waterflood‑debris flow: International Association of Engineering Geology Bulletin (Paris, France), v. 28, p. 177‑182. [1 PT (8)]

**New Hampshire**

1. Flaccus, E., 1958, White Mountain landslides: Appalachia, v. 24, no. 12, p. 175‑191. [1 PT (1,2), 1 PT (1,3)]

2. Hitchcock, C.H., 1885, The recent landslide in the White Mountains: Science, vol. 6, no. 130, p. 85-87. [1 PT (1,2)]

3. Pirsson, L.V., and Rice, W.N., 1911, Geology of Tripyramid Mountain: American Journal of Science, 4th Series, v. 31, p. 269‑274. [1 PT (1,3)]

**New Jersey**

3. Asbury Park Press, 1999, Digging into mudslide mystery, Highlands, New Jersey, January 5. [1 PT (2,3,4)]

4. \_\_\_1999, History repeats in Highlands, Highlands, New Jersey, January 11. [1 PT (2,3,4)]

2. Minard, J.P., 1974, Slump blocks in the Atlantic Highlands of New Jersey, U.S. Geological Survey Professional Paper 898. [1 PT (2,3,4)]

1. Star-Ledger, 1996, Mudslide wipes out home, Sparta, New Jersey, January 20. [1 PT (1)]

**New Mexico**

5. Cardinali, M., Guzzetti, F., and Brabb, E.E., 1990, Preliminary maps showing landslide deposits and related features in New Mexico: U.S. Geological Survey Open-File Report 90-293, 4 map sheets, scale 1:500,000. [3402 PT (5)]

1. Hunt, C.B., 1977, Surficial geology of northeast New Mexico, geologic map 40: New Mexico Bureau of Mines and Mineral Resources, Division of New Mexico Institute of Mining and Technology, scale 1:500,000. [2 PT (1)]

2. \_\_\_1978, Surficial geology of northwest New Mexico, geologic map 43: New Mexico Bureau of Mines and Mineral Resources, Division of New Mexico Institute of Mining and Technology; scale 1:500,000. [3 PT (2)]

3. Leach, L., 1982, More mudslides predicted in Red River area: Albuquerque Journal, July 23, 1982. [1 PT (3)]

4. Watson, R.A., and Wright, H.E., Jr., 1963, Landslides on the east flank of the Chuska Mountains, northeastern New Mexico: American Journal of Science, v. 261, no. 6, p. 525‑548. [1 PT (4)]

**New York**

1. Bougucki, D.J., 1977, Debris slide hazard in the Adirondack Province of New York State: Environmental Geology, v. 1, p. 317‑328. [1 PT (1)]

3. Fickies, R.H., and Brabb, E.E., 1989, Landslide inventory map of New York: New York State Museum - Geological Survey Circular 52, scale 1:500,000. [69 PT (3)]

2. Renwick, W.H., 1977, Erosion caused by intense rainfall in a small catchment in New York State: Geology, v. 5, p. 361‑364. [1 PT (2)]

**North Carolina**

7. Clark, G.M., 1987, Debris slide and debris flow events in the Appalachians south of the glacial border: Geological Society of America Reviews in Engineering Geology, v. 7, p. 125 - 129. [19 PT (7)]

1. Glass, F.R., 1981, Unstable rock slopes along Interstate 40 through Pigeon River Gorge, Haywood County, North Carolina: Annual Highway Geology Symposium, 32nd Proceedings, Gatlinburg, TN, 15 p. [1 PT (1)]

3. Gryta, J.J., and Bartholomew, M.S., 1977, Evidence for late Cenozoic debris-avalanche type deposits in Watuga County, North Carolina: Geological Society of America Southeastern Section, Abstracts with Programs, p. 142-143. [1 PT (3,4)]

4. \_\_\_1977, Evidence for late Cenozoic debris-avalanche type deposits in Watauga Co., North Carolina: Geological Society of America Abstracts with Programs, v. 9, no. 2, p. 142-143. [1 PT (3,4)]

5. Lewis, S.E., 1983, Geologic investigations in the Blue Ridge of northwestern North Carolina: Carolina Geological Society Field Trip Guide Book (North Carolina Division of Land Resources). [1 PT (5)]

9. Neary, D.G., and Swift, L.W., Jr., 1987, Rainfall threshold for triggering a debris avalanching event in the southern Appalachian Mountains: Geological Society of America Reviews in Engineering Geology, v. 7, p. 81 -92. [1 POLY (6,9)]

6. Pomeroy, J.S., 1991, Map showing late 1977 debris flows near Asheville, western North Carolina: U.S. Geological Survey Open-File Report 91-334, scale 1:24,000. [1 POLY (6,9)]

8. Water Resources Branch, 1949, Floods of August 1940 in the southeastern states: U.S. Geological Survey Water-Supply Paper 1066. [1 POLY (8)]

10. Gardner, C.H., 1999, written commun.

**Ohio**

2. Davies, W.E., and Ohlmacher, G.C., 1978, Landslides and related features of the Knoxville, Ohio - West Virginia quadrangle: U.S. Geological Survey Open-File Report 78-1057. [1 POLY (2)]

1. Hackman, R.J., 1978, Landslides and related features of the Round Bottom, Ohio - West Virginia quadrangle: U.S. Geological Survey Open-File Report 78-1056. [1 POLY (1)]

**Oregon**

11. Anonymous, 1974, Mudslide at Canyonville Oregon: Engineering News Record, 1974. [1 PT (11)]

1. Beaulieu, J.D., 1973, Environmental geology of the inland Tillamook and Clatsop Counties, Oregon: Oregon Department of Geology and Mineral Industries, Bulletin 79, scale 1:62,500. [1 PT (1)]

2. \_\_\_1977, Geologic hazards of parts of northern Hood River, Wasco, and Sherman Counties, Oregon: Oregon Department of Geology and Mineral Industries Bulletin 91, scale 1:63:360. [2 PT (2)]

3. \_\_\_1978, Surficial geologic hazard concepts for Oregon: Oregon Department of Geology and Mineral Industries Bulletin, v. 40, no. 3, p. 41‑56. [1 PT (3)]

4. Beaulieu, J.D., and Hughes, P.W., 1974, Environmental geology of western Linn County, Oregon: Oregon Department of Geology and Mineral Industries, Bulletin 84, scale 1:62,500. [1 PT (4)]

5. \_\_\_1975, Environmental geology of western Coos and Douglas Counties, Oregon: Oregon Department of Geology and Mineral Industries Bulletin 87 [3 PT (5)]

6. Bela, J.L., 1979, Geologic hazards of eastern Benton County, Oregon: Oregon Department of Geology and Mineral Industries Bulletin 98, [1 PT (6)]

7. \_\_\_1980, Geologic hazards of eastern Benton County, Oregon [abs.]: Geological Society of America, Abstracts with Programs, v. 12, no. 3, p. 96. [1 PT (7)]

22. Benda, L., 1984, Debris flows in the Oregon Coast Range‑ Predicting behavior and risk to fish habitats, *in* Bowles, D.S., ed., Delineation of landslide, flash flood and debris flow hazards in Utah; Proceedings of a specialty conference: Utah Water Research Laboratory, Logan, Utah, June 14‑15, 1984, p. 153-162. [1 PT (22)]

23. \_\_\_1990, Influence of debris flows on channels and valley floors in the Oregon Coast Ranges: Earth Surface Processes and Landforms, v. 15, no. 5, p. 457-446. [1 POLY (23)]

8. Brabb, E.E., Reconaissance field investigtaions in Oregon, 1982, 1985. [4 PT (8)]

10. Dyrness, C.T., 1967, Mass soil movements in the H. J. Andrews experimental forest: U.S. Forest Service, Pacific Northwest Forest and Range Experiment Station, Research Paper PNW‑42, 13 p. [1 PT (10)]

12. Friday, J., 1983, Debris flow hazard assessment for the Oregon Caves National Monument: U.S. Geological Survey, Water Resources Investigations Report 85‑4100, 20 p. [1 PT (12)]

24. Gallino, G.L., 1985, Pollalie Creek debris flow and subsequent dam-break flood of 1980, East Fork Hood River basin, Oregon: U.S. Geological Survey Water-Supply Paper 2273. [1 PT (24)]

13. Hicks, B.A., 1982, Geology, geomorphology, and dynamics of mass movement in parts of the middle Santiam River drainage, West Cascades, Oregon: Oregon State University, unpublished M.S. thesis, 168 p. [1 PT (13)]

14. Hicks, B.G., 1976, Upper Applegate River Basin landslide study - Rogue River National Forest: U.S. Corp. of Engineers, 33 p., scale 1:62,500. [1 POLY (14)]

15. Higgins, J.D., Naik, B., Mills, S.V., Copp, H., Roberson, J.A., 1983, The mechanics of mudflows: State of Washington, Water Research Center Report 51, 116 p. [1 PT (15,18)]

25. Johnson, S.E., 1997, 1996 Tumult Creek debris flows and debris avalanches in the Columbia River Gorge east of Portland, Oregon, *in* Chen, Cheng-lung, ed., First International Symposium on debris-flow hazards mitigation: New York, American Society of Civil Engineers, p. 395 - 404. [1 PT (25)]

16. Ketcheson, G., and Froehlich, H.A., 1978, Hydrologic factors and environmental impacts of mass soil movements in the Oregon Coast Range: Oregon State University, Corvallis, Water Resources Research Institute, WRRI 56, 33 p. [1 PT (3 PT (16)]

17. Meyers, R., 1972, Trucker recalls slamming into muck, debris: Landslide, v. 1, no. 1, p. 26. [1 PT (17)]

18. Schlicker, H.G., and Finlayson, C.T., 1979, Geology and geologic hazards of northwestern Clackamas County, Oregon: Oregon Department of Geology and Mineral Industries, Bulletin 99, 79 p., scale 1:24,000. [4 PT (18), 1 PT (15,18)]

20. Swanson, F.J., and Swanston, D.N., 1977, Complex mass‑movement terrains in the western Cascade Range, Oregon: Geological Society of America, Reviews in Engineering Geology, v. 3, p. 113‑126. [1 PT (20)]

21. Washington Post, 1982, Mudslide at Little Lobster Creek: Washington Post, March 3, 1982. [1 PT (21)]

**Pennsylvania**

9. Clark, G.M., 1987, Debris slide and debris flow events in the Appalachians south of the glacial border: Geological Society of America Reviews in Engineering Geology, v. 7, p. 125 - 129. [2 PT (9)]

1. Johnson, A.M., Rahn, P.H., 1970, Mobilization of debris flows: Zeitschrift für Geomorphologie, v. 9, p. 168‑186. [1 PT (1)]

2. Pomeroy, J.S., 1979, Storm‑induced landslides in the Johnstown area, Pennsylvania, July 19‑20, 1977 [abs.]: Geological Society of America Abstracts with Programs, v. 11, no. 1, p. 49 (debris avalanches). [1 PT (2,3,4)]

11. \_\_\_1979, Landslides and related features of the Bolivar, PA quadrangle: U.S. Geological Survey Open-File Report 79-1314, scale 1:24,000. [1 POLY (11)]

12. \_\_\_1979, Landslides and related features of the Cassville, PA quadrangle: U.S. Geological Survey Open-File Report 79-1314, scale 1:24,000. [1 POLY (12)]

13. \_\_\_1979, Landslides and related features of the Huntingdon, PA quadrangle: U.S. Geological Survey Open-File Report 79-1314, scale 1:24,000. [1 POLY (13)]

14. \_\_\_1979, Landslides and related features of the Westline, PA quadrangle: U.S. Geological Survey Open-File Report 81-238, scale 1:24,000. [1 POLY (14)]

3. \_\_\_1980, Storm‑induced debris avalanching and related phenomena in the Johnstown area, Pennsylvania, with references to other studies in the Appalachians: U.S. Geological Survey Professional Paper 1191, 24 p. [1 PT (2,3,4)]

4. \_\_\_1982, Geomorphic effects of the July 19‑20, 1977, storm in a part of the Little Conemaugh River area northeast of Johnstown, Pennsylvania: Northeastern Geology, v. 4, no. 1, p. 1‑9. [1 PT (2,3,4)]

5. \_\_\_1982, Landslides in the greater Pittsburgh region, Pennsylvania: U.S. Geological Survey Professional Paper 1228, 48 p. [1 PT (5)]

6. \_\_\_1983, Relict debris flows in northwestern Pennsylvania: Northeastern Geology, v. 5, no. 1, p. 1‑7. [11 PT (6)]

10. \_\_\_1984, Storm-induced slope movements at East Brady, northwestern Pennsylvania: U.S. Geological Survey Bulletin 1618, 16 p. [1 PT (10)]

7. Stewart, J.E., 1952, Notable local floods of 1942-43, *in* Eisenlohr, W. S., ed., Floods of July 18, 1942 in North‑Central Pennsylvania: U.S. Geological Survey, Water‑Supply Paper 1134‑B, p. 75-78. [1 PT (7)]

8. Wilshusen, J.P., 1979, Geologic hazards in Pennsylvania: Pennsylvania Geologic Survey, Educational Series 9, p. 56. [9 PT (8)]

##### South Dakota

1. Crandell, D.R., 1952, Landslides and rapid-flowage phenomena near Pierre, South Dakota: Economic Geology, v. 47, no. 5, p. 548-568. [1 PT (1)]

2. Harwood, D.G., 1994, Processes and rates of shoreline bluff recession at Lake Sharpe, South Dakota: Bulletin of the Association of Engineering Geologists, v. 31, no. 1, p. 5-13. [1 POLY (2)]

##### Tennessee

1. Bogucki, D.J., 1971, Debris slides and related flood damage associated with the September 1, 1951, cloudburst in the Mt. Le Conte‑Sugarland Mountain area, Great Smoky Mountains National Park [abs.]: Dissertation Abstracts International, v. 32, no. 1, p. 365B‑366B. [1 PT (1,2)]

2. \_\_\_1976, Debris slides in the Mt. Le Conte area, Great Smoky Mountains National Park, U.S.A: Geografiska Annaler, v. 58, no. 3, p. 179‑191. [1 PT (1,2)]

4. Clark, G.M., 1987, Debris slide and debris flow events in the Appalachians south of the glacial border: Geological Society of America Reviews in Engineering Geology, v. 7, p. 125 - 129. [11 PT (4)]

8. Outerbridge, W.F., 1981, Landslide and related features of the Bald Knob, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (8)]

7. \_\_\_1982, Landslide and related features of the Ausmus, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (7)]

10. \_\_\_1982, Landslide and related features of the Big Ridge Park, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (10)]

17. \_\_\_ 1982, Landslide and related features of the Coleman Gap, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (17)]

18. \_\_\_1982, Landslide and related features of the Clouds, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (18)]

25. \_\_\_ 1982, Landslide and related features of the Fork Ridge, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (25)]

31. \_\_\_ 1982, Landslide and related features of the Howard Quarter, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (31)]

35. \_\_\_ 1982, Landslide and related features of the Lee Valley, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (35)]

37. \_\_\_ 1982, Landslide and related features of the Luttrell, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (37)]

44. \_\_\_1982, Landslide and related features of the Powder Springs, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (44)]

56. \_\_\_ 1982, Landslide and related features of the Well Spring, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (56)]

57. \_\_\_1982, Landslide and related features of the Wheeler, TN quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (57)]

9. Taylor, A.R., and Thomas, R.E., 1982, Landslide and related features of the Barthell S.W., TN quadrangle: U.S. Geological Survey Open-File Report 82-6535, scale 1:24,000. [1 POLY (9)]

5. Thomas, R.E., 1981, Landslide and related features of the Altamont, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (5)]

6. \_\_\_1981, Landslide and related features of the Alto, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (6)]

11. \_\_\_1981, Landslide and related features of the Brayton, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (11)]

12. \_\_\_1981, Landslide and related features of the Brockdell, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (12)]

13. \_\_\_1981, Landslide and related features of the Burrow Cave, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (13)]

14. \_\_\_1981, Landslide and related features of the Cane Hollow, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (14)]

15. \_\_\_1981, Landslide and related features of the Cardwell Mountain, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (15)]

19. \_\_\_1981, Landslide and related features of the Collins, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (19)]

20. \_\_\_1981, Landslide and related features of the Curtistown, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (20)]

21. \_\_\_1981, Landslide and related features of the Daus, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (21)]

22. \_\_\_1981, Landslide and related features of the DeRossett, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (22)]

23. \_\_\_1981, Landslide and related features of the Dorton, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (23)]

26. \_\_\_1981, Landslide and related features of the Grassy Grove, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (26)]

27. \_\_\_1981, Landslide and related features of the Henson Gap, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (27)]

28. \_\_\_1981, Landslide and related features of the Herbert Domain, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (28)]

29. \_\_\_1981, Landslide and related features of the Hillsboro, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (29)]

32. \_\_\_ 1981, Landslide and related features of the Irving College, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (32)]

34. \_\_\_1981, Landslide and related features of the Ketner Gap, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (34)]

36. \_\_\_ 1981, Landslide and related features of the Lonewood, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (36)]

38. \_\_\_1981, Landslide and related features of the Melvine, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (38)]

39. \_\_\_1981, Landslide and related features of the Melvine, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (39)]

40. \_\_\_1981, Landslide and related features of the Mount Airy, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (40)]

41. \_\_\_1981, Landslide and related features of the Orme, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (41)]

42. \_\_\_1981, Landslide and related features of the Pikeville, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (42)]

43. \_\_\_1981, Landslide and related features of the Pitcher Ridge, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (43)]

45. \_\_\_1981, Landslide and related features of the Sampson, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (45)]

46. \_\_\_1981, Landslide and related features of the Savage Point, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (46)]

47. \_\_\_1981, Landslide and related features of the Sequatchie, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (47)]

48. \_\_\_1981, Landslide and related features of the Sewanee, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (48)]

49. \_\_\_1981, Landslide and related features of the Sinking Cove, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (49)]

50. \_\_\_1981, Landslide and related features of the South Pittsburg, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (50)]

51. \_\_\_1981, Landslide and related features of the Tracy City, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (51)]

52. \_\_\_1981, Landslide and related features of the Vandever, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (52)]

53. \_\_\_1981, Landslide and related features of the Viola, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (53)]

54. \_\_\_1981, Landslide and related features of the Wauhatchie, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (54)]

55. \_\_\_1981, Landslide and related features of the Welchland, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (55)]

58. \_\_\_ 1981, Landslide and related features of the White City, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (58)]

59. \_\_\_1981, Landslide and related features of the Whitwell, TN quadrangle: U.S. Geological Survey Open-File Report 81-1318, scale 1:24,000. [1 POLY (59)]

16. Thomas, R.E., and Taylor, A.R., 1982, Landslide and related features of the Clarkrange, TN quadrangle: U.S. Geological Survey Open-File Report 82-653, scale 1:24,000. [1 POLY (16)]

24. \_\_\_1982, Landslide and related features of the Duncan Flats, TN quadrangle: U.S. Geological Survey Open-File Report 82-653, scale 1:24,000. [1 POLY (24)]

30. \_\_\_1982, Landslide and related features of the Honey Creek, TN quadrangle: U.S. Geological Survey Open-File Report 82-653, scale 1:24,000. [1 POLY (30)]

33. \_\_\_1982, Landslide and related features of the Jacksboro, TN quadrangle: U.S. Geological Survey Open-File Report 82-653, scale 1:24,000. [1 POLY (33)]

**Texas**

1. Lovejoy, E.M.P., 1972, Wisconsin boulder flow and its geomorphic implications, Franklin Mountains, El Paso County, Texas: Geologic Society of America Bulletin, v. 83, p. 3501‑3508. [1 PT (1)]

**Utah**

38. Baum, R.L., and Fleming, R.W., 1989, Landslides and debris flows in Ephraim Canyon, Central Utah, *in* Landslide Processes and theory: U.S. Geological Survey Bulletin 1842. [1 PT (38)]

2. Blackwelder, E., 1928, Mudflows as a geologic agent in semiarid mountains: Geological Society of America Bulletin, v. 39, no. 2, p. 465‑480. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

3. Brabb, E.E., Reconnaissance field investigations in Utah, 1982, 1983. See also: Brabb, E.E., Wieczorek, G.F., and Harp, E.L., 1989, Map showing 1983 landslides in Utah: U.S. Geological Survey Miscellaneous Field Studies Map MF-2085, scale 1:500,000. [2 PT (3)]

4. Brabb, E.E., and Harp, E., transcripts of plane flight above Utah, June 13‑18, 1983. See also: Brabb, E.E., Wieczorek, G.F., and Harp, E.L., 1989, Map showing 1983 landslides in Utah: U.S. Geological Survey Miscellaneous Field Studies Map MF-2085, scale 1:500,000. [4 POLY (4), 1 PT (4)]

6. Crawford, A.L. and Thackwell, F.E., 1931, Some aspects of the mudflows north of Salt Lake City, Utah: Utah Academy of Science, Proceedings, v. 8, p. 97‑105. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

8. Desert News, 1984, Moving mud swallows traintrack; Potential slides dot the Wasatch, May 16. [1 PT (8)]

9. Fleming, R.W., Schuster, R.L., Johnson, R.B., and Robinson, S.L., 1977, Recent movement of the Manti, Utah, landslide: 15th Annual Engineering Geology and Soils Engineering Symposium, Proceedings, p. 161‑178. [1 PT (9,34)]

10. Fuller, H.K., Williams, V.S., and Colton, R.B., 1981, Map showing areas of landsliding in the Kaiparowits coal-basin area, Utah: U.S. Geological Survey, Miscellaneous Investigation Series Map I-1033-H; scale 1:125,000. [3 PT (10), 1 POLY (10)]

11. Godfrey, A.E., 1980, Debris avalanche deposits north of Mount Ellen, *in* Picard, M. D. (ed.), Henry Mountains Symposium: Utah Geological Association Publication, v. 8, p. 171-176. [1 PT (11)]

40. Harty, K.M., 1991, Landslide map of the Trenton 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [6 PT (40)]

41. \_\_\_1991, Landslide map of the Logan 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [12 PT (41)]

42. \_\_\_1991, Landslide map of the Promontory Point 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [4 PT (42)]

43. \_\_\_1991, Landslide map of the Ogden 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [292 (43)]

44. \_\_\_1991, Landslide map of the Tooele 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [50 PT (44)]

45. \_\_\_1991, Landslide map of the Salt Lake City 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [386 PT (45)]

46. \_\_\_1991, Landslide map of the Dutch John 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [1 PT (46)]

47. \_\_\_1991, Landslide map of the Rush Valley 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [36 PT (47)]

48. \_\_\_1991, Landslide map of the Provo 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [250 PT (48)]

49. \_\_\_ 1991, Landslide map of the Nephi 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [1128 (49)]

50. \_\_\_ 1991, Landslide map of the Price 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [2 PT (50)]

51. \_\_\_1991, Landslide map of the Tule Valley 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [4 PT (51)]

52. \_\_\_1991, Landslide map of the Salina 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [2 PT (52)]

53. \_\_\_1991, Landslide map of the Beaver 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [1 PT (53)]

54. \_\_\_1991, Landslide map of the La Sal 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [1 PT (54)]

55. \_\_\_1991, Landslide map of the Cedar City 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [1 PT (55)]

56. \_\_\_1991, Landslide map of the Saint George 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [1 PT (56)]

57. \_\_\_1991, Landslide map of the Kanab 30° by 60° quadrangle, Utah: Utah Geological Survey Open-File Report, (digital data - http://its.state.ut.us/agrc), scale 1:100,000. [1 PT (57)]

13. Kaliser, B.N., 1983, Geologic Hazards of 1983: Utah Geological and Mineralogical Survey, Quarterly Review, v. 3, no. 3, p. 2. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

14. \_\_\_1972, Environmental geology of Bear Lake area, Rich County, Utah: Utah Geological and Mineralogical Survey Bulletin 96, 32 p. [1 PT (14)]

15. \_\_\_not dated, Environmental geology and geological hazards in Utah; a photographic series: Utah Geological and Mineralogical Survey, Earth Science Education Series Report 2, 5 p. [1 POLY (15)]

16. Lips, E.W., Wieczorek, G.F., Boschetto, H.B., 1984, Factors influencing debris-flow runout, *in* Bowles, D.S., ed., Delineation of landslide, flash flood and debris flow hazards in Utah; Proceedings of a specialty conference, Logan: Utah Water Research Laboratory, RG85-3, p. 115. [4 PT (16)]

17. Marshall, R.E., 1949, The Quaternary system in Utah, *in* The oil and gas possibilities of Utah, Utah Geological and Mineralogical Survey, p. 109‑118. [1 PT (17,32)]

18. Miller, R.D., 1980, Surficial map along part of the Wasatch Front, Salt Lake Valley, Utah: U.S. Geological Survey, Miscellaneous Field Studies Map MF-1198, scale 1:100,000. [1 PT (18)]

19. Pack, F.J., 1923, Torrential potential of desert waters: Pan‑American Geologist, v. 40, p. 349-356. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

20. Peninsula Times Tribune, 1984, Rain soaks east, Heat hits Rockies. [1 PT (20)]

22. The Pyramid, 1984, Flood waters cause damage, May 16, v. 92, no. 20. [2 PT (22)]

37. Pierson, T.C., 1984, Composition and dynamics of Rudd Canyon Mud flows, *in* Bowles, D.S. ed., Delineation of landslide, flash flood and debris flow hazards in Utah; Proceedings of a specialty conference: General Series, Utah Water Research Laboratory, G85-3, p. 132-152. Meeting: Logan, Utah, June 14-15, 1984. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

23. Shroder, J.F., Jr., 1971, Landslides of Utah: Utah Geological and Mineral Survey, Bulletin 90, 51 p. [6 PT (23), 1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

24. U.S. Forest Service, 1972, Landslide inventory map 340‑4U, Peterson Quadrangle: U.S. Forest service, Wasatch National Forest, Salt Lake Ranger District, Ogden, UT, scale 1:24,000. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

25. \_\_\_1972, Landslide Inventory Map 340‑1U, Snow Basin Quadrangle: U.S. Forest Service, Wasatch and Cache National Forest, Salt Lake and Ogden Ranger Districts, Ogden, UT, scale 1:24,000. [1 POLY (25,26,28,30)]

26. \_\_\_1972, Landslide Inventory Map 340‑ 3U, Kaysville Quadrangle: U.S. Forest Service, Wasatch National Forest, Salt Lake Ranger District, Ogden, UT, scale 1:24,000. [1 POLY (25,26,28,30)]

27. \_\_\_1972, Landslide Inventory Map 327‑2U, Farmington Quadrangle: U.S. Forest Service, Wasatch National Forest, Salt Lake Ranger District, Ogden, UT, scale 1:24,000. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

28. \_\_\_1972, Landslide Inventory Map 340‑2U, Ogden Quadrangle: U.S. Forest Service, Wasatch and Cache National Forests, Salt Lake and Ogden Ranger Districts, Ogden, UT, scale 1:24,000. [1 POLY (25,26,28,30)]

29. \_\_\_1972, Landslide inventory Map 327‑U, Bountiful Quadrangle: U.S. Forest Service, Wasatch National Forest, Salt Lake Ranger District, Ogden, UT, scale 1:24,000. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

30. \_\_\_1972, Landslide Inventory Map 353‑4U, Snow Basin Quadrangle: U.S. Forest Service, Cache National Forest, Ogden Ranger District, Ogden, UT, scale 1:24,000. [1 POLY (25,36,28,30]

31. Vandre, B.C., 1984, Rudd Creek debris flow, *in* Bowles, D.S., ed., Delineation of landslide, flash flood and debris flow hazards in Utah; Proceedings of a specialty conference: Utah Water Research Laboratory, Logan, Utah, June 14‑15, 1984, p. 117-131. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

32. Van Horn, R., 1972, Landslide and associated deposits map of the Sugar House Quadrangle, Salt Lake County, Utah: U.S. Geological Survey Miscellaneous Geologic Investigations Map I‑766D, scale 1:24,000. [1 PT (17,32)]

39. Vaugn, D.M., 1997, A major debris flow along the Wasatch Front in northern Utah, U.S.A: Physical Geography, v. 18, no. 3, p. 246-262. [1 PT (39)]

34. Wallaee, R.G., 1977, Boulder terraces and debris flows in Six Mile and Manti Canyons, west edge of Wasatch Plateau, Utah [abs.]: Geological Society of America, Abstracts with Programs, v. 9, no. 5, p. 663. [1 PT (9,34)]

35. Wieczorek, G.F., Ellen, S., Lips, E.W., Cannon, S.H., Short, D.H., 1983, Potential for debris flow and debris flood along the Wasatch Front between Salt Lake City and Willard, Utah, and measures for their mitigation: U.S. Geological Survey, Open‑File Report 83‑635, scale 1:100:000. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

36. \_\_\_ 1984, Identification of debris flow and debris flood potential along the Wasatch Front between Salt Lake City and Willard, Utah, *in* Bowles, D.S., ed, Delineation of landslide, flash flood and debris flow hazards in Utah; Proceedings of a specialty conference: General Series, Utah Water Research Laboratory, G85-3, p. 9., Meeting in Logan, Utah, June 14-15, 1984. [1 POLY (2,6,13,19,23,24,27,29,31,35,36,37)]

**Vermont**

4. Baskerville, C.A., and Ohlmacher, G.C., 1987, Recent Slope movements in Vermont, *in* Schultz, A. P., and Southworth, C. S., eds., Landslides of Eastern North America: U.S. Geological Survey Circular 1008, Papers presented at the southeast section of the GSA Symposium, March 26, 1987. [1 PT (4)]

1. Ratte, C.A., and Rhodes, D.D., 1977, Hurricane induced landslides on Dorset Mountain, Vermont [abs.]: Geological Society of America, Abstracts with Programs, v. 9, no. 3, p. 311. [1 PT (1,2)]

2. \_\_\_1981, The debris avalanche in the Green Mountains of Vermont: Appalachia Journal, p. 143-145. [1 PT (1,2)]

3. \_\_\_1982, Are the Green Mountains of Vermont really as serene as they look?: written commun. [1 PT (3)]

**Virginia**

1. Bartholomew, M.J., 1977, Geology of the Greenfield and Sherando Quadrangles, Virginia: Virginia Division of Mineral Resources, Publication 4, 43 p. [1 POLY (1)]

11. Clark, G.M., 1987, Debris slide and debris flow events in the Appalachians south of the glacial border: Geological Society of America Reviews in Engineering Geology, v. 7, p. 125-129. [7 PT (11)

2. Hack, J.T., and Goodlett, J.C., 1960, Geomorphology and forest ecology of a mountain region in the central Appalachians: U.S. Geological Survey Professional Paper 347, 66 p. [1 POLY (2),1 POLY (2,40)]

28. Hackman, R.J., and Thomas, R.E., 1979, Landslides and related features of the Hightown, VA-WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (28), 1 POLY (28,49,50)]

33. \_\_\_1979, Landslides and related features of the Mountain Grove, VA-WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (33)]

40. \_\_\_ 1979, Landslides and related features of the Reddish Knob, VA-WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (2,40)]

43. \_\_\_1979, Landslides and related features of the Sunrise, VA-WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (43)]

34. \_\_\_1979, Landslides and related features of the Mustoe, VA-WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (34), 1 POLY (34,49,50)]

3. Hull, J.C., Scott, R.C., 1982, Plant succession on debris avalanches of Nelson County, Virginia: Castanea, v. 47, p. I58‑I76. [1 POLY (3,4,5,6,7,8,9,10)]

49. Jacobsen, R.B., 1993, Geomorphic Studies of the storm and flood of November 3-5, 1985, in the upper Potomac and Cheat River basins: U. S. Geological Survey Bulletin, p. A1-A3. [1 POLY (28,49,50)] 1 POLY (34,49,50), 1 POLY (44,49,50)]

50. Jacobson, R.B., Cron, E.D., and McGeehin, J.P., 1989, Slope movements triggered by heavy rainfall, November 3-5, in Virginia and West Virginia, U.S.A., *in* Shultz, A.P., and Jibson, R.W., eds., Landslide processes of the eastern United States and Puerto Rico: Geological Society of America Special Paper 236. [1 POLY (28,49,50)] 1 POLY (34,49,50), 1 POLY (44,49,50)]

48. Johnson, S., 1999, Debris flows of 1996 on the Maury River, west flank of the Blue Ridge, Rockbridge County, VA: written commun. [1 POLY (48)]

4. Kudaida, A.J., Jr., 1971, Debris avalanching as a natural hazard in the southern Appalachians, a case study of the Davis Creek watershed, Virginia: East Tennessee State University, unpublished M.S. thesis. [1 POLY (3,4,5,6,7,8,9,10)]

47. Morgan, B.A., Wieczorek, G.F., and Campbell, R.H., 1999, Map of rainfall, debris flows, and flood effects of the June 27, 1995, storm in Madison County, Virginia: U.S. Geological Survey Investigations Map I-2623-A, scale 1:24,000. [1 POLY (47)]

23. Outerbridge, W.F., 1979, Landslides and related features of the Flat Gap, VA-KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (23)]

25. \_\_\_1979, Landslides and related features of the Grundy, VA quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (25)]

26. \_\_\_1979, Landslides and related features of the Harman, VA-KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (26)]

27. \_\_\_1979, Landslides and related features of the Haysi, VA-KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (27)]

29. \_\_\_1979, Landslides and related features of the Hurley, VA-KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (29)]

30. \_\_\_1979, Landslides and related features of the Jenkins East, VA-KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (30)]

39. \_\_\_1979, Landslides and related features of the Prater, VA quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (39)]

12. \_\_\_ 1982, Landslides and related features of the Appalachia, VA – KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (12)]

13. \_\_\_1982, Landslides and related features of the Ben Hur, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (13)]

24. \_\_\_1982, Landslides and related features of the Fort Blackmore, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (24)]

31. \_\_\_1982, Landslides and related features of the Lebanon, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (31)]

32. \_\_\_1982, Landslides and related features of the Moll Creek, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (32)]

36. \_\_\_ 1982, Landslides and related features of the Norton, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (36)]

37. \_\_\_1982, Landslides and related features of the Pennington Gap, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (37)]

41. \_\_\_1982, Landslides and related features of the Rose Hill, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (41)]

42. \_\_\_1982, Landslides and related features of the St. Paul, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (42)]

45. \_\_\_1982, Landslides and related features of the Wise, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (45)]

16. Outerbridge , W.F., and Thomas, R.E., 1979, Landslides and related features of the Caney Ridge, VA quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (16)]

22. \_\_\_ 1979, Landslides and related features of the Duty, VA quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (22)]

35. \_\_\_1979, Landslides and related features of the Nora, VA quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (35)]

38. \_\_\_1979, Landslides and related features of the Pound, VA quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (38)]

44. \_\_\_ 1979, Landslides and related features of the Vansant, VA quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (44), 1 POLY (44,49,50)]

14. \_\_\_1979, Landslides and related features of the Big A Mountain, VA quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (14)]

19. \_\_\_1979, Landslides and related features of the Clintwood, VA-KY quadrangle: U.S. Geological Survey Open-File Report 79-714, scale 1:24,000. [1 POLY (19)]

20. \_\_\_1982, Landslides and related features of the Coeburn, VA-KY quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (20)]

15. \_\_\_1982, Landslides and related features of the Brumley, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (15)]

17. \_\_\_1982, Landslides and related features of the Carbo, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (17)]

18. \_\_\_1982, Landslides and related features of the Clinchport, VA quadrangle: U.S. Geological Survey Open-File Report 82-0422, scale 1:24,000. [1 POLY (18)]

21. Thomas, R.E., and Hackman, R.J., 1979, Landslides and related features of the Cow Knob, VA-WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (21)]

46. \_\_\_1979, Landslides and related features of the Woodstock, VA-WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (46)]

5. Virginia Minerals, 1969, Natural features caused by a catastrophic storm in Nelson and Amherst Counties, Virginia: Virginia Minerals, Special Issue (October), 16 p. [1 POLY (3,4,5,6,7,8,9,10)]

6. Washington Post, 1982, Amtrak train derailed by mudslide: February 19. [1 POLY (3,4,5,6,7,8,9,10)]

7. Webb, H.W., Nunan, W.E., and Penley, H.M., 1970, Road log of storm‑damaged areas in central Virginia: Virginia Minerals, v. 16, no. 1, p. 1‑10. [1 POLY (3,4,5,6,7,8,9,10)]

8. Williams, G.P., and Guy, H.P., 1971, Debris avalanches, a geomorphic hazard, *in* Coates, D. R., (compiler) Environmental Geomorphology: Dowden, Hutchinson and Ross, Stroudsburg, PA, p. 25‑46. [1 POLY (3,4,5,6,7,8,9,10)]

9. \_\_\_1973, Erosional and deposition aspects of Hurricane Camille in Virginia, 1969: U.S. Geological Survey Professional Paper 804, 80 p. [1 POLY (3,4,5,6,7,8,9,10)]

10. Woodruff, J.F., 1971, Debris avalanches as an erosional agent in the Appalachian Mountains: Journal of Geography, v. 70, no. 7, p. 399‑405. [1 POLY (3,4,5,6,7,8,9,10)]

**Washington**

42. Brabb, E.E., Reconnaisance field investigations in Washington, 1982, 1985. [26 PT (42)]

1. Crandell, D.R., 1963, Paradise debris flow at Mount Rainier, Washington: U.S. Geological Survey Professional Paper 475‑B, p. B135‑139. [1 POLY (1,2,4,5,6,7,14,26)]

2. \_\_\_1971, Postglacial lahars from Mount Rainier Volcano, Washington: U.S. Geological Survey Professional Paper 677, 75 p. [1 POLY (1,2,4,5,6,7,14,26)]

4. Crandell, D.R., and Waldron, H.H., 1956, A recent volcanic mudflow of exceptional dimensions from Mt. Rainier, Washington: American Journal of Science, v. 254, no. 6, p. 349‑369. [1 POLY (1,2,4,5,6,7,14,26)]

5. Crandell, D.R., and Fahnestock, R.K., 1965, Rockfalls and avalanches from Little Tahoma Peak on Mount Rainier, Washington: U.S. Geological Survey Bulletin 1221A, p. A1‑A30. [1 POLY (1,2,4,5,6,7,14,26)]

6. \_\_\_1966, Rock‑fragment flows at Mount Rainier, Washington [abs.]: Geological Society of America, Special Paper 87, p. 281‑282. [1 POLY (1,2,4,5,6,7,14,26)]

7. Crandell, D.R., and Mullineaux, D.R., 1969, Volcanic hazards at Mount Rainier, Washington: U.S. Geological Survey Bulletin 1238, 26 p. [1 POLY (1,2,4,5,6,7,14,26)]

8. Cummans, J., 1981, Chronology of mudflows in the South Fork and North Fork Toutle Rivers following the May 18 eruption, *in* Lipman, P. W., Mullineaux, D. R., eds., The 1980 eruptions of Mount St. Helens, Washington: U. S. Geological Survey Professional Paper 1250, p. 347‑377. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

10. Daily News, 1978, Rain, hail dump mud on highway, September 11. [1 PT (10,11)]

11. Daily News, 1978, Hillside home hit by mud, August 14. [1 PT (10,11)]

14. Fiksdal, A.J., and Brunengo, M.J., 1980, Forest slope stability project; phase 1: Washington Department of Natural Resources, Division of Geology and Earth Resources, Technical Report DOE 80-2A, 16 p.[10 POLY (14), 1 POLY (1,2,4,5,6,7,14,26), 1 POLY (14,15), 1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41), 1 POLY (14,24,32)]

15. \_\_\_1981, Forest slope stability project, phase II: Washington State Department of Ecology, Report WDOE 81-14, 62 p. [1 POLY (15,17), [1 POLY (14,15), [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

16. Frank, D., Post, A., and Friedman, J.D., 1975, Recurrent geothermally‑induced debris avalanches on Boulder Glacier, Mount Baker, Washington: U.S. Geological Survey, Journal of Research, v. 3, no. 1, p. 77‑87. [1 POLY (16)]

41. Gilkey, K.E., 1982, Sedimentology of debris flows during the 1980 eruption of Mt. St. Helens: Geological Society of America Abstracts-with-Programs, Cordilleran Section, Anaheim CA. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

38. Heller, P.L., 1981, Small landslide types and controls on glacial deposits: Lower Skagit River drainage, northern Cascade Range, Washington: Environmental Geology, v. 3, p. 221-228. [56 PT (38)]

17. Higgins, J.D., Bijayanada, N., Mills, S.V., Copp, H., Roberson, J.A., 1983, The mechanics of mudflows: Report - Washington State University, Water Research center, v. 51, p. 116. [1 POLY (15,17)]

18. Hoblitt, R.P., Miller, C.D., Wallance, J.W., 1981, Origin and stratigraphy of the deposition produced by the May 18 directed blast, *in* Lipman, P.W., Mullineaux, D.R., eds., The 1980 eruptions of Mount St. Helens, Washington: U.S. Geological Survey Professional Paper 1250, p. 401-419. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

19. Janda, R.J., Scott, K.M., Nolan, K.M., Martinson, H.A., 1981, Lahar movement, effects and deposits, *in* Lipman, P.W., Mullineaux, D.R., eds., The 1980 eruptions of Mount St. Helens, Washington: U. S. Geological Survey Professional Paper 1250, p. 461-478. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

20. Japan Society of Landslides, 1979, Field Trip Guidebook to landslides, West Coast of North America: Tokyo. [(1 PT (20)]

21. Jones, F.O., not dated, U.S. Highway Research Board, #66: unpublished report. [1 PT (21)]

22. Kieffer, S.W., 1981, Fluid dynamics of the May 18 blast at Mount St. Helens, *in* Lipman, P.W., Mullineaux, D.R., eds., The eruptions of Mount St. Helens, Washington: U.S. Geological Survey Professional Paper 1250, p. 379-400. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

23. Klock, G.O., and Helvey, J.D., 1976, Debris flows following wildfire in north central Washington: Third Federal Inter‑Agency Sediment Conference, Proceedings, v. 1, p. 91‑98. [1 PT (23)]

24. Lisle, T.E., Lehre, A.K., Martinson, H.A., Meyer, D. F., Nelan, M., and Smith, R., 1982, Stream channel adjustments after the 1980 Mount St. Helens eruptions: Source unknown. [1 POLY (14,24,32)]

25. Lombard, R.E., Miles, M.B., Nelson, L.M., Kresh, D.L., Carpenter, P.J., 1981, The impact of mudflows of May 18 on the lower Toutle and Cowlitz Rivers, *in* Lipman, P.W. and Mullineaux, D.R., eds., The 1980 eruptions of Mount St. Helens, Washington: U.S. Geological Survey Professional Paper 1250, p. 693-699. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

26. McKee, B., 1968, The destruction of Mount Rainier, *in* Association of Engineering Geologist, 1968 National Meeting, Seattle, WA, Guidebook to field trips, p. 46-52. [1 POLY (1,2,4,5,6,7,14,26)]

37. Miller, D.J., 1991 Damage in King County from the storm of January 9,1990: Washington Geology, v. 19, no. 1, p 28-37. [1 POLY (37)]

27. Moore, J.G., Sisson, T.W., 1981, Deposits and effects of the May 18 pyroclastic surge *in* Lipman, P.W. and Mullineaux, D.R. eds., The eruptions of Mount St. Helens, Washington: U.S. Geological Survey Professional Paper 1250, p. 421-438. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

28. Mullineaux, D.R. and Crandell, D.R., 1962, Recent lahars from Mount St. Helens, Washington: Geological Society of America Bulletin, v. 73, no. 7, p. 855-869. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

29. Rowley, P.D., Kuntz, M.A., and Macleod, N.S., 1981, Pyroclastic‑flow deposits, *in* Lipman, P.W. and Mullineaux, D.R., eds., The eruptions of Mount St. Helens, Washington: U.S. Geological Survey Professional Paper 1250, p. 489-512. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

31. Schuster, R.L. 1981, Effects of the eruptions on civil works and operations in the Pacific Northwest, *in* Lipman, P.W. and Mullineaux, D.R., eds., The eruptions of Mount St. Helens, Washington: U.S. Geological Survey Professional Paper 1250, p. 701-718. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

32. \_\_\_1982, Environmental effects of landslides associated with the 18 May 1980 eruption of Mount St. Helens, State of Washington, U.S.A.: *in* Sheko, A., ed., Landslides and Mudflows: Reports of Alma-Ata International Seminar, October 1981: UNESCO, published by Centre of International Projects, GKNT, Moscow, U.S.S.R., p. 69‑86. [1 POLY (14,24,32)]

33. Swift, C.H. and Kresch, G.L., 1983, Mudflow hazards along the Toutle and Cowlitz Rivers from a hypothetical failure of Spirit Lake blockage: United States Geological Survey, Water‑Resources Investigations Report 82‑4125, p. 10 p. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

39. Thorsen, G.W., and Othburg, K.L., 1978, Slope stability pilot project for department of Ecology: Department of Natural Resources, Division of Geology and Earth Resources, Olympia, WA 98504, 14 p. [25 PT (39)]

34. Voight, B., Glicken, H., Janda, R.J., and Douglass, P.M., 1981, Catastrophic landslide avalanche of May 18, *in* Lipman, P.W. and Mullineaux, D.R., eds., The 1980 eruptions of Mount St. Helens, Washington: U.S. Geological Survey Professional Paper 1250, p. 347‑377. [1 POLY (8,14,15,19,22,25,27,28,29,31,33,34,41)]

35. Waters, A.C., 1973, The Columbia River Gorge; basalt stratigraphy, ancient lava dams, and landslide dams, *in* Geologic Field Trips in Northern Oregon and Southern Washington; Trip 4: Oregon Department of Geology and Mineral Industries, Bulletin 77, p. 133‑162. [1 PT (35)]

**West Virginia**

4. Author unknown, 1973, Flashflood. Washington Post, June 10, 1973, p. A4. 1 POLY (2,4)]

6. Clark, G.M., 1987, Debris slide and debris flow events in the Appalachians south of the glacial border: Geological Society of America Reviews in Engineering Geology, v. 7, p. 125 - 129. [7 PT (6)]

52. Jacobsen, R.B., 1993, Geomorphic Studies of the storm and flood of November 3-5, 1985, in the upper Potomac and Cheat River basins: U. S. Geological Survey Bulletin, p. A1-A3. [1 POLY (5,16,52), 1 POLY (5,20,52), 1 POLY (5,23,52), 1 POLY (5,38,52), 1 POLY (5,43,52), 1 POLY (5,46,52)]

5. Jacobson, R.B., Cron, E.D., and McGeehin, J.P., 1989, Slope movements triggered by heavy rainfall, November 3-5, in Virginia and West Virginia, U.S.A., *in* Shultz, A.P., and Jibson, R.W., eds., Landslide processes of the eastern United States and Puerto Rico: Geological Society of America Special Paper 236, p. 1-13. [1 POLY (5,16,52), 1 POLY (5,20,52), 1 POLY (5,23,52), 1 POLY (5,38,52), 1 POLY (5,43,52), 1 POLY (5,46,52)]

2. Lessing, P., Kulander, B.R., Wilson, B.D., Dean, S.L., and Woodring, S.M., 1976, West Virginia landslides and slide-prone areas: West Virginia Geological and Economics Survey Environmental Geology Bulletin, v. 15, no. 64, 23 sheets, scale 1:24,000. [1 POLY (2,4)]

7. \_\_\_1982, Landslides and related features of the Barnabus, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (7)]

15. \_\_\_ 1982, Landslides and related features of the Chapmanville, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (15)]

17. \_\_\_1982, Landslides and related features of the Delbarton, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (17)]

22. \_\_\_ 1982, Landslides and related features of the Holdon, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (22)]

24. \_\_\_ 1982, Landslides and related features of the Kermit, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (24)]

29. Outerbridge, W.F., 1982, Landslides and related features of the Majestic, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (29)]

30. \_\_\_1982, Landslides and related features of the Matewan, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (30)]

36. \_\_\_ 1982, Landslides and related features of the Myrtle, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (36)]

37. \_\_\_ 1982, Landslides and related features of the Naugatuck, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (37)]

45. \_\_\_1982, Landslides and related features of the Trace, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (45)]

47. \_\_\_ 1982, Landslides and related features of the Webb, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (47)]

49. \_\_\_ 1982, Landslides and related features of the Webb, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (49)]

50. \_\_\_1982, Landslides and related features of the Wilsondale, WV quadrangle: U.S. Geological Survey Open-File Report 82-51, scale 1:24,000. [1 POLY (50)]

3. Schneider, R.H., 1973, Debris slides and related flood damage resulting from Hurricane Camille, 19‑20 August and subsequent storm, 5‑6 September, 1969, in the Spring Creek drainage basin, Greenbrier County, West Virginia: University of Tennessee, unpublished Ph. D. thesis, 131 p. [1 PT (3)]

8. Thomas, R.E., and Hackman, R.J., 1979, Landslides and related features of the Bergton, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (8)]

10. \_\_\_1979, Landslides and related features of the Durbin, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (10)]

13. \_\_\_1979, Landslides and related features of the Brandywine, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (13)]

16. \_\_\_ 1979, Landslides and related features of the Circleville, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (16),1 POLY (5,16,52)]

18. \_\_\_1979, Landslides and related features of the Elkins, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (18)]

19. \_\_\_1979, Landslides and related features of the Fort Seybert, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (19)]

20. \_\_\_1979, Landslides and related features of the Franklin, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (20), 1 POLY (5,20,52)]

21. \_\_\_1979, Landslides and related features of the Glady, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (21)]

23. \_\_\_1979, Landslides and related features of the Hopeville, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (23), 1 POLY (5,23,52)]

26. \_\_\_1979, Landslides and related features of the Lost City, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (26)]

27. \_\_\_1979, Landslides and related features of the Lost River State Park, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (27)]

28. \_\_\_1979, Landslides and related features of the Harman, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (28)]

31. \_\_\_1979, Landslides and related features of the Milan, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (31)]

32. \_\_\_1979, Landslides and related features of the Mill Creek, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (32)]

34. \_\_\_1979, Landslides and related features of the Moatstown, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (34)]

35. \_\_\_1979, Landslides and related features of the Mozer, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (35)]

38. \_\_\_1979, Landslides and related features of the Onego, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (38),1 POLY (5,38,52)]

40. \_\_\_1979, Landslides and related features of the Palo Alto, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (40), 1 POLY (2,40)]

41. \_\_\_1979, Landslides and related features of the Petersburg West, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (41)]

42. \_\_\_1979, Landslides and related features of the Snyder Knob, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (42)]

43. \_\_\_1979, Landslides and related features of the Spruce Knob, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (43),1 POLY (5,43,52)]

44. \_\_\_1979, Landslides and related features of the Thornwood, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (44)]

46. \_\_\_1979, Landslides and related features of the Upper Tract, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (46), 1 POLY (5,46,52)]

51. \_\_\_1979, Landslides and related features of the Upper Tract, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (51)]

9. \_\_\_1980, Landslides and related features of the Beverly East, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (9)]

11. \_\_\_1980, Landslides and related features of the Beverly West, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (11)]

12. \_\_\_1980, Landslides and related features of the Bowden, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (12)]

14. \_\_\_1980, Landslides and related features of the Cass, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (14)]

25. \_\_\_1980, Landslides and related features of the Laneville, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (25)]

33. \_\_\_1980, Landslides and related features of the Minnehaha Springs, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (33)]

39. \_\_\_1980, Landslides and related features of the Paddy Knob, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (39)]

48. \_\_\_1980, Landslides and related features of the Whitmer, WV quadrangle: U.S. Geological Survey Open-File Report 80-194, scale 1:24,000. [1 POLY (48)]

**Wyoming**

1. Bailey, R G., 1971, Landslide hazards related to land use planning in Teton National Forest, northwest Wyoming: U.S. Forest Service, Intermountain Region, 131 p.

3. Holland, T.W., and Everitt, M.C., 1974, The Shell Canyon landslides, a geological engineering case history, *in* Voight, B., and Voight, M.A., eds., Rock mechanics, the American Northwest: Pennsylvania State University, University Park, PA, p. 37-44. [1 PT (3,7)]

4. Jensen, J.M., 1983, The upper Gros Ventre landslide of Wyoming; A dendronology of landslide events and the possible mechanics of failure: Geological Society of America, Abstracts with Programs, v. 15, no. 5, p. 387. [1 PT (4,5,6,8)]

5. Keefer, W.R., and Love, J.D., 1956, Landslides along the Gros Ventre River, Teton County, Wyoming: Wyoming Geological Association, 11th Annual Field Conference Guidebook, p. 24‑28. [1 PT (4,5,6,8)]

6. Lawrence, D.B., and Lawrence, E.G., 1958, Historic landslides of the Gros Ventre Valley, Wyoming: Mazama, v. 40, no. 13, p. 42‑52. [1 PT (4,5,6,8)]

9. Meyer, G.A., and Wells, S.G., 1997, Fire-related sedimentation events on alluvial fans, Yellowstone National Park, U.S.A.: Journal of Sedimentary Research, Section A.: Sedimentary Petrology and Process, v. 67, no. 5, p. 776-791. [1 PT (9)]

8. Palmquist, R.C., Cloud, T.A., Jensen, J., 1981, Landslide history, middle reach of Gros Ventre River Valley, Wyoming: National Geographic Research, v. 1, no. 1, p. 152-153. [1 PT (4,5,6,8)]

7. Schuster, R.L. and Everitt, M.C., 1968, Slope stability problems in Shell Canyon, Wyoming [abs.]: Geological Society of America Abstracts for 1967, Special Paper 115, p. 444‑445. [1 PT (3,7)]