Table 2-1 The Analog profiles

Channel Name	Parameter	Scale

units/mm	Designation on

digital profile
1X9I	coaxial inphase (900 Hz)	2.5 ppm	CXI (900Hz)
1X9Q	coaxial quadrature (900 Hz)	2.5 ppm	CXQ (900Hz)
3P9I	coplaner inphase (900 Hz)	2.5 ppm	CPI (900Hz)
3P9Q	coplaner quadrature (900 Hz)	2.5 ppm	CPQ (900Hz)
2P7I	coplaner inphase	5 ppm	CPI (7200Hz)
2P7Q	coplaner quadrature	5 ppm	CPQ (7200Hz)
4P5I	coplaner inphase	10 ppm	CPI (56000Hz)
4P5Q	coplaner quadrature	10 ppm	CPQ (56000Hz)
ALTR	altimeter	3 m	ALT
CMGC	magnetics, coarse	25 nt	MAG
CMGF	magnetics, fine	2.5 nt
VF1T	VLF - total: primary station	2%
VF1Q	VLF - quad: primary station	2%
VF2T	VLF - total: secondary station	2%
VF2Q	VLF - quad: secondary station	2%
CXSP	coaxial spherics monitor	CXS
CPSP	coplanar spherics monitor	CPS
CXPL	coaxial powerline monitor	CXP
CPPL	coplanar powerline monitor	CPP