Table 3-1 Plots Available from Survey

MAP PRODUCT	NO. OF SHEETS	ANOMALY MAP	PROFILES ON MAP	CONTOURS	SHADOW MAP
INK	COLOR
Electromagnetic anomalies	2	12,000	N/A	N/A	N/A	N/A
Probable Bedrock conductors	-	N/A	N/A	N/A	N/A	N/A
Resistivity (900 Hz)1	-	N/A	-	-	-	-
Resistivity (7,200 Hz)	2	N/A	-	12,000	12,000	-
Resistivity (56,000 Hz)1	-	N/A	-	-	-	-
EM Magnetite	-	N/A	-	-	-	-
Total Field Magnetics	2	N/A	-	12,000	12,000	-
Enhanced Magnetics	-	N/A	-	-	-	-
1st Vertical Derivative Magnetics	2	N/A	-	12,000	12,000	-
2nd Vertical Derivative Magnetics	-	N/A	-	-	-	-
Filtered Total Field VLF	2	N/A	-	12,000	12,000	-
VLF Profiles	-	N/A	-	-	-	-
Electromagnetic Profiles (900 Hz)	-	N/A	-	-	-
Electromagnetic Profiles

(7200 Hz)	-	N/A	-	-	-	-

N/A	Not Available this contract

Not required this contract

12,000	scale of delivered map

1

resistivities computed by contractor as part of new USGS work

NOTES:

Inked contour maps are provided on transparent media and show flight lines, EM anomalies, and suitable registration. Two paper prints of each map are supplied.