Tidal Analysis for Station F

-Computed from hourly-averaged pressure data (P_1 from 6042pt-a1h.nc)

number of observations = 3190
number of good observations = 3189
record length (days) = 132.92

start time: 05-Dec-1999 13:00:00
rayleigh criterion = 1.0
Greenwich phase computed with nodal corrections applied to amplitude 
and phase relative to center time

x0= 7.47e+003, x trend= 0

var(x)= 1974.5266   var(xp)= 1778.4525   var(xres)= 196.7847
percent var predicted/var original= 90.1 %

     tidal amplitude and phase with 95% CI estimates

tide   freq       amp     amp_err    pha    pha_err     snr
 MM   0.0015122    4.9270    4.660    52.98    55.30      1.1
 MSF  0.0028219    1.8308    3.761   346.86   145.99     0.24
 ALP1 0.0343966    0.1643    0.657   281.02   198.20    0.063
 2Q1  0.0357064    0.4798    0.743   115.80   103.61     0.42
 Q1   0.0372185    1.0958    0.937   168.44    53.24      1.4
*O1   0.0387307    6.1910    0.972   171.07     9.61       41
 NO1  0.0402686    0.7014    1.383   132.97   130.91     0.26
*K1   0.0417807    9.5503    0.864   180.29     5.80 1.2e+002
 J1   0.0432929    0.4491    0.754   197.15   106.82     0.35
 OO1  0.0448308    0.9648    1.212   208.36    77.81     0.63
 UPS1 0.0463430    0.1026    0.807   265.78   223.21    0.016
 EPS2 0.0761773    0.7326    0.759   321.66    68.25     0.93
*MU2  0.0776895    2.3683    0.890   353.93    22.08      7.1
*N2   0.0789992   12.5196    0.967   325.14     4.54 1.7e+002
*M2   0.0805114   54.7803    0.897   350.41     0.90 3.7e+003
*L2   0.0820236    1.3719    0.681    23.82    33.03      4.1
*S2   0.0833333   12.2154    0.880    22.73     4.06 1.9e+002
 ETA2 0.0850736    0.3903    0.744   263.58   141.65     0.28
 MO3  0.1192421    0.5665    0.490    36.19    48.91      1.3
*M3   0.1207671    0.5760    0.403    37.46    49.63        2
 MK3  0.1222921    0.2534    0.346    74.97    91.54     0.54
*SK3  0.1251141    1.0822    0.430   308.60    24.25      6.3
 MN4  0.1595106    0.1122    0.246   247.63   149.41     0.21
*M4   0.1610228    0.5500    0.386   161.85    34.76        2
 SN4  0.1623326    0.1807    0.253    10.74   103.57     0.51
*MS4  0.1638447    0.6064    0.361   145.26    31.81      2.8
 S4   0.1666667    0.5631    0.408   323.62    37.93      1.9
 2MK5 0.2028035    0.1211    0.142   332.36    84.11     0.73
 2SK5 0.2084474    0.1578    0.183    17.61    73.33     0.75
*2MN6 0.2400221    0.2948    0.136   294.93    28.33      4.7
*M6   0.2415342    0.2618    0.124   347.49    27.73      4.5
 2MS6 0.2443561    0.2028    0.147    23.79    36.24      1.9
 2SM6 0.2471781    0.0755    0.117    33.84   100.75     0.42
 3MK7 0.2833149    0.1368    0.165   130.56    75.47     0.69
 M8   0.3220456    0.0030    0.123   268.04   240.01   0.0006