ACTIVITY ID:  01SCC02	USGS CMG FACS EQUIPMENT LOG	
EQUIPMENT
SYSTEM	EQUIP
TYPE	EQUIP
CODE	EQUIPMENT
BRAND	EQUIPMENT
MODEL	EQUIPMENT
MEDIA	COMMENTS	
Applied Acoustics	Seismic	Boomer	Applied Acoustics	CSP300	Digital	AA200 plate, 100 Joules, Elics DelphSeismic V 203, NexGen 10 ch phone, BSI PC, UTM_401_1.pln,	
						12Khz Sample Freq., OYO608 Plotter	
EdgeTech X-Star	Chirp	Chirp	EdgeTech	X-Star	Digital - Paper	Using SB424 towfish, Elics FSSB V203
25Khz Sample Freq	
DGPS	Navigation	Nav	CSI	CSI DGPS Max	Digital	WAAS/Beacon DGPS, HYPack Lite Software V14.8, Output supplied to all systems Innerspace 488 for depth	
GPS	Navigation	Nav	Trimble	Centurian
P-Code	Digital	used for boomer lines 82-93,
Fugawi	
						CHIRP: 2m down, 2m back (starboard)
PHONES: 6 m back, 3m off (starboard)	
						PLATE: 10m back, 1m off (port)
100 Joules, 500Ms shot, 100MS save
Phones 4,5,6,7 on – 2m  phone spacing	
Vibracore	Vibracore	VC