{"text_format":"1","workbook":"xlsx","n_sheets":26,"sheets":["6295000","C11","C12","C13","C14","C15","C16","6309000","C18","C19","C20","C21","DS Powder","D1","D2","D3","D4","D5","6327500","D7","D8","D9","D10","D11","D12","6329500"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":26,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"6295000","index":0,"n_rows":24,"n_cols":21,"rows_kept":24,"cut":false,"hidden":false,"merged":[[0,1,1,20],[6,2,6,20],[9,2,9,20],[60,2,60,8],[63,2,63,8],[21,2,21,20],[43,2,44,8],[54,2,54,8],[57,2,57,8],[45,1,47,1],[48,2,48,8],[51,2,51,8],[12,2,12,20],[15,2,15,20],[18,2,18,20],[4,1,4,20]]}
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for streamflow-gaging station 06295000 (Yellowstone River at Forsyth, Mont.) and for the downstream end of Reach C10 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",64000,56600,44900,33600,26100,20600,16400,13400,9890,7770,6470,5530,5110,4650,4130,3550,2760,1910,1490]
[null,"Regulated",50100,43800,33800,24200,17300,13200,11000,9770,8220,7280,6520,5820,5430,5040,4630,4200,3580,2900,2540]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",19000,15100,11400,8700,7680,7040,6490,6100,5370,4850,4410,3930,3660,3360,3010,2620,1990,1540,1250]
[null,"Regulated",19800,15700,12000,9660,8650,7860,7430,7030,6430,5940,5470,5020,4770,4510,4200,3830,3230,2770,2520]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",75700,68900,60000,52000,45800,41300,37200,33600,27500,22400,17600,12700,10600,9440,7780,6840,5930,5100,4580]
[null,"Regulated",61100,54500,46500,39600,34300,30200,26700,23400,17600,13600,10800,8180,7310,6430,5810,5080,4330,3760,3430]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",60200,52100,42100,33600,28000,24100,20900,18500,15200,13200,11500,10100,9490,8910,8320,7530,6150,5230,4510]
[null,"Regulated",46600,40100,32200,25000,19700,15900,13200,11500,9530,8230,7170,6090,5610,5120,4580,4090,3320,2660,2350]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11200,10300,9030,8070,7410,6970,6650,6360,5850,5460,5060,4510,4160,3790,3450,2990,2280,1400,1110]
[null,"Regulated",12100,11400,10400,9400,8910,8450,8040,7720,7240,6800,6340,5790,5420,5030,4650,4200,3590,2830,2520]

{"sheet":"C11","index":1,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[6,1,6,20],[20,2,20,20],[23,2,23,20],[65,2,65,8],[47,1,49,1],[50,2,50,8],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[45,2,46,8]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C11 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",64500,57200,45400,34000,26400,20900,16700,13600,10100,7900,6570,5610,5190,4720,4180,3580,2790,1920,1500]
[null,"Regulated",50500,44200,34100,24400,17400,13400,11200,9890,8330,7370,6610,5890,5500,5100,4690,4240,3620,2930,2570]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",19700,15500,11700,8880,7830,7170,6610,6190,5460,4930,4480,3980,3700,3400,3050,2640,2010,1560,1270]
[null,"Regulated",20200,16100,12300,9850,8800,8000,7550,7150,6530,6020,5550,5080,4830,4560,4250,3870,3260,2800,2550]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",76200,69400,60500,52500,46200,41700,37600,34000,27800,22600,17900,12900,10800,9630,7920,6980,6060,5190,4660]
[null,"Regulated",61300,54800,46800,39900,34600,30400,26800,23500,17700,13700,10900,8300,7430,6540,5910,5180,4410,3840,3480]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",60900,52700,42600,34100,28400,24400,21200,18800,15400,13400,11700,10300,9670,9070,8460,7660,6300,5340,4630]
[null,"Regulated",47100,40400,32500,25200,19900,16000,13300,11600,9640,8310,7240,6170,5670,5170,4630,4120,3370,2700,2410]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11300,10400,9120,8170,7510,7050,6720,6430,5920,5530,5120,4550,4200,3830,3470,3000,2300,1400,1110]
[null,"Regulated",12200,11500,10500,9540,9030,8550,8130,7810,7320,6880,6420,5860,5480,5090,4700,4240,3630,2850,2540]

{"sheet":"C12","index":2,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C12 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",64600,57200,45400,34000,26400,20900,16700,13600,10100,7910,6580,5620,5190,4720,4180,3580,2790,1920,1500]
[null,"Regulated",50500,44200,34100,24400,17400,13400,11200,9900,8330,7380,6620,5900,5510,5110,4690,4250,3620,2930,2580]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",19700,15500,11700,8900,7850,7180,6620,6200,5470,4940,4480,3980,3700,3400,3050,2640,2010,1560,1270]
[null,"Regulated",20300,16100,12300,9860,8810,8020,7560,7160,6540,6020,5560,5080,4830,4560,4250,3880,3260,2800,2550]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",76200,69500,60500,52500,46300,41700,37600,34000,27800,22600,17900,12900,10800,9650,7940,7000,6070,5200,4660]
[null,"Regulated",61300,54800,46900,39900,34600,30400,26800,23500,17700,13700,10900,8310,7440,6550,5920,5190,4410,3840,3480]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",61000,52800,42700,34100,28400,24500,21200,18800,15400,13400,11700,10300,9680,9080,8470,7670,6310,5350,4640]
[null,"Regulated",47100,40400,32500,25200,19900,16000,13300,11600,9640,8320,7250,6170,5670,5170,4630,4120,3380,2700,2410]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11300,10400,9130,8180,7510,7060,6730,6440,5920,5540,5130,4550,4200,3830,3470,3000,2300,1400,1110]
[null,"Regulated",12200,11500,10500,9550,9040,8560,8140,7820,7330,6880,6420,5860,5480,5090,4700,4240,3630,2850,2540]

{"sheet":"C13","index":3,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C13 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",64600,57200,45400,34000,26400,20900,16700,13700,10100,7920,6590,5630,5200,4730,4190,3580,2790,1920,1500]
[null,"Regulated",50500,44200,34100,24400,17400,13400,11200,9900,8340,7380,6620,5900,5510,5110,4700,4250,3630,2930,2580]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",19800,15500,11700,8910,7860,7180,6630,6210,5470,4940,4490,3990,3710,3400,3050,2650,2020,1560,1270]
[null,"Regulated",20300,16100,12300,9870,8820,8020,7570,7170,6550,6030,5570,5090,4830,4560,4260,3880,3260,2800,2550]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",76200,69500,60600,52500,46300,41700,37600,34000,27800,22700,17900,12900,10900,9660,7940,7000,6070,5210,4670]
[null,"Regulated",61400,54800,46900,39900,34600,30400,26800,23500,17700,13700,10900,8310,7450,6550,5930,5190,4420,3850,3490]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",61000,52800,42700,34100,28400,24500,21200,18800,15500,13400,11700,10300,9700,9090,8480,7680,6320,5360,4650]
[null,"Regulated",47200,40400,32500,25200,19900,16000,13300,11600,9650,8320,7250,6180,5680,5170,4630,4120,3380,2710,2410]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11300,10400,9130,8180,7520,7070,6730,6440,5930,5540,5130,4560,4210,3830,3480,3000,2300,1400,1110]
[null,"Regulated",12200,11500,10500,9560,9050,8570,8150,7830,7330,6890,6430,5870,5490,5100,4700,4240,3640,2850,2540]

{"sheet":"C14","index":4,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C14 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",64700,57300,45500,34100,26500,20900,16700,13700,10100,7940,6600,5630,5210,4730,4190,3590,2790,1930,1510]
[null,"Regulated",50600,44300,34100,24400,17500,13400,11200,9920,8350,7390,6630,5910,5520,5120,4700,4250,3630,2930,2580]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",19900,15600,11700,8930,7870,7200,6640,6220,5480,4950,4500,3990,3710,3400,3050,2650,2020,1560,1270]
[null,"Regulated",20300,16100,12300,9890,8840,8040,7580,7180,6560,6030,5570,5090,4840,4570,4260,3880,3260,2810,2550]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",76300,69600,60600,52600,46300,41800,37600,34000,27800,22700,17900,12900,10900,9680,7960,7020,6090,5220,4670]
[null,"Regulated",61400,54800,46900,39900,34600,30500,26900,23500,17700,13700,10900,8330,7460,6570,5940,5200,4430,3860,3490]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",61100,52900,42800,34200,28400,24500,21200,18800,15500,13500,11800,10300,9710,9110,8500,7690,6330,5370,4660]
[null,"Regulated",47200,40400,32500,25200,19900,16100,13400,11700,9660,8330,7260,6180,5680,5180,4640,4120,3390,2710,2420]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11400,10500,9140,8190,7530,7070,6740,6450,5940,5550,5140,4560,4210,3830,3480,3010,2300,1400,1110]
[null,"Regulated",12300,11600,10500,9570,9060,8580,8160,7840,7340,6890,6430,5870,5490,5100,4710,4250,3640,2850,2540]

{"sheet":"C15","index":5,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C15 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",64700,57300,45500,34100,26500,20900,16700,13700,10100,7940,6600,5640,5210,4740,4200,3590,2800,1930,1510]
[null,"Regulated",50600,44300,34200,24400,17500,13400,11200,9920,8360,7400,6640,5920,5520,5120,4710,4260,3630,2940,2580]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",19900,15600,11700,8940,7880,7200,6640,6220,5490,4950,4500,4000,3710,3410,3060,2650,2020,1560,1270]
[null,"Regulated",20400,16200,12400,9900,8850,8050,7590,7180,6560,6040,5580,5100,4840,4570,4270,3890,3260,2810,2550]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",76300,69600,60700,52600,46400,41800,37700,34100,27900,22700,17900,12900,10900,9690,7970,7030,6090,5220,4680]
[null,"Regulated",61400,54800,46900,39900,34700,30500,26900,23500,17700,13700,10900,8330,7470,6570,5940,5210,4430,3860,3500]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",61100,52900,42800,34200,28500,24500,21300,18900,15500,13500,11800,10300,9720,9120,8500,7700,6340,5370,4660]
[null,"Regulated",47300,40500,32600,25200,19900,16100,13400,11700,9670,8330,7270,6190,5690,5180,4640,4130,3390,2710,2420]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11400,10500,9150,8200,7530,7080,6750,6460,5940,5550,5140,4560,4210,3840,3480,3010,2300,1400,1110]
[null,"Regulated",12300,11600,10500,9580,9060,8580,8160,7840,7340,6900,6440,5880,5500,5110,4710,4250,3640,2850,2540]

{"sheet":"C16","index":6,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C16 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",64700,57300,45500,34100,26500,20900,16700,13700,10100,7950,6600,5640,5210,4740,4200,3590,2800,1930,1510]
[null,"Regulated",50600,44300,34200,24400,17500,13400,11200,9920,8360,7400,6640,5920,5520,5120,4710,4260,3630,2940,2580]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",19900,15600,11700,8940,7880,7210,6650,6220,5490,4960,4500,4000,3710,3410,3060,2650,2020,1560,1270]
[null,"Regulated",20400,16200,12400,9910,8850,8050,7590,7190,6560,6040,5580,5100,4840,4570,4270,3890,3260,2810,2550]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",76300,69600,60700,52600,46400,41800,37700,34100,27900,22700,17900,12900,10900,9690,7970,7030,6100,5220,4680]
[null,"Regulated",61400,54800,46900,39900,34700,30500,26900,23500,17700,13700,10900,8330,7470,6570,5950,5210,4430,3860,3500]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",61100,52900,42800,34200,28500,24500,21300,18900,15500,13500,11800,10300,9730,9120,8510,7700,6340,5380,4670]
[null,"Regulated",47300,40500,32600,25200,19900,16100,13400,11700,9670,8340,7270,6190,5690,5180,4640,4130,3390,2710,2420]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11400,10500,9150,8200,7540,7080,6750,6460,5940,5550,5140,4560,4210,3840,3480,3010,2300,1400,1110]
[null,"Regulated",12300,11600,10500,9580,9070,8580,8160,7840,7350,6900,6440,5880,5500,5110,4710,4250,3640,2850,2540]

{"sheet":"6309000","index":7,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[47,1,49,1],[50,2,50,8],[53,2,53,8],[14,2,14,20],[17,2,17,20],[20,2,20,20],[8,2,8,20],[11,2,11,20],[6,1,6,20],[62,2,62,8],[65,2,65,8],[23,2,23,20],[45,2,46,8],[56,2,56,8],[59,2,59,8]]}
[]
[null,"Annual and seasonal flow-duration data for streamflow-gaging station 06309000 (Yellowstone River at Miles City, Mont.) for unregulated and regulated streamflow conditions, 1928–2002."]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for streamflow-gaging station 06309000 (Yellowstone River at Miles City, Mont.) and for the downstream end of Reach C17 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",66100,58800,46700,35100,27300,21600,17400,14300,10600,8300,6870,5860,5420,4910,4330,3670,2870,1960,1540]
[null,"Regulated",51600,45300,34900,24800,17800,13800,11600,10230,8640,7640,6880,6110,5710,5290,4860,4370,3740,3010,2670]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",21700,16600,12400,9430,8290,7540,6960,6470,5730,5170,4680,4130,3820,3500,3150,2710,2080,1600,1320]
[null,"Regulated",21500,17100,13100,10400,9250,8430,7910,7500,6830,6240,5800,5250,4990,4690,4400,4000,3330,2890,2620]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",77600,71000,62000,53800,47500,42800,38600,35000,28600,23300,18600,13400,11500,10200,8350,7410,6430,5470,4880]
[null,"Regulated",62000,55500,47800,40600,35400,31000,27200,23800,17800,13900,11200,8640,7790,6860,6220,5470,4640,4070,3630]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",63000,54500,44200,35400,29400,25400,22000,19600,16100,14000,12300,10800,10200,9550,8880,8050,6730,5670,4980]
[null,"Regulated",48600,41200,33300,25700,20400,16400,13700,12000,9950,8550,7460,6390,5840,5310,4760,4200,3530,2820,2570]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11700,10800,9390,8460,7790,7300,6940,6650,6120,5740,5300,4670,4320,3930,3540,3040,2340,1400,1110]
[null,"Regulated",12600,11900,10800,9950,9380,8850,8410,8090,7560,7100,6640,6050,5650,5260,4840,4350,3750,2890,2590]

{"sheet":"C18","index":8,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C18 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",66100,58800,46700,35100,27300,21600,17400,14300,10600,8300,6870,5860,5420,4910,4330,3670,2870,1960,1540]
[null,"Regulated",51600,45300,34900,24800,17800,13800,11600,10200,8640,7640,6880,6110,5710,5290,4860,4370,3740,3010,2670]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",21700,16600,12400,9430,8290,7540,6960,6470,5730,5170,4680,4130,3820,3500,3150,2710,2080,1600,1320]
[null,"Regulated",21500,17100,13100,10400,9250,8430,7910,7500,6830,6240,5800,5250,4990,4690,4400,4000,3330,2890,2620]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",77600,71000,62000,53800,47500,42800,38600,35000,28600,23300,18600,13400,11500,10200,8350,7410,6430,5470,4880]
[null,"Regulated",62000,55500,47800,40600,35400,31000,27200,23800,17800,13900,11200,8640,7790,6860,6220,5470,4640,4070,3630]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",63000,54500,44200,35400,29400,25400,22000,19600,16100,14000,12300,10800,10200,9550,8880,8050,6730,5670,4980]
[null,"Regulated",48600,41200,33300,25700,20400,16400,13700,12000,9950,8550,7460,6390,5840,5310,4760,4200,3530,2820,2570]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11700,10800,9390,8460,7790,7300,6940,6650,6120,5740,5300,4670,4320,3930,3540,3040,2340,1400,1110]
[null,"Regulated",12600,11900,10800,9950,9380,8850,8410,8090,7560,7100,6640,6050,5650,5260,4840,4350,3750,2890,2590]

{"sheet":"C19","index":9,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C19 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",66400,59100,46900,35200,27400,21700,17500,14400,10600,8330,6890,5870,5430,4920,4330,3670,2870,1960,1530]
[null,"Regulated",51900,45500,35000,24900,17900,13900,11600,10300,8670,7660,6900,6120,5720,5300,4870,4370,3740,3000,2660]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",22000,16800,12500,9510,8350,7580,6990,6490,5740,5180,4680,4130,3820,3500,3150,2710,2080,1590,1310]
[null,"Regulated",21900,17400,13200,10500,9310,8480,7940,7520,6840,6250,5810,5250,4990,4700,4400,4000,3340,2890,2610]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",78000,71300,62300,54000,47700,42900,38700,35100,28700,23400,18700,13500,11500,10200,8400,7440,6460,5500,4900]
[null,"Regulated",62400,55800,48000,40800,35500,31100,27300,23900,17900,14000,11200,8670,7820,6890,6250,5500,4660,4080,3630]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",63300,54800,44400,35500,29500,25500,22100,19700,16200,14000,12300,10800,10200,9580,8910,8080,6740,5680,4960]
[null,"Regulated",48900,41500,33400,25800,20500,16400,13700,12000,9970,8570,7470,6400,5850,5310,4760,4200,3510,2810,2550]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11700,10800,9410,8480,7810,7320,6960,6670,6130,5750,5310,4680,4330,3930,3550,3040,2320,1390,1090]
[null,"Regulated",12600,11900,10800,9970,9400,8870,8430,8110,7580,7120,6660,6060,5660,5270,4850,4360,3740,2890,2580]

{"sheet":"C20","index":10,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C20 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",66500,59200,46900,35300,27400,21700,17500,14400,10700,8340,6890,5880,5430,4920,4330,3670,2870,1950,1520]
[null,"Regulated",51900,45600,35100,24900,17900,13900,11600,10300,8670,7660,6900,6130,5730,5300,4870,4380,3730,3000,2660]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",22100,16900,12500,9530,8360,7590,6990,6490,5740,5180,4680,4130,3820,3500,3150,2710,2080,1590,1300]
[null,"Regulated",21900,17400,13200,10500,9320,8490,7940,7520,6850,6260,5810,5250,4990,4700,4400,4000,3340,2880,2610]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",78100,71400,62400,54100,47700,43000,38800,35100,28700,23400,18700,13500,11600,10200,8410,7450,6460,5500,4910]
[null,"Regulated",62500,55800,48100,40800,35500,31100,27300,23900,17900,14000,11300,8680,7820,6900,6260,5510,4670,4080,3630]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",63400,54900,44400,35600,29500,25500,22100,19700,16200,14100,12400,10800,10200,9590,8920,8080,6750,5680,4950]
[null,"Regulated",48900,41500,33400,25800,20500,16400,13700,12000,9980,8570,7470,6400,5850,5310,4760,4200,3510,2800,2540]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11700,10800,9410,8480,7810,7320,6960,6670,6140,5750,5310,4680,4330,3940,3550,3040,2320,1380,1080]
[null,"Regulated",12600,11900,10800,9970,9400,8880,8440,8120,7580,7120,6660,6070,5670,5270,4850,4360,3740,2880,2570]

{"sheet":"C21","index":11,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach C21 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",66600,59200,46900,35300,27500,21700,17500,14400,10700,8350,6900,5880,5440,4920,4340,3670,2870,1950,1520]
[null,"Regulated",52000,45600,35100,24900,17900,13900,11700,10300,8680,7670,6910,6130,5730,5300,4870,4380,3730,3000,2650]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",22200,16900,12600,9540,8370,7600,7000,6500,5750,5180,4680,4130,3820,3500,3150,2710,2080,1590,1300]
[null,"Regulated",22000,17500,13300,10500,9330,8500,7950,7530,6850,6260,5810,5260,5000,4700,4400,4000,3340,2880,2610]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",78200,71400,62400,54100,47800,43000,38800,35200,28800,23400,18700,13500,11600,10200,8420,7450,6470,5510,4910]
[null,"Regulated",62600,55900,48100,40800,35600,31100,27300,23900,17900,14000,11300,8690,7830,6910,6270,5510,4670,4080,3630]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",63500,54900,44400,35600,29600,25500,22100,19700,16200,14100,12400,10900,10200,9590,8920,8090,6750,5680,4950]
[null,"Regulated",49000,41600,33400,25800,20500,16500,13700,12000,9980,8580,7470,6400,5850,5310,4760,4200,3510,2800,2540]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11700,10800,9420,8480,7810,7320,6960,6670,6140,5760,5320,4680,4330,3940,3550,3040,2320,1380,1080]
[null,"Regulated",12600,11900,10800,9980,9410,8880,8440,8120,7590,7130,6660,6070,5670,5270,4850,4360,3740,2880,2570]

{"sheet":"DS Powder","index":12,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the Yellowstone River downstream from mouth of Powder River for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",70800,63100,49200,37000,29000,23000,18700,15300,11200,8790,7160,6060,5580,5020,4390,3720,2830,1890,1340]
[null,"Regulated",55700,48400,36700,26000,18800,14600,12200,10800,9060,7940,7140,6320,5890,5420,4960,4430,3670,2880,2500]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",26400,20200,14100,10600,9100,8160,7330,6750,5900,5300,4730,4140,3830,3520,3180,2730,2100,1450,1140]
[null,"Regulated",26700,20900,14700,11400,10100,9120,8330,7780,7040,6450,5900,5310,5050,4780,4420,3980,3410,2830,2540]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",84000,75400,66400,56900,50200,44900,40400,36700,30200,24800,20000,14200,12200,10600,9020,7860,6810,5840,5200]
[null,"Regulated",67800,59600,51200,43100,37100,32300,28200,24800,18600,14800,11900,9150,8210,7360,6700,5910,4960,4160,3580]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",67800,59100,46600,37200,31000,26700,23100,20600,17100,14700,12900,11400,10700,9990,9320,8420,6940,5810,4620]
[null,"Regulated",52600,45100,34800,27000,21400,17000,14200,12500,10300,8850,7600,6470,5940,5340,4760,4150,3280,2610,2230]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11800,11000,9690,8710,8020,7550,7190,6890,6330,5910,5460,4800,4420,3990,3620,3070,2090,1220,776]
[null,"Regulated",12800,12100,11100,10200,9660,9170,8730,8400,7850,7380,6890,6230,5840,5400,4940,4450,3620,2830,2380]

{"sheet":"D1","index":13,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D1 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",70800,63100,49200,37000,29000,23000,18700,15300,11200,8790,7160,6060,5580,5020,4390,3720,2830,1890,1340]
[null,"Regulated",55700,48400,36700,26000,18800,14600,12200,10800,9060,7940,7140,6320,5890,5420,4960,4430,3670,2880,2490]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",26400,20200,14100,10600,9100,8160,7330,6750,5900,5300,4730,4140,3830,3520,3180,2730,2100,1450,1140]
[null,"Regulated",26700,20900,14700,11400,10100,9120,8330,7780,7040,6450,5900,5310,5050,4780,4420,3980,3410,2830,2540]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",84000,75500,66400,56900,50200,44900,40400,36700,30200,24800,20000,14200,12200,10600,9030,7860,6810,5840,5210]
[null,"Regulated",67800,59600,51200,43100,37200,32400,28200,24800,18600,14800,11900,9150,8210,7360,6700,5910,4970,4160,3580]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",67900,59100,46600,37200,31000,26700,23100,20600,17100,14700,12900,11400,10700,9990,9330,8420,6940,5810,4620]
[null,"Regulated",52700,45100,34800,27000,21400,17000,14200,12500,10300,8850,7600,6470,5940,5340,4760,4150,3280,2610,2230]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11800,11000,9690,8710,8020,7550,7190,6890,6330,5920,5460,4800,4420,3990,3620,3070,2090,1220,775]
[null,"Regulated",12800,12100,11100,10200,9660,9170,8740,8400,7850,7380,6890,6230,5840,5400,4940,4450,3610,2830,2380]

{"sheet":"D2","index":14,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D2 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",70900,63200,49300,37100,29000,23100,18700,15300,11300,8810,7170,6070,5580,5020,4390,3720,2830,1890,1330]
[null,"Regulated",55900,48500,36800,26000,18800,14600,12200,10800,9070,7950,7150,6330,5900,5420,4960,4440,3670,2880,2490]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",26500,20300,14100,10600,9130,8180,7350,6760,5900,5300,4730,4140,3830,3520,3180,2730,2100,1440,1130]
[null,"Regulated",26800,21000,14700,11400,10100,9140,8340,7790,7040,6450,5900,5310,5050,4780,4420,3980,3410,2820,2540]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",84200,75600,66500,57000,50300,44900,40500,36700,30200,24900,20100,14200,12200,10600,9050,7880,6820,5860,5220]
[null,"Regulated",68000,59800,51300,43200,37200,32400,28300,24800,18600,14800,11900,9170,8220,7380,6710,5920,4980,4160,3580]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",68000,59300,46700,37300,31000,26700,23100,20600,17100,14700,13000,11400,10700,10000,9340,8440,6940,5820,4610]
[null,"Regulated",52800,45200,34900,27000,21400,17000,14200,12500,10300,8860,7610,6470,5950,5340,4760,4150,3270,2610,2220]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11800,11000,9700,8710,8030,7550,7190,6900,6330,5920,5460,4800,4420,4000,3620,3070,2090,1210,765]
[null,"Regulated",12800,12100,11100,10200,9670,9180,8750,8410,7860,7390,6890,6240,5850,5410,4940,4450,3610,2820,2380]

{"sheet":"D3","index":15,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D3 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",71500,63700,49600,37300,29200,23200,18900,15400,11300,8860,7210,6090,5600,5040,4390,3720,2820,1880,1310]
[null,"Regulated",56300,48900,37000,26200,18900,14700,12200,10800,9120,7990,7180,6360,5920,5440,4970,4440,3660,2860,2470]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",27100,20700,14300,10800,9220,8250,7390,6790,5920,5320,4730,4140,3830,3530,3190,2730,2110,1430,1110]
[null,"Regulated",27400,21500,14900,11500,10200,9220,8390,7820,7070,6480,5910,5310,5050,4790,4420,3980,3420,2820,2530]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",85000,76100,67000,57400,50600,45200,40700,36900,30400,25000,20200,14300,12300,10700,9120,7930,6870,5900,5250]
[null,"Regulated",68700,60200,51700,43500,37400,32500,28400,24900,18700,14900,12000,9220,8270,7430,6770,5970,5010,4170,3580]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",68600,59800,46900,37500,31200,26900,23300,20700,17200,14800,13000,11400,10700,10100,9390,8480,6970,5830,4570]
[null,"Regulated",53200,45700,35000,27200,21500,17000,14200,12500,10400,8900,7620,6480,5960,5350,4760,4150,3240,2580,2180]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11800,11000,9740,8740,8050,7580,7220,6920,6360,5940,5480,4820,4430,4000,3630,3080,2060,1190,726]
[null,"Regulated",12900,12200,11200,10300,9700,9210,8780,8450,7890,7420,6920,6260,5870,5420,4950,4460,3600,2820,2350]

{"sheet":"D4","index":16,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D4 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",71700,64000,49800,37400,29300,23300,18900,15400,11400,8890,7220,6100,5610,5040,4400,3730,2820,1870,1300]
[null,"Regulated",56600,49000,37100,26200,18900,14800,12300,10900,9150,8000,7200,6370,5930,5440,4970,4450,3650,2860,2460]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",27300,20900,14400,10800,9260,8280,7410,6800,5930,5320,4740,4140,3830,3530,3190,2730,2110,1420,1100]
[null,"Regulated",27700,21700,15000,11500,10300,9260,8420,7830,7080,6490,5910,5320,5060,4800,4420,3980,3430,2810,2520]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",85300,76300,67300,57500,50700,45300,40800,37000,30500,25100,20300,14400,12400,10700,9160,7950,6890,5920,5270]
[null,"Regulated",69000,60500,51900,43700,37500,32600,28400,24900,18800,15000,12100,9250,8300,7460,6790,6000,5030,4180,3570]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",68800,60000,47100,37600,31300,26900,23300,20700,17200,14900,13100,11500,10800,10100,9410,8500,6980,5840,4550]
[null,"Regulated",53500,45900,35100,27200,21500,17100,14300,12600,10400,8910,7630,6490,5960,5350,4760,4140,3220,2570,2160]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11800,11000,9750,8760,8070,7600,7240,6940,6370,5950,5490,4820,4430,4010,3640,3080,2040,1180,708]
[null,"Regulated",12900,12200,11200,10300,9710,9230,8800,8460,7900,7430,6940,6270,5880,5430,4950,4460,3590,2810,2340]

{"sheet":"D5","index":17,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D5 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",71800,64100,49800,37400,29300,23400,19000,15500,11400,8900,7230,6100,5610,5050,4400,3730,2820,1870,1300]
[null,"Regulated",56700,49100,37100,26300,19000,14800,12300,10900,9160,8010,7200,6370,5930,5450,4980,4450,3650,2850,2460]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",27400,21000,14400,10900,9280,8300,7420,6810,5930,5330,4740,4140,3830,3530,3190,2730,2110,1420,1100]
[null,"Regulated",27800,21800,15000,11600,10300,9280,8430,7840,7080,6490,5920,5320,5060,4800,4420,3980,3430,2810,2520]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",85500,76400,67300,57600,50800,45300,40800,37000,30500,25100,20400,14400,12400,10700,9180,7960,6900,5930,5280]
[null,"Regulated",69100,60600,52000,43700,37500,32700,28500,25000,18800,15000,12100,9260,8310,7470,6800,6000,5040,4180,3570]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",68900,60100,47100,37600,31300,27000,23400,20800,17300,14900,13100,11500,10800,10100,9420,8510,6980,5850,4540]
[null,"Regulated",53600,46000,35100,27300,21600,17100,14300,12600,10400,8920,7640,6490,5970,5350,4760,4140,3220,2570,2150]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11800,11000,9760,8760,8070,7600,7240,6940,6370,5950,5490,4830,4440,4010,3640,3080,2040,1180,701]
[null,"Regulated",12900,12200,11200,10300,9720,9240,8810,8470,7910,7440,6940,6270,5880,5440,4960,4470,3580,2810,2340]

{"sheet":"6327500","index":18,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[65,2,65,8],[50,2,50,8],[45,2,46,8],[47,1,49,1],[23,2,23,20],[62,2,62,8],[8,2,8,20],[11,2,11,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for streamflow-gaging station 06327500 (Yellowstone River at Glendive, Mont.)  and for the downstream end of Reach D6 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",72000,64200,49900,37500,29400,23400,19000,15500,11400,8920,7240,6110,5620,5050,4400,3730,2820,1870,1290]
[null,"Regulated",56800,49200,37200,26300,19000,14800,12300,10900,9170,8020,7210,6380,5940,5450,4980,4450,3650,2850,2450]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",27600,21100,14500,10900,9310,8320,7430,6820,5940,5330,4740,4140,3830,3530,3190,2730,2110,1410,1090]
[null,"Regulated",28000,21900,15100,11600,10300,9300,8440,7850,7090,6500,5920,5320,5060,4800,4420,3980,3430,2810,2520]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",85700,76600,67500,57700,50900,45400,40900,37100,30600,25200,20400,14400,12400,10700,9200,7980,6910,5940,5290]
[null,"Regulated",69300,60700,52100,43800,37600,32700,28500,25000,18800,15000,12100,9280,8320,7490,6820,6020,5050,4180,3570]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",69100,60300,47200,37700,31400,27000,23400,20800,17300,14900,13100,11500,10800,10100,9440,8520,6990,5850,4530]
[null,"Regulated",53700,46100,35200,27300,21600,17100,14300,12600,10400,8930,7640,6490,5970,5350,4760,4140,3210,2560,2140]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11800,11000,9770,8770,8080,7610,7250,6950,6380,5960,5500,4830,4440,4010,3640,3080,2030,1170,689]
[null,"Regulated",12900,12200,11200,10300,9730,9250,8820,8480,7920,7450,6950,6280,5890,5440,4960,4470,3580,2810,2330]

{"sheet":"D7","index":19,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D7 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",72100,64300,49900,37500,29400,23400,19000,15500,11400,8900,7250,6110,5620,5050,4400,3730,2820,1860,1280]
[null,"Regulated",56800,49200,37200,26200,19000,14800,12300,10900,9150,8020,7190,6350,5920,5430,4960,4420,3620,2800,2390]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",28900,21600,14800,11000,9370,8360,7490,6890,5990,5380,4780,4170,3860,3550,3210,2740,2120,1420,1100]
[null,"Regulated",29100,22400,15400,11700,10300,9330,8500,7910,7150,6550,5950,5360,5090,4830,4440,4000,3440,2810,2530]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",85400,76600,67500,57700,50800,45300,40800,37000,30500,25100,20300,14500,12500,10700,9240,8030,6960,5950,5310]
[null,"Regulated",68900,60700,52100,43800,37500,32500,28300,24800,18700,14900,12000,9250,8310,7490,6790,6000,5080,4230,3580]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",69500,60500,47300,37700,31400,27000,23400,20800,17300,14900,13000,11400,10700,10000,9310,8410,6890,5760,4440]
[null,"Regulated",54000,46100,35200,27200,21500,17000,14200,12500,10300,8820,7520,6370,5840,5240,4650,4040,3110,2470,2050]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11900,11000,9800,8780,8080,7610,7240,6940,6360,5940,5460,4790,4410,3990,3620,3060,2010,1140,659]
[null,"Regulated",13000,12200,11200,10300,9730,9250,8820,8480,7920,7430,6920,6240,5850,5420,4940,4450,3570,2780,2310]

{"sheet":"D8","index":20,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D8 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",72200,64300,49800,37400,29300,23400,19000,15500,11400,8890,7260,6100,5620,5050,4410,3730,2820,1850,1280]
[null,"Regulated",56800,49300,37100,26200,18900,14700,12300,10800,9130,8010,7170,6330,5900,5420,4950,4400,3590,2760,2340]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",30000,22000,15000,11100,9420,8400,7550,6940,6030,5410,4800,4200,3880,3570,3220,2750,2120,1430,1110]
[null,"Regulated",30000,22700,15600,11800,10400,9350,8540,7960,7200,6580,5980,5390,5110,4850,4460,4020,3450,2820,2530]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",85200,76700,67500,57700,50700,45200,40700,36900,30400,25000,20300,14600,12500,10800,9260,8060,7000,5960,5320]
[null,"Regulated",68600,60600,52100,43700,37400,32400,28200,24700,18600,14800,11900,9230,8300,7490,6770,5980,5100,4280,3580]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",69700,60600,47400,37800,31400,27000,23400,20800,17200,14800,13000,11400,10700,9940,9210,8320,6810,5680,4370]
[null,"Regulated",54200,46100,35200,27200,21500,17000,14100,12400,10200,8740,7430,6270,5750,5140,4550,3950,3030,2390,1980]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11900,11100,9820,8780,8080,7600,7240,6930,6350,5920,5440,4760,4380,3970,3600,3040,2000,1110,635]
[null,"Regulated",13100,12300,11200,10300,9730,9240,8830,8490,7910,7410,6890,6220,5830,5400,4930,4430,3560,2760,2290]

{"sheet":"D9","index":21,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D9 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",72300,64400,49800,37400,29300,23400,19000,15500,11400,8880,7260,6100,5620,5050,4410,3730,2820,1850,1270]
[null,"Regulated",56800,49300,37100,26100,18900,14700,12300,10800,9120,8010,7160,6320,5880,5410,4940,4390,3580,2730,2310]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",30600,22300,15200,11100,9450,8420,7580,6970,6060,5440,4820,4220,3890,3580,3230,2750,2120,1430,1120]
[null,"Regulated",30600,23000,15800,11900,10400,9370,8570,7990,7230,6610,5990,5400,5130,4860,4470,4030,3460,2820,2530]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",85000,76700,67500,57700,50600,45100,40600,36800,30300,25000,20300,14700,12600,10800,9280,8090,7030,5970,5330]
[null,"Regulated",68400,60600,52100,43700,37300,32300,28100,24600,18500,14800,11900,9220,8290,7490,6760,5960,5110,4300,3590]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",69900,60700,47400,37800,31400,27000,23400,20800,17200,14800,12900,11300,10600,9890,9140,8260,6760,5640,4330]
[null,"Regulated",54300,46100,35200,27200,21400,16900,14100,12400,10200,8680,7370,6210,5680,5090,4500,3900,2980,2340,1930]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",11900,11100,9830,8780,8080,7600,7230,6920,6340,5900,5420,4750,4370,3960,3590,3030,1990,1090,620]
[null,"Regulated",13200,12300,11200,10300,9730,9240,8830,8490,7910,7400,6870,6200,5810,5390,4920,4420,3550,2740,2280]

{"sheet":"D10","index":22,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D10 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",72500,64500,49800,37300,29300,23300,19000,15600,11300,8860,7270,6100,5610,5040,4410,3740,2830,1840,1260]
[null,"Regulated",56800,49400,37000,26000,18800,14600,12200,10800,9090,8000,7130,6280,5850,5390,4920,4350,3530,2660,2230]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",32400,23000,15600,11300,9530,8480,7670,7070,6130,5500,4870,4260,3930,3610,3250,2770,2130,1440,1140]
[null,"Regulated",32100,23600,16200,12100,10400,9410,8640,8080,7320,6670,6040,5460,5170,4900,4500,4060,3480,2820,2540]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",84600,76800,67400,57600,50400,44900,40400,36600,30100,24900,20200,14900,12700,10900,9330,8150,7100,5990,5350]
[null,"Regulated",67800,60600,52000,43600,37100,32100,27900,24300,18300,14600,11800,9180,8270,7500,6720,5930,5150,4380,3600]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",70400,60900,47500,37800,31500,27000,23500,20700,17100,14700,12800,11200,10500,9760,8960,8100,6620,5510,4210]
[null,"Regulated",54700,46200,35300,27100,21300,16800,14000,12300,10000,8540,7200,6030,5510,4930,4340,3760,2840,2210,1810]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",12000,11200,9870,8790,8090,7600,7220,6900,6320,5870,5370,4690,4320,3930,3560,3010,1970,1050,578]
[null,"Regulated",13400,12400,11300,10400,9740,9240,8830,8500,7900,7370,6830,6150,5760,5360,4900,4390,3530,2700,2260]

{"sheet":"D11","index":23,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[8,2,8,20],[11,2,11,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[6,1,6,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[23,2,23,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D11 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",72600,64500,49800,37300,29300,23300,19000,15600,11300,8840,7280,6100,5610,5040,4410,3740,2830,1830,1260]
[null,"Regulated",56800,49400,37000,26000,18800,14600,12200,10800,9070,8000,7110,6260,5830,5380,4910,4320,3500,2620,2180]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",33600,23500,15900,11400,9580,8510,7720,7130,6180,5550,4900,4290,3960,3630,3270,2780,2140,1450,1150]
[null,"Regulated",33100,24100,16400,12200,10400,9440,8690,8130,7380,6720,6070,5490,5190,4920,4520,4080,3490,2820,2550]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",84400,76800,67400,57600,50300,44800,40300,36500,30000,24800,20100,15000,12700,10900,9360,8190,7150,6000,5370]
[null,"Regulated",67400,60600,52000,43600,37000,31900,27800,24200,18200,14500,11700,9160,8260,7500,6690,5910,5170,4420,3600]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",70700,61100,47600,37800,31500,27000,23500,20700,17100,14700,12800,11200,10500,9680,8850,8010,6540,5430,4130]
[null,"Regulated",55000,46200,35300,27000,21300,16800,13900,12200,9910,8440,7100,5930,5400,4830,4240,3670,2750,2130,1730]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",12100,11200,9900,8800,8090,7600,7220,6890,6310,5850,5340,4660,4290,3910,3540,2990,1950,1020,552]
[null,"Regulated",13500,12400,11300,10400,9740,9240,8830,8500,7900,7350,6800,6120,5730,5340,4880,4370,3520,2670,2240]

{"sheet":"D12","index":24,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[53,2,53,8],[56,2,56,8],[59,2,59,8],[62,2,62,8],[6,1,6,20],[14,2,14,20],[17,2,17,20],[20,2,20,20],[23,2,23,20],[65,2,65,8],[45,2,46,8],[47,1,49,1],[50,2,50,8],[8,2,8,20],[11,2,11,20]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for the downstream end of reach D12 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",72600,64600,49700,37300,29200,23300,19000,15600,11300,8830,7290,6090,5610,5040,4420,3740,2830,1820,1250]
[null,"Regulated",56800,49400,37000,25900,18800,14600,12200,10700,9060,8000,7100,6240,5810,5370,4900,4310,3480,2580,2140]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",34500,23800,16100,11500,9620,8550,7770,7170,6210,5580,4930,4320,3970,3640,3280,2790,2140,1460,1150]
[null,"Regulated",33900,24400,16600,12200,10500,9460,8730,8170,7420,6750,6090,5510,5210,4940,4530,4090,3490,2830,2550]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",84200,76800,67400,57600,50300,44800,40300,36400,30000,24700,20100,15000,12800,10900,9390,8220,7180,6010,5380]
[null,"Regulated",67100,60500,52000,43600,37000,31800,27700,24000,18200,14400,11600,9140,8250,7500,6680,5890,5190,4460,3610]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",71000,61200,47700,37900,31500,27000,23500,20700,17100,14700,12700,11100,10400,9620,8760,7920,6470,5360,4070]
[null,"Regulated",55100,46200,35300,27000,21200,16700,13800,12100,9840,8370,7010,5840,5310,4750,4160,3590,2680,2060,1660]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",12100,11200,9910,8800,8090,7590,7210,6890,6300,5830,5310,4640,4270,3900,3520,2980,1940,993,530]
[null,"Regulated",13500,12400,11300,10400,9740,9230,8840,8500,7900,7330,6770,6090,5700,5330,4870,4350,3510,2650,2230]

{"sheet":"6329500","index":25,"n_rows":26,"n_cols":21,"rows_kept":26,"cut":false,"hidden":false,"merged":[[2,1,3,20],[47,1,49,1],[50,2,50,8],[53,2,53,8],[14,2,14,20],[17,2,17,20],[20,2,20,20],[8,2,8,20],[11,2,11,20],[6,1,6,20],[62,2,62,8],[65,2,65,8],[23,2,23,20],[45,2,46,8],[56,2,56,8],[59,2,59,8]]}
[]
[]
[null,"Appendix 6. Annual and seasonal flow-duration data at selected streamflow-gaging stations and interpolated for selected locations on the Yellowstone River, Mont., for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,"[Abbreviation: ft3/s, cubic feet per second. Symbol: %, percent]"]
[]
[null,"Annual and seasonal flow-duration data for streamflow-gaging station 06329500 (Yellowstone River near Sydney, Mont.) and for the downstream end of Reach D13 for unregulated and regulated streamflow conditions, 1928–2002."]
[]
[null,null,"Streamflow, in ft3/s, which was equaled or exceeded for indicated percent of time"]
[null,null,0.01,0.02,0.05,0.1,0.15,0.2,0.25,0.3,0.4,0.5,0.6,0.7,0.75,0.8,0.85,0.9,0.95,0.98,0.99]
[null,"Streamflow condition"]
[null,null,"Annual"]
[null,"Unregulated ",72800,64700,49700,37200,29200,23300,19000,15600,11300,8810,7300,6090,5610,5040,4420,3740,2830,1810,1240]
[null,"Regulated",56800,49500,36900,25800,18700,14500,12200,10700,9030,7990,7070,6210,5780,5350,4880,4270,3440,2520,2060]
[null,null,"Winter (January–March)"]
[null,"Unregulated ",36200,24500,16500,11600,9700,8600,7850,7260,6280,5640,4970,4360,4010,3670,3300,2800,2150,1470,1170]
[null,"Regulated",35300,25000,17000,12400,10500,9500,8800,8250,7500,6810,6130,5560,5250,4970,4560,4120,3510,2830,2560]
[null,null,"Spring (Apri–June)"]
[null,"Unregulated ",83800,76900,67400,57600,50100,44600,40100,36200,29800,24600,20000,15200,12900,11000,9430,8280,7250,6030,5400]
[null,"Regulated",66600,60500,52000,43500,36800,31600,27500,23800,18000,14300,11500,9110,8230,7500,6640,5860,5220,4530,3620]
[null,null,"Summer (July–September)"]
[null,"Unregulated ",71400,61400,47800,37900,31500,27000,23500,20700,17000,14600,12600,11000,10300,9500,8590,7780,6340,5240,3960]
[null,"Regulated",55500,46200,35300,26900,21100,16600,13700,12000,9700,8230,6860,5680,5150,4600,4010,3460,2550,1940,1550]
[null,null,"Fall (October–December)"]
[null,"Unregulated ",12200,11300,9950,8810,8090,7590,7200,6870,6280,5800,5270,4590,4230,3870,3490,2950,1920,950,492]
[null,"Regulated",13700,12500,11300,10400,9740,9230,8840,8510,7890,7300,6730,6050,5660,5300,4850,4320,3490,2610,2200]