# Mining Claim Activity on Federal Lands, 1976-2003

Metadata also available as

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: J. Douglas Causey
      Publication_Date: 2004
      Title: Mining Claim Activity on Federal Lands, 1976-2003
      Edition: 1
      Geospatial_Data_Presentation_Form: vector digital data
      Series_Information:
        Series_Name: Digital Series
        Issue_Identification: 124
      Publication_Information:
        Publication_Place: Menlo Park, CA
        Publisher: U.S. Geological Survey
      Online_Linkage: <http://pubs.usgs.gov/ds/124/>
  Description:
    Abstract:
      The az_pls_03 spatial data set (shapefile) contains Public Land Survey section polygons that had mining claims recorded in the U.S. Bureau of Land Management's LR2000 database as of January 15, 2004 for the period from 1976 to 2003.
    Purpose:
      This spatial database was designed to be used with the U.S Bureau of Land Management LR2000 database. It contains a field, MTRS, that allows linking information in the LR2000 case_tbl and case_land tables. However, it is only valid for data downloaded from the LR2000 database January 15, 2004, since the database is dynamic and new information may have been added after that date, or older information corrected.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: January 15, 2004
    Currentness_Reference:
      Date that BLM extracted mine claim data from their LR2000 database to provide to U.S. Geological Survey
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: Annually
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -114.690987
      East_Bounding_Coordinate: -109.045891
      North_Bounding_Coordinate: 37.000015
      South_Bounding_Coordinate: 31.333086
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: None
      Theme_Keyword: Mining claim
      Theme_Keyword: Public Land Survey
      Theme_Keyword: Meridian
      Theme_Keyword: Township
      Theme_Keyword: Range
      Theme_Keyword: Section
    Place:
      Place_Keyword_Thesaurus: None
      Place_Keyword: Arizona
  Access_Constraints: None
  Use_Constraints:
    This spatial database is not meant to be used or displayed at any scale larger than 1:100,000 (for example, 1:24,000). Any hardcopies utilizing these datasets shall clearly indicate their source. If the user has modified the data in any way, they are obligated to describe the types of modifications they have performed on the hardcopy map. User specifically agrees not to misrepresent these data sets, nor imply that changes they made were approved by the U.S. Geological Survey.
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: J. Douglas Causey
        Contact_Organization: U.S. Geological Survey
      Contact_Position: Geologist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 904 W. Riverside Ave, Rm 202
        City: Spokane
        State_or_Province: WA
        Postal_Code: 99201-1087
        Country: USA
      Contact_Voice_Telephone: 509.368.3116
      Contact_Facsimile_Telephone: 509.368.3199
      Contact_Electronic_Mail_Address: dcausey@usgs.gov
  Data_Set_Credit:
    Arizona State Land Department, Arizona Land Resources Information System
  Security_Information:
    Security_Classification_System: None
    Security_Classification: Unclassified
    Security_Handling_Description: None
  Native_Data_Set_Environment:
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.0.0.535

Data_Quality_Information:
  Attribute_Accuracy:
    Attribute_Accuracy_Report: Not stated in source metadata
  Logical_Consistency_Report: Not stated in source metadata
  Completeness_Report: Not stated in source metadata
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report:
        Approximate horizontal accuracy is 51 meters, assuming source data meets National Map Accuracy Standards.
    Vertical_Positional_Accuracy:
      Vertical_Positional_Accuracy_Report: Unknown
  Lineage:
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator:
            Arizona State Land Department, Arizona Land Resources Information System
          Publication_Date: Not published
          Title: Township, Range, and Section Grid Lines
          Edition: 1
          Online_Linkage: Contact originator
      Source_Scale_Denominator: 100000
      Type_of_Source_Media: digital tape media
      Source_Time_Period_of_Content:
        Source_Currentness_Reference: publication date
      Source_Citation_Abbreviation: AZ_PLS
      Source_Contribution: Digital file
    Process_Step:
      Process_Description:
        A field, MTRS, was added to the PLS database by concatenating meridian, township, range, and section information into one 18-character string. The string is in the format MM TTTTT RRRRR SSS where MM is a 2-digit number, TTTTT is township, RRRRR is range, and SSS is section for any valid Public Land Survey values. Township and range are 5 characters of the form XXXYZ where X is a numeric, Y is 0 or 2, and Z is N or S for township and E or W for range. A Y value of 2 means that the township or range are fractional township or ranges, otherwise the value is 0. Section is a 3-digit numeric. Then all fields except MTRS were deleted.

        All datasets were then projected to Geographic coordinate system, NAD27 datum.

        The spatial database was attached to a list of unique MTRS values from the LR2000 database and all polygons that had a record in the LR2000 database were selected. This selection was saved as the present shapefile.

      Process_Date: 2004
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: J. Douglas Causey
            Contact_Organization: U.S. Geological Survey
          Contact_Position: Geologist
          Contact_Address:
            Address_Type: mailing and physical address
            Address: 904 W. Riverside Ave., Rm 202
            City: Spokane
            State_or_Province: WA
            Postal_Code: 99201-1087
            Country: USA
          Contact_Voice_Telephone: 509.368.3116
          Contact_Facsimile_Telephone: 509.368.3199
          Contact_Electronic_Mail_Address: dcausey@usgs.gov

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: G-polygon
      Point_and_Vector_Object_Count: 19384

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Geographic:
      Latitude_Resolution: 0.05
      Longitude_Resolution: 0.05
      Geographic_Coordinate_Units: Decimal degrees
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1927
      Ellipsoid_Name: Clarke 1866
      Semi-major_Axis: 6378206.400000
      Denominator_of_Flattening_Ratio: 294.978698

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: az_pls_03
      Entity_Type_Definition:
        Public Land Survey sections containing mining claims recorded in the U.S. Bureau of Land Management LR2000 database January 15, 2004
      Entity_Type_Definition_Source: This document
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: MTRS
      Attribute_Definition: Feature area
      Attribute_Definition_Source: ESRI
    Attribute:
      Attribute_Label: MTRS
      Attribute_Definition:
        Meridian, Township, Range, Section concatenated string. Full description of this string provided in Process Step section.
      Attribute_Definition_Source: Causey, J.D. (2004)

Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: U.S. Geological Survey Information Services
      Contact_Address:
        Address_Type: mailing address
        Address: P.O. Box 25286
        City: Denver
        State_or_Province: CO
        Postal_Code: 80225USA
      Contact_Instructions:
        This report is available only in electronic format either for purchase on CD-ROM or from USGS Information Services at no cost from URL = <http://pubs.usgs.gov/ds/124>
  Resource_Description: Downloadable Data
  Distribution_Liability:
    The U.S. Geological Survey (USGS) provides these geographic data "as is." The USGS makes no guarantee or warranty concerning the accuracy of information contained in the geographic data. The USGS further makes no warranties, either expressed or implied as to any other matter whatsoever, including, without limitation, the condition of the product, or its fitness for any particular purpose. The burden for determining fitness for use lies entirely with the user. Although these data have been processed successfully on computers of the USGS, no warranty, expressed or implied, is made by the USGS regarding the use of these data on any other system, nor does the fact of distribution constitute or imply such warranty. In no event shall the USGS have liability whatsoever for payment of any consequential, incidental, indirect, special, or tort damages of any kind, including, but not limited to, any loss of profits arising out of use of or reliance on the geographic data or arising out of the delivery, installation, operation, or support by the USGS. This spatial database is not meant to be used or displayed at any scale larger than 1:100,000 (for example, 1:24,000).
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: Shapefile
        File_Decompression_Technique: no compression applied
        Transfer_Size: 3.278
      Digital_Transfer_Option:
        Online_Option:
          Online_Computer_and_Operating_System: <http://pubs.usgs.gov/ds/124/>
        Offline_Option:
          Offline_Media: CD-ROM
    Fees: Subject to change
  Technical_Prerequisites: Software capable of reading shapefile format files

Metadata_Reference_Information:
  Metadata_Date: 20050711
  Metadata_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: J. Douglas Causey
        Contact_Organization: U.S. Geological Survey
      Contact_Position: Geologist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 904 W. Riverside Ave, Rm 202
        City: Spokane
        State_or_Province: WA
        Postal_Code: 99201-1087
        Country: USA
      Contact_Voice_Telephone: 509.368.3116
      Contact_Facsimile_Telephone: 509.368.3199
      Contact_Electronic_Mail_Address: dcausey@usgs.gov
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Access_Constraints: None
  Metadata_Use_Constraints: None
  Metadata_Security_Information:
    Metadata_Security_Classification: Unclassified
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile

Generated by `mp` version 2.8.6 on Mon Jul 11 08:46:51 2005