Tidal Analysis for Station B

-calculated from pressure data (P_4023 of 5972p-a1h.nc)

number of observations = 1993
number of good observations = 1993
record length (days) = 83.04

start time: 24-Jan-2000
rayleigh criterion = 1.0
Greenwich phase computed with nodal corrections applied to amplitude 
and phase relative to center time

x0= 6.36e+003, x trend= 0

var(x)= 2470.2426   var(xp)= 2156.6085   var(xres)= 319.878
percent var predicted/var original= 87.3 %

     tidal amplitude and phase with 95% CI estimates

tide   freq       amp     amp_err    pha    pha_err     snr
 MM   0.0015122   10.6620    7.681    82.02    47.35      1.9
 MSF  0.0028219    5.0085    6.693    34.91    94.48     0.56
 ALP1 0.0343966    0.9908    1.431   130.65    85.24     0.48
 2Q1  0.0357064    0.7742    1.214    99.55   115.69     0.41
 Q1   0.0372185    1.6753    1.427   143.31    57.48      1.4
*O1   0.0387307    6.1431    1.533   170.33    14.04       16
 NO1  0.0402686    1.9369    2.402   224.70    94.30     0.65
*K1   0.0417807    7.4738    1.408   179.24    11.49       28
 J1   0.0432929    1.1656    1.340   116.60    77.60     0.76
 OO1  0.0448308    1.5103    1.953   266.09    87.15      0.6
 UPS1 0.0463430    0.9161    1.767   359.10   124.89     0.27
 EPS2 0.0761773    0.2030    1.063   323.33   230.28    0.036
 MU2  0.0776895    1.5870    1.481    12.26    61.53      1.1
*N2   0.0789992   12.3762    1.427   326.62     7.50       75
*M2   0.0805114   61.4069    1.478   350.50     1.40 1.7e+003
*L2   0.0820236    2.2090    1.247    36.97    31.39      3.1
*S2   0.0833333   14.6969    1.529    24.46     6.35       92
 ETA2 0.0850736    1.0239    1.535   233.75    93.39     0.44
 MO3  0.1192421    0.9947    1.092    19.58    65.21     0.83
 M3   0.1207671    1.3408    0.962    64.74    42.31      1.9
 MK3  0.1222921    0.6435    0.882   127.06    81.82     0.53
 SK3  0.1251141    1.2303    1.009   343.50    48.32      1.5
 MN4  0.1595106    0.0819    0.395   207.08   212.79    0.043
*M4   0.1610228    0.9504    0.506   160.57    35.37      3.5
 SN4  0.1623326    0.2536    0.441    15.46   124.22     0.33
*MS4  0.1638447    1.2096    0.520   156.29    27.31      5.4
*S4   0.1666667    0.8678    0.507     7.73    38.13      2.9
*2MK5 0.2028035    0.3209    0.214    42.11    46.64      2.3
*2SK5 0.2084474    0.4623    0.249    77.77    29.26      3.5
*2MN6 0.2400221    0.5057    0.293   304.96    34.81        3
*M6   0.2415342    1.0325    0.311   354.93    17.87       11
*2MS6 0.2443561    0.5571    0.316    56.75    29.35      3.1
 2SM6 0.2471781    0.0834    0.211   132.17   168.83     0.16
 3MK7 0.2833149    0.0406    0.116   306.79   164.65     0.12
 M8   0.3220456    0.0431    0.073   225.83   112.83     0.35