Tidal Analysis for Station E

-Computed from hourly-averaged pressure data (P_4023 from 6032tcp-a1h.nc)

number of observations = 3193  
number of good observations = 3193  
record length (days) = 133.04

start time: 04-Dec-1999 20:00:00
rayleigh criterion = 1.0
Greenwich phase computed with nodal corrections applied to amplitude 
and phase relative to center time

x0= 3.59e+003, x trend= 0

var(x)= 2603.3593   var(xp)= 2261.1172   var(xres)= 342.755
percent var predicted/var original= 86.9 %

     tidal amplitude and phase with 95% CI estimates

tide   freq       amp     amp_err    pha    pha_err     snr
 MM   0.0015122    6.0159    5.567    59.66    67.50      1.2
 MSF  0.0028219    1.4941    4.736   344.60   171.50      0.1
 ALP1 0.0343966    0.3755    0.835   299.25   145.22      0.2
 2Q1  0.0357064    0.7051    0.935    82.07    86.65     0.57
 Q1   0.0372185    1.1008    1.072   154.34    58.28      1.1
*O1   0.0387307    6.0339    1.087   166.05    11.32       31
 NO1  0.0402686    0.7822    1.442   176.11   144.70     0.29
*K1   0.0417807   10.2347    1.079   179.07     5.56       90
 J1   0.0432929    0.3142    0.719   195.37   162.75     0.19
 OO1  0.0448308    1.2865    1.569   237.89    88.46     0.67
 UPS1 0.0463430    0.1922    1.035    53.74   212.79    0.034
 EPS2 0.0761773    0.7019    0.939   322.55    93.90     0.56
*MU2  0.0776895    2.7344    1.129   356.17    22.29      5.9
*N2   0.0789992   14.0991    1.077   326.16     4.90 1.7e+002
*M2   0.0805114   61.9325    1.287   351.66     1.13 2.3e+003
*L2   0.0820236    1.5232    1.050    22.99    34.39      2.1
*S2   0.0833333   13.6476    1.331    23.86     4.56 1.1e+002
 ETA2 0.0850736    0.3619    0.948   268.22   163.51     0.15
 MO3  0.1192421    0.8917    0.653    40.32    44.64      1.9
*M3   0.1207671    0.9505    0.606    43.26    39.89      2.5
 MK3  0.1222921    0.3706    0.583    65.51    99.98      0.4
*SK3  0.1251141    1.5554    0.665   315.19    26.17      5.5
 MN4  0.1595106    0.1938    0.345   159.34   124.11     0.32
*M4   0.1610228    1.1467    0.396   167.51    18.59      8.4
 SN4  0.1623326    0.3672    0.396    12.47    75.36     0.86
*MS4  0.1638447    1.1918    0.391   165.58    18.69      9.3
*S4   0.1666667    0.6347    0.427   337.66    42.85      2.2
*2MK5 0.2028035    0.3052    0.208     6.08    45.78      2.2
*2SK5 0.2084474    0.3758    0.242    38.40    37.60      2.4
*2MN6 0.2400221    0.6320    0.173   311.47    11.94       13
*M6   0.2415342    1.1385    0.161   354.82     7.62       50
*2MS6 0.2443561    0.5651    0.162    51.20    14.61       12
 2SM6 0.2471781    0.0329    0.122    84.76   202.15    0.072
 3MK7 0.2833149    0.0865    0.121   281.53    95.52     0.51
 M8   0.3220456    0.0201    0.054   205.88   183.43     0.14