ACTIVITY ID:  01SCC01	USGS CMG FACS EQUIPMENT LOG	
EQUIPMENT
SYSTEM	EQUIPMENT
TYPE	EQUIP
CODE	EQUIPMENT
BRAND	EQUIPMENT
MODEL	EQUIPMENT
MEDIA	COMMENTS	
Applied Acoustics	Seismic	Boom	Applied Acoustics	CSP300	Digital	AA200 plate, 100 Joules, Elics DelphSeismic V 203, NexGen 10 ch phone, BSI PC,UTM_401_1.pln, 	
						12KHz Sample Freq.	
EdgeTech X-Star	Chirp	Chirp	EdgeTech	X-Star	Digital - Paper	Using SB424 towfish, Elics FSSB V203
25Khz Sample Freq.	
DGPS	Navigation	Nav	CSI	CSI DGPS Max	Digital	WAAS/Beacon DGPS , HYPack Lite Software V14.8, Output supplied to all systems Innerspace 488 for depth 	
						CHIRP: 2m down, 2m back (starboard)
PHONES: 6 m back, 3m off (starboard)	
						PLATE: 10m back , 1m off (port)
100 Joules, 500Ms shot, 100MS save
phones 4,5,6,7 on – 2m  phone spacing	
Vibracore	Vibracore	VC