Identification_Information:
  Citation:
    Citation_Information:
      Originator: Louisiana Oil Spill Coordinator's Office
      Publication_Date: 2007
      Title: Landsat Thematic Mapper Satellite Image 2005, UTM Zone 15 NAD83, LOSCO (2007) [landsat5tm_la_lsu_2005.sid]
      Geospatial_Data_Presentation_Form: raster digital data
      Publication_Information:
        Publication_Place: Baton Rouge, LA
        Publisher: Louisiana Oil Spill Coordinator's Office
      Online_Linkage: http://lagic.lsu.edu/loscoweb
  Description:
    Abstract: This data set is a Landsat Thematic Mapper satellite image of the State of Louisiana using bands 7-5-3 as an RGB composite.
    Purpose: For reference purposes
  Time_Period_of_Content:
    Time_Period_Information:
      Range_of_Dates/Times:
        Beginning_Date: 20050519
        Ending_Date: 20061030
    Currentness_Reference: Range of dates of imagery
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -94.054712
      East_Bounding_Coordinate: -88.619189
      North_Bounding_Coordinate: 33.023605
      South_Bounding_Coordinate: 28.835891
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: None
      Theme_Keyword: remote sensing
      Theme_Keyword: thematic mapper
      Theme_Keyword: Landsat 5
    Place:
      Place_Keyword_Thesaurus: None
      Place_Keyword: Louisiana
    Temporal:
      Temporal_Keyword_Thesaurus: None
      Temporal_Keyword: Winter 2002
  Access_Constraints: None
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: DeWitt Braud
        Contact_Organization: Louisiana State University, Coastal Studies Institute
      Contact_Address:
        Address_Type: physical address
        Address: Louisiana State University
        City: Baton Rouge
        State_or_Province: LA
        Postal_Code: 70803
        Country: USA
      Contact_Electronic_Mail_Address: dbraud1@lsu.edu
      Hours_of_Service: 0800-1630 CST
  Data_Set_Credit:
    Louisiana Department of Environmental Quality for acquisition of the following Landsat 5 Thematic Mapper scenes:

    p25r37 11june2006
    p25r37 13july2006
    p25r38 30oct2005
  Security_Information:
    Security_Classification_System: None
  Native_Data_Set_Environment: Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.2.0.1324
Data_Quality_Information:
  Attribute_Accuracy:
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report: RMS = 1 pixel which is equivalent to 28.5 meters.
  Lineage:
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: USGS EROS Data Center
          Publication_Date: 2005-2006
          Title: Landsat 5 Thematic Mapper multispectral 25-meter imagery
          Geospatial_Data_Presentation_Form: remote-sensing image
          Other_Citation_Details:
            Scenes Used:

            p21r39 18oct2005
            p21r40 18oct2005
            p22r39 09oct2005
            p22r39 25oct2005
            p22r40 25oct2005
            p23r37 30sept2005
            p23r38 16oct2005
            p23r39 16oct2005
            p23r40 16oct2005
            p24r37 19may2006
            p24r38 23oct2005
            p24r39 21sep2005
            p24r39 23oct2005

            LDEQ acquisitions:
            p25r37 11june2006
            p25r37 13july2006
            p25r38 30oct2005
          Online_Linkage: http://edc.usgs.gov/
      Type_of_Source_Media: CD-ROM
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Range_of_Dates/Times:
            Beginning_Date: 20050519
            Beginning_Time: unknown
            Ending_Date: 20061030
            Ending_Time: unknown
        Source_Currentness_Reference: Range of dates of imagery
      Source_Citation_Abbreviation: EROS
      Source_Contribution: LandsatTM image
    Process_Step:
      Process_Description:
        Scenes were subset to bands 3, 5, 7 and converted to at-satellite reflectance, then rescaled to 8-bit data range.
        During the mosaic process, the scenes were color-balanced arranged in RGB-753 order. Seam lines were used to eliminate clouds. The output file was cut to the Louisiana state boundary, and was converted to a GeoTIFF and a MrSID 1:10 compressed image.
      Source_Used_Citation_Abbreviation: EROS
      Process_Date: 2006
      Process_Contact:
        Contact_Information:
          Contact_Person_Primary:
            Contact_Person: DeWitt Braud
            Contact_Organization: Louisiana State University, Coastal Studies Institute
          Contact_Address:
            Address_Type: physical address
            Address: Louisiana State University
            City: Baton Rouge
            State_or_Province: LA
            Postal_Code: 70803
            Country: USA
          Contact_Electronic_Mail_Address: dbraud1@lsu.edu
          Hours_of_Service: 0800-1630 CST
  Cloud_Cover: Less than one percent.
Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Raster
  Raster_Object_Information:
    Raster_Object_Type: Pixel
    Row_Count: 16030
    Column_Count: 17830
    Vertical_Count: 1
Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Grid_Coordinate_System:
        Grid_Coordinate_System_Name: Universal Transverse Mercator
        Universal_Transverse_Mercator:
          UTM_Zone_Number: 15
          Transverse_Mercator:
            Scale_Factor_at_Central_Meridian: 0.999600
            Longitude_of_Central_Meridian: -93.000000
            Latitude_of_Projection_Origin: 0.000000
            False_Easting: 500000.000000
            False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: row and column
        Coordinate_Representation:
          Abscissa_Resolution: 28.500000
          Ordinate_Resolution: 28.500000
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222
Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Band_1
    Attribute:
      Attribute_Label: ObjectID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Value
    Attribute:
      Attribute_Label: Count
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Band_2
    Attribute:
      Attribute_Label: ObjectID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Value
    Attribute:
      Attribute_Label: Count
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Band_3
    Attribute:
      Attribute_Label: ObjectID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Value
    Attribute:
      Attribute_Label: Count
Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: David Gisclair
        Contact_Organization: Louisiana Oil Spill Coordinator's Office
      Contact_Position: Technical Assistance Program (TAP) Director
      Contact_Address:
        Address_Type: mailing address
        Address: Louisiana Oil Spill Coordinator's Office
        Address: Office of the Governor
        Address: P.O. Box 94095
        City: Baton Rouge
        State_or_Province: Louisiana
        Postal_Code: 70804
        Country: USA
      Contact_Voice_Telephone: (225) 219-5800
      Contact_Facsimile_Telephone: (225) 219-5802
      Contact_Electronic_Mail_Address: dgisclair@losco.state.la.us
      Hours_of_Service: 0800-1700 CST
  Resource_Description: landsat5tm_la_lsu_2005.sid
  Distribution_Liability:
    The data herein, including but not limited to geographic data, tabular data, analytical data, electronic data structures or files, are provided "as is" without warranty of any kind, either expressed or implied, or statutory, including, but not limited to, the implied warranties or merchantability and fitness for a particular purpose. The entire risk as to the quality and performance of the data is assumed by the user. No guarantee of accuracy is granted, nor is any responsibility for reliance thereon assumed. In no event shall the Louisiana Oil Spill Coordinator's Office (LOSCO) be liable for direct, indirect, incidental, consequential or special damages of any kind, including, but not limited to, loss of anticipated profits or benefits arising out of use of or reliance on the data. The LOSCO does not accept liability for any damages or misrepresentation caused by inaccuracies in the data or as a result of changes to the data caused by system transfers or other transformations or conversions, nor is there responsibility assumed to maintain the data in any manner or form.
    These data have been developed from the best available sources. Although efforts have been made to ensure that the data are accurate and reliable, errors and variable conditions originating from physical sources used to develop the data may be reflected in the data supplied. Users must be aware of these conditions and bear responsibility for the appropriate use of the information with respect to possible errors, scale, resolution, rectification, positional accuracy, development methodology, time period, environmental and climatic conditions and other circumstances specific to these data. The user is responsible for understanding the accuracy limitations of the data provided herein. The burden for determining fitness for use lies entirely with the user. The user should refer to the accompanying metadata notes for a description of the data and data development procedures.

    Although these data have been processed successfully on computers at the LOSCO, no guarantee, expressed or implied, is made by LOSCO regarding the use of these data on any other system, nor does the act of distribution constitute or imply any such warranty. Distribution of these data is intended for information purposes and should not be considered authoritative for navigational, engineering, legal and other site-specific uses.
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: MrSID
        File_Decompression_Technique: MrSID
        Transfer_Size: 45.248
      Digital_Transfer_Option:
        Offline_Option:
          Offline_Media: DVD-ROM
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: MrSID
        Format_Version_Number: 1.4
        File_Decompression_Technique: MrSID Viewer
        Transfer_Size: 45.248
      Digital_Transfer_Option:
        Offline_Option:
          Offline_Media: CD-ROM
    Ordering_Instructions: To obtain more information about ordering this data on DVD-ROM, please visit http://lagic.lsu.edu/loscoweb/ for more information.
Metadata_Reference_Information:
  Metadata_Date: 20070426
  Metadata_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Dina Knight
        Contact_Organization: Louisiana State University, Center for GeoInformatics
      Contact_Position: Geospatial Scientist/Research Associate 4
      Contact_Address:
        Address_Type: mailing and physical address
        Address: Louisiana State University
        Address: 280 Engineering Research & Development Bldg.
        City: Baton Rouge
        State_or_Province: LA
        Postal_Code: 70803
        Country: USA
      Contact_Voice_Telephone: REQUIRED: The telephone number by which individuals can speak to the organization or individual.
      Contact_Electronic_Mail_Address: dknight@lsu.edu
      Hours_of_Service: 0800-1630 CST
      Contact_Instructions: Electronic mail preferred
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: http://www.esri.com/metadata/esriprof80.html
    Profile_Name: ESRI Metadata Profile
