#
# U.S. Geological Survey
# National Water Information System
# Retrieved: 2011-04-01 18:52:24 EDT
#
# ---------------------WARNING---------------------
# The data you have obtained from this automated
# U.S. Geological Survey database have not received
# Director's approval and as such are provisional
# and subject to revision.  The data are released
# on the condition that neither the USGS nor the
# United States Government may be held liable for
# any damages resulting from its use.
#
# More data may be available offline.
# For more information on these data,  contact  Arkansas Water Data Inquiries.
# This file contains the annual peak streamflow data.
#
# This information includes the following fields:
#
#  agency_cd     Agency Code
#  site_no       USGS station number
#  peak_dt       Date of peak streamflow (format YYYY-MM-DD)
#  peak_tm       Time of peak streamflow (24 hour format, 00:00 - 23:59)
#  peak_va       Annual peak streamflow value in cfs
#  peak_cd       Peak Discharge-Qualification codes (see explanation below)
#  gage_ht       Gage height for the associated peak streamflow in feet
#  gage_ht_cd    Gage height qualification codes
#  year_last_pk  Peak streamflow reported is the highest since this year
#  ag_dt         Date of maximum gage-height for water year (if not concurrent with peak)
#  ag_tm         Time of maximum gage-height for water year (if not concurrent with peak)
#  ag_gage_ht    maximum Gage height for water year in feet (if not concurrent with peak)
#  ag_gage_ht_cd maximum Gage height code
#
# Sites in this file include:
#  USGS 07077555 Cache River near Cotton Plant, AR
#
# Peak Streamflow-Qualification Codes(peak_cd):
#   1 ... Discharge is a Maximum Daily Average
#   2 ... Discharge is an Estimate
#   3 ... Discharge affected by Dam Failure
#   4 ... Discharge less than indicated value,
#           which is Minimum Recordable Discharge at this site
#   5 ... Discharge affected to unknown degree by
#           Regulation or Diversion
#   6 ... Discharge affected by Regulation or Diversion
#   7 ... Discharge is an Historic Peak
#   8 ... Discharge actually greater than indicated value
#   9 ... Discharge due to Snowmelt, Hurricane,
#           Ice-Jam or Debris Dam breakup
#   A ... Year of occurrence is unknown or not exact
#   B ... Month or Day of occurrence is unknown or not exact
#   C ... All or part of the record affected by Urbanization,
#            Mining, Agricultural changes, Channelization, or other
#   D ... Base Discharge changed during this year
#   E ... Only Annual Maximum Peak available for this year
#
# Gage height qualification codes(gage_ht_cd,ag_gage_ht_cd):
#   1 ... Gage height affected by backwater
#   2 ... Gage height not the maximum for the year
#   3 ... Gage height at different site and(or) datum
#   4 ... Gage height below minimum recordable elevation
#   5 ... Gage height is an estimate
#   6 ... Gage datum changed during this year
#
#
agency_cd	site_no	peak_dt	peak_tm	peak_va	peak_cd	gage_ht	gage_ht_cd	year_last_pk	ag_dt	ag_tm	ag_gage_ht	ag_gage_ht_cd	modify_dt	peak_md
5s	15s	10d	6s	8s	27s	8s	13s	4s	10d	6s	8s	11s	19d	19n
USGS	07077555	1987-07-13		1550		13.30							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1987-12-28		9950		20.22							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1988-11-28		8420		19.85							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1990-02-20		6580		19.32							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1991-01-11		9300		20.07							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1991-12-13		4580		18.57							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1993-04-26		3490		17.46							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1993-12-08		7120		19.36							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1994-12-22		4270		18.28							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1995-12-30		1610		13.10							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1997-03-07	13:00	9540		20.10							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1998-03-17	04:00	3980		17.75							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	1999-02-07	14:00	3980		17.87							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2000-06-16	23:59	3080		16.86							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2001-03-04	19:00	5560		19.12							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2001-12-21	03:00	8100		20.23							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2003-05-25	19:00	6540		19.66							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2004-05-11	15:00	4440		18.33							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2005-01-17	08:59	6130		19.12							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2006-03-22	09:00	1970		14.30							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2007-01-22	20:00	6360		19.20							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2008-04-06	12:00	9330		20.05							0000-00-00 00:00:00	2010-07-07 21:27:04
USGS	07077555	2009-05-07	12:00	8380		19.93							0000-00-00 00:00:00	2010-07-07 21:27:04
